;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
NOTOR REC OPAL DROPPED 3K 600 ELOX LL START_21850;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21850.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046509934;Notor recessed LED Opal dropped ;21850;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX LL START_21851;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21851.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046509972;Notor recessed LED Opal dropped ;21851;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX LL START_21852;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21852.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510015;Notor recessed LED Opal dropped ;21852;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX LL START_21853;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21853.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510053;Notor recessed LED Opal dropped ;21853;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX LL START_21854;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21854.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510091;Notor recessed LED Opal dropped ;21854;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX LL START_21855;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21855.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510138;Notor recessed LED Opal dropped ;21855;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE LL START_21856;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21856.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510176;Notor recessed LED Opal dropped ;21856;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE LL START_21857;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21857.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510213;Notor recessed LED Opal dropped ;21857;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE LL START_21858;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21858.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510251;Notor recessed LED Opal dropped ;21858;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE LL START_21859;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21859.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510299;Notor recessed LED Opal dropped ;21859;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE LL START_21860;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21860.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510336;Notor recessed LED Opal dropped ;21860;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE LL START_21861;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21861.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510374;Notor recessed LED Opal dropped ;21861;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 ELOX HL START_21862;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21862.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510411;Notor recessed LED Opal dropped ;21862;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX HL START_21863;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21863.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510459;Notor recessed LED Opal dropped ;21863;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX HL START_21864;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21864.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510497;Notor recessed LED Opal dropped ;21864;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX HL START_21865;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21865.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510534;Notor recessed LED Opal dropped ;21865;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX HL START_21866;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21866.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510572;Notor recessed LED Opal dropped ;21866;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX HL START_21867;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21867.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510619;Notor recessed LED Opal dropped ;21867;46;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE HL START_21868;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21868.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510657;Notor recessed LED Opal dropped ;21868;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE HL START_21869;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21869.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510695;Notor recessed LED Opal dropped ;21869;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE HL START_21870;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21870.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510732;Notor recessed LED Opal dropped ;21870;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE HL START_21871;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21871.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510770;Notor recessed LED Opal dropped ;21871;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE HL START_21872;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21872.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510817;Notor recessed LED Opal dropped ;21872;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE HL START_21873;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21873.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046510855;Notor recessed LED Opal dropped ;21873;46;min. 80
NOTOR REC OPAL DROPPED 3K 600 ELOX LL SIN/CON/END_21874;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21874.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510893;Notor recessed LED Opal dropped ;21874;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX LL SIN/CON/END_21875;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21875.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510930;Notor recessed LED Opal dropped ;21875;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX LL SIN/CON/END_21876;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21876.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046510978;Notor recessed LED Opal dropped ;21876;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX LL SIN/CON/END_21877;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21877.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511012;Notor recessed LED Opal dropped ;21877;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX LL SIN/CON/END_21878;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21878.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511050;Notor recessed LED Opal dropped ;21878;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX LL SIN/CON/END_21879;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21879.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511098;Notor recessed LED Opal dropped ;21879;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE LL SIN/CON/END_21880;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21880.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511135;Notor recessed LED Opal dropped ;21880;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE LL SIN/CON/END_21881;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21881.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511173;Notor recessed LED Opal dropped ;21881;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE LL SIN/CON/END_21882;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21882.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511210;Notor recessed LED Opal dropped ;21882;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE LL SIN/CON/END_21883;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21883.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511258;Notor recessed LED Opal dropped ;21883;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE LL SIN/CON/END_21884;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21884.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511296;Notor recessed LED Opal dropped ;21884;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE LL SIN/CON/END_21885;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21885.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511333;Notor recessed LED Opal dropped ;21885;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 ELOX HL SIN/CON/END_21886;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21886.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511371;Notor recessed LED Opal dropped ;21886;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX HL SIN/CON/END_21887;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21887.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511418;Notor recessed LED Opal dropped ;21887;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX HL SIN/CON/END_21888;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21888.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511456;Notor recessed LED Opal dropped ;21888;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX HL SIN/CON/END_21889;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21889.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511494;Notor recessed LED Opal dropped ;21889;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX HL SIN/CON/END_21890;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21890.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511531;Notor recessed LED Opal dropped ;21890;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX HL SIN/CON/END_21891;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21891.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046511579;Notor recessed LED Opal dropped ;21891;46;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE HL SIN/CON/END_21892;90.500000000000;1.9;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21892.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511616;Notor recessed LED Opal dropped ;21892;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE HL SIN/CON/END_21893;90.500000000000;3.7;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21893.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511654;Notor recessed LED Opal dropped ;21893;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE HL SIN/CON/END_21894;90.500000000000;7.4;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21894.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511692;Notor recessed LED Opal dropped ;21894;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE HL SIN/CON/END_21895;90.500000000000;1.9;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21895.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511739;Notor recessed LED Opal dropped ;21895;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE HL SIN/CON/END_21896;90.500000000000;3.7;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21896.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511777;Notor recessed LED Opal dropped ;21896;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE HL SIN/CON/END_21897;90.500000000000;7.4;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21897.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;Standard;White;Fagerhult_White_aluminium;7320046511814;Notor recessed LED Opal dropped ;21897;46;min. 80
NOTOR REC OPAL DROPPED 3K 600 ELOX LL START_21850-402;90.500000000000;3.5;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21850-402.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046509958;Notor recessed LED Opal dropped ;21850-402;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX LL START_21851-402;90.500000000000;3.5;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21851-402.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046509996;Notor recessed LED Opal dropped ;21851-402;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX LL START_21852-402;90.500000000000;3.5;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21852-402.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510039;Notor recessed LED Opal dropped ;21852-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX LL START_21853-402;90.500000000000;3.5;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21853-402.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510077;Notor recessed LED Opal dropped ;21853-402;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX LL START_21854-402;90.500000000000;3.5;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21854-402.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510114;Notor recessed LED Opal dropped ;21854-402;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX LL START_21855-402;90.500000000000;3.5;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21855-402.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510152;Notor recessed LED Opal dropped ;21855-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE LL START_21856-402;90.500000000000;3.5;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21856-402.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510190;Notor recessed LED Opal dropped ;21856-402;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE LL START_21857-402;90.500000000000;3.5;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21857-402.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510237;Notor recessed LED Opal dropped ;21857-402;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE LL START_21858-402;90.500000000000;1.9;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21858-402.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510275;Notor recessed LED Opal dropped ;21858-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE LL START_21859-402;90.500000000000;3.7;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21859-402.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510312;Notor recessed LED Opal dropped ;21859-402;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE LL START_21860-402;90.500000000000;7.4;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21860-402.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510350;Notor recessed LED Opal dropped ;21860-402;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE LL START_21861-402;90.500000000000;1.9;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21861-402.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510398;Notor recessed LED Opal dropped ;21861-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 ELOX HL START_21862-402;90.500000000000;3.7;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21862-402.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510435;Notor recessed LED Opal dropped ;21862-402;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX HL START_21863-402;90.500000000000;7.4;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21863-402.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510473;Notor recessed LED Opal dropped ;21863-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX HL START_21864-402;90.500000000000;1.9;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21864-402.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510510;Notor recessed LED Opal dropped ;21864-402;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX HL START_21865-402;90.500000000000;3.7;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21865-402.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510558;Notor recessed LED Opal dropped ;21865-402;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX HL START_21866-402;90.500000000000;7.4;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21866-402.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510596;Notor recessed LED Opal dropped ;21866-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX HL START_21867-402;90.500000000000;1.9;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21867-402.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510633;Notor recessed LED Opal dropped ;21867-402;46;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE HL START_21868-402;90.500000000000;3.7;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21868-402.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510671;Notor recessed LED Opal dropped ;21868-402;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE HL START_21869-402;90.500000000000;7.4;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21869-402.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510718;Notor recessed LED Opal dropped ;21869-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE HL START_21870-402;90.500000000000;1.9;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21870-402.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510756;Notor recessed LED Opal dropped ;21870-402;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE HL START_21871-402;90.500000000000;3.7;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21871-402.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510794;Notor recessed LED Opal dropped ;21871-402;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE HL START_21872-402;90.500000000000;7.4;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21872-402.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510831;Notor recessed LED Opal dropped ;21872-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE HL START_21873-402;90.500000000000;1.9;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21873-402.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046510879;Notor recessed LED Opal dropped ;21873-402;46;min. 80
NOTOR REC OPAL DROPPED 3K 600 ELOX LL SIN/CON/END_21874-402;90.500000000000;3.7;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21874-402.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510916;Notor recessed LED Opal dropped ;21874-402;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX LL SIN/CON/END_21875-402;90.500000000000;7.4;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21875-402.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510954;Notor recessed LED Opal dropped ;21875-402;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX LL SIN/CON/END_21876-402;90.500000000000;1.9;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21876-402.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046510992;Notor recessed LED Opal dropped ;21876-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX LL SIN/CON/END_21877-402;90.500000000000;3.7;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21877-402.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511036;Notor recessed LED Opal dropped ;21877-402;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX LL SIN/CON/END_21878-402;90.500000000000;7.4;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21878-402.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511074;Notor recessed LED Opal dropped ;21878-402;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX LL SIN/CON/END_21879-402;90.500000000000;1.9;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21879-402.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511111;Notor recessed LED Opal dropped ;21879-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE LL SIN/CON/END_21880-402;90.500000000000;3.7;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21880-402.IES;Notor recessed LED Opal dropped ;aluminium;797;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;797;3000;3000;20;100;100;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511159;Notor recessed LED Opal dropped ;21880-402;8;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE LL SIN/CON/END_21881-402;90.500000000000;7.4;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21881-402.IES;Notor recessed LED Opal dropped ;aluminium;1621;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1621;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511197;Notor recessed LED Opal dropped ;21881-402;14;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE LL SIN/CON/END_21882-402;90.500000000000;1.9;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21882-402.IES;Notor recessed LED Opal dropped ;aluminium;3243;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3243;3000;3000;20;100;130;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511234;Notor recessed LED Opal dropped ;21882-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE LL SIN/CON/END_21883-402;90.500000000000;3.7;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21883-402.IES;Notor recessed LED Opal dropped ;aluminium;815;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;815;4000;4000;20;100;102;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511272;Notor recessed LED Opal dropped ;21883-402;8;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE LL SIN/CON/END_21884-402;90.500000000000;7.4;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21884-402.IES;Notor recessed LED Opal dropped ;aluminium;1653;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1653;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511319;Notor recessed LED Opal dropped ;21884-402;14;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE LL SIN/CON/END_21885-402;90.500000000000;1.9;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21885-402.IES;Notor recessed LED Opal dropped ;aluminium;3307;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;3307;4000;4000;20;100;132;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511357;Notor recessed LED Opal dropped ;21885-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 600 ELOX HL SIN/CON/END_21886-402;90.500000000000;3.7;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21886-402.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511395;Notor recessed LED Opal dropped ;21886-402;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 ELOX HL SIN/CON/END_21887-402;90.500000000000;7.4;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21887-402.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511432;Notor recessed LED Opal dropped ;21887-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 ELOX HL SIN/CON/END_21888-402;90.500000000000;1.9;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21888-402.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511470;Notor recessed LED Opal dropped ;21888-402;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 ELOX HL SIN/CON/END_21889-402;90.500000000000;3.7;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21889-402.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511517;Notor recessed LED Opal dropped ;21889-402;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 ELOX HL SIN/CON/END_21890-402;90.500000000000;7.4;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21890-402.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511555;Notor recessed LED Opal dropped ;21890-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 ELOX HL SIN/CON/END_21891-402;90.500000000000;1.9;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21891-402.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;DALIPhasePulseControl;Anodised;Fagerhult_Anodised;7320046511593;Notor recessed LED Opal dropped ;21891-402;46;min. 80
NOTOR REC OPAL DROPPED 3K 600 WHITE HL SIN/CON/END_21892-402;90.500000000000;3.7;3000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21892-402.IES;Notor recessed LED Opal dropped ;aluminium;1418;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1418;3000;3000;20;100;109;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511630;Notor recessed LED Opal dropped ;21892-402;13;min. 80
NOTOR REC OPAL DROPPED 3K 1200 WHITE HL SIN/CON/END_21893-402;90.500000000000;7.4;3000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21893-402.IES;Notor recessed LED Opal dropped ;aluminium;2893;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2893;3000;3000;20;100;116;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511678;Notor recessed LED Opal dropped ;21893-402;25;min. 80
NOTOR REC OPAL DROPPED 3K 2400 WHITE HL SIN/CON/END_21894-402;90.500000000000;1.9;3000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21894-402.IES;Notor recessed LED Opal dropped ;aluminium;5785;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5785;3000;3000;20;100;126;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511715;Notor recessed LED Opal dropped ;21894-402;46;min. 80
NOTOR REC OPAL DROPPED 4K 600 WHITE HL SIN/CON/END_21895-402;90.500000000000;3.7;4000;L 589 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21895-402.IES;Notor recessed LED Opal dropped ;aluminium;1451;Fagerhult_Opal;Ceiling;Recessed ;589;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1451;4000;4000;20;100;112;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511753;Notor recessed LED Opal dropped ;21895-402;13;min. 80
NOTOR REC OPAL DROPPED 4K 1200 WHITE HL SIN/CON/END_21896-402;90.500000000000;7.4;4000;L 1174 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21896-402.IES;Notor recessed LED Opal dropped ;aluminium;2950;Fagerhult_Opal;Ceiling;Recessed ;1174;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2950;4000;4000;20;100;118;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511791;Notor recessed LED Opal dropped ;21896-402;25;min. 80
NOTOR REC OPAL DROPPED 4K 2400 WHITE HL SIN/CON/END_21897-402;90.500000000000;1.9;4000;L 2343 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21897-402.IES;Notor recessed LED Opal dropped ;aluminium;5901;Fagerhult_Opal;Ceiling;Recessed ;2343;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;5901;4000;4000;20;100;128;Created 14/05/2018;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046511838;Notor recessed LED Opal dropped ;21897-402;46;min. 80
