;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Description##OTHER##;ColorRenderingIndex##Other##
Notor 65 Delta 3K 800 Anodised Start/Single LL DALIPhasePulseControl_13364-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13364-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046635800;Notor 65 Delta Start/Single;13364-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 800 Anodised Start/Single HL DALIPhasePulseControl_13365-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13365-402.IES;Notor 65 Delta;aluminium;2216;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2216;3000;3000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046635848;Notor 65 Delta Start/Single;13365-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 Anodised Start/Single LL DALIPhasePulseControl_13366-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13366-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046635886;Notor 65 Delta Start/Single;13366-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 Anodised Start/Single HL DALIPhasePulseControl_13367-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13367-402.IES;Notor 65 Delta;aluminium;2333;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2333;4000;4000;20;65;101;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046635923;Notor 65 Delta Start/Single;13367-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 800 White Start/Single LL DALIPhasePulseControl_13368-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13368-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046635961;Notor 65 Delta Start/Single;13368-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 800 White Start/Single HL DALIPhasePulseControl_13369-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13369-402.IES;Notor 65 Delta;aluminium;2216;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2216;3000;3000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046636005;Notor 65 Delta Start/Single;13369-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 White Start/Single LL DALIPhasePulseControl_13370-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13370-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046636043;Notor 65 Delta Start/Single;13370-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 White Start/Single HL DALIPhasePulseControl_13371-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13371-402.IES;Notor 65 Delta;aluminium;2333;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2333;4000;4000;20;65;101;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046636081;Notor 65 Delta Start/Single;13371-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single LL DALIPhasePulseControl_13372-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13372-402.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046636128;Notor 65 Delta Start/Single;13372-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single LL eSenseActiLumeSingleLuminaire_13372-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13372-442.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046636166;Notor 65 Delta Start/Single;13372-442;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single LL DALIPhasePulseControl1PullDimCord_13372-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13372-449.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046636142;Notor 65 Delta Start/Single;13372-449;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single HL DALIPhasePulseControl_13373-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13373-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046636203;Notor 65 Delta Start/Single;13373-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single HL eSenseActiLumeSingleLuminaire_13373-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13373-442.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046636241;Notor 65 Delta Start/Single;13373-442;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single HL DALIPhasePulseControl1PullDimCord_13373-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13373-449.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046636227;Notor 65 Delta Start/Single;13373-449;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single LL DALIPhasePulseControl_13374-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13374-402.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046636289;Notor 65 Delta Start/Single;13374-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single LL eSenseActiLumeSingleLuminaire_13374-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13374-442.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046636326;Notor 65 Delta Start/Single;13374-442;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single LL DALIPhasePulseControl1PullDimCord_13374-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13374-449.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046636302;Notor 65 Delta Start/Single;13374-449;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single HL DALIPhasePulseControl_13375-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13375-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046636364;Notor 65 Delta Start/Single;13375-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single HL eSenseActiLumeSingleLuminaire_13375-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13375-442.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046636401;Notor 65 Delta Start/Single;13375-442;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single HL DALIPhasePulseControl1PullDimCord_13375-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13375-449.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046636388;Notor 65 Delta Start/Single;13375-449;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single LL DALIPhasePulseControl_13376-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13376-402.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046636449;Notor 65 Delta Start/Single;13376-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single LL eSenseActiLumeSingleLuminaire_13376-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13376-442.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046636487;Notor 65 Delta Start/Single;13376-442;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single LL DALIPhasePulseControl1PullDimCord_13376-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13376-449.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046636463;Notor 65 Delta Start/Single;13376-449;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single HL DALIPhasePulseControl_13377-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13377-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046636524;Notor 65 Delta Start/Single;13377-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single HL eSenseActiLumeSingleLuminaire_13377-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13377-442.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046636562;Notor 65 Delta Start/Single;13377-442;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single HL DALIPhasePulseControl1PullDimCord_13377-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13377-449.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046636548;Notor 65 Delta Start/Single;13377-449;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single LL DALIPhasePulseControl_13378-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13378-402.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046636609;Notor 65 Delta Start/Single;13378-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single LL eSenseActiLumeSingleLuminaire_13378-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13378-442.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046636647;Notor 65 Delta Start/Single;13378-442;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single LL DALIPhasePulseControl1PullDimCord_13378-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13378-449.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046636623;Notor 65 Delta Start/Single;13378-449;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single HL DALIPhasePulseControl_13379-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13379-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046636685;Notor 65 Delta Start/Single;13379-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single HL eSenseActiLumeSingleLuminaire_13379-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13379-442.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046636722;Notor 65 Delta Start/Single;13379-442;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single HL DALIPhasePulseControl1PullDimCord_13379-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13379-449.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046636708;Notor 65 Delta Start/Single;13379-449;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single LL DALIPhasePulseControl_13380-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13380-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046636760;Notor 65 Delta Start/Single;13380-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single LL eSenseActiLumeSingleLuminaire_13380-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13380-442.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046636807;Notor 65 Delta Start/Single;13380-442;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single LL DALIPhasePulseControl1PullDimCord_13380-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13380-449.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046636784;Notor 65 Delta Start/Single;13380-449;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single HL DALIPhasePulseControl_13381-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13381-402.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046636845;Notor 65 Delta Start/Single;13381-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single HL eSenseActiLumeSingleLuminaire_13381-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13381-442.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046636883;Notor 65 Delta Start/Single;13381-442;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Start/Single HL DALIPhasePulseControl1PullDimCord_13381-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13381-449.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046636869;Notor 65 Delta Start/Single;13381-449;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single LL DALIPhasePulseControl_13382-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13382-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046636920;Notor 65 Delta Start/Single;13382-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single LL eSenseActiLumeSingleLuminaire_13382-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13382-442.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046636968;Notor 65 Delta Start/Single;13382-442;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single LL DALIPhasePulseControl1PullDimCord_13382-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13382-449.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046636944;Notor 65 Delta Start/Single;13382-449;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single HL DALIPhasePulseControl_13383-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13383-402.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637002;Notor 65 Delta Start/Single;13383-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single HL eSenseActiLumeSingleLuminaire_13383-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13383-442.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;eSenseActiLumeSingleLuminaire;Anodised;Fagerhult_Alugrey_Aluminium;7320046637040;Notor 65 Delta Start/Single;13383-442;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Start/Single HL DALIPhasePulseControl1PullDimCord_13383-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13383-449.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;Anodised;Fagerhult_Alugrey_Aluminium;7320046637026;Notor 65 Delta Start/Single;13383-449;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single LL DALIPhasePulseControl_13384-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13384-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637088;Notor 65 Delta Start/Single;13384-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single LL eSenseActiLumeSingleLuminaire_13384-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13384-442.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046637125;Notor 65 Delta Start/Single;13384-442;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single LL DALIPhasePulseControl1PullDimCord_13384-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13384-449.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046637101;Notor 65 Delta Start/Single;13384-449;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single HL DALIPhasePulseControl_13385-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13385-402.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637163;Notor 65 Delta Start/Single;13385-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single HL eSenseActiLumeSingleLuminaire_13385-442;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13385-442.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046637200;Notor 65 Delta Start/Single;13385-442;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Start/Single HL DALIPhasePulseControl1PullDimCord_13385-449;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13385-449.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046637187;Notor 65 Delta Start/Single;13385-449;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single LL DALIPhasePulseControl_13386-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13386-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637248;Notor 65 Delta Start/Single;13386-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single LL eSenseActiLumeSingleLuminaire_13386-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13386-442.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046637286;Notor 65 Delta Start/Single;13386-442;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single LL DALIPhasePulseControl1PullDimCord_13386-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13386-449.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046637262;Notor 65 Delta Start/Single;13386-449;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single HL DALIPhasePulseControl_13387-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13387-402.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637323;Notor 65 Delta Start/Single;13387-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single HL eSenseActiLumeSingleLuminaire_13387-442;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13387-442.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;eSenseActiLumeSingleLuminaire;White;Fagerhult_White_aluminium;7320046637361;Notor 65 Delta Start/Single;13387-442;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Start/Single HL DALIPhasePulseControl1PullDimCord_13387-449;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13387-449.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl1PullDimCord;White;Fagerhult_White_aluminium;7320046637347;Notor 65 Delta Start/Single;13387-449;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Start/Single LL DALIPhasePulseControl_13388-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13388-402.IES;Notor 65 Delta;aluminium;2945;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;2945;3000;3000;20;65;91;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637408;Notor 65 Delta Start/Single;13388-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Start/Single HL DALIPhasePulseControl_13389-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13389-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;95;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637446;Notor 65 Delta Start/Single;13389-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Start/Single LL DALIPhasePulseControl_13390-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13390-402.IES;Notor 65 Delta;aluminium;3100;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;3100;4000;4000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637484;Notor 65 Delta Start/Single;13390-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Start/Single HL DALIPhasePulseControl_13391-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13391-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;100;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637521;Notor 65 Delta Start/Single;13391-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Start/Single LL DALIPhasePulseControl_13392-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13392-402.IES;Notor 65 Delta;aluminium;2945;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;2945;3000;3000;20;65;91;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637569;Notor 65 Delta Start/Single;13392-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Start/Single HL DALIPhasePulseControl_13393-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13393-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;95;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637606;Notor 65 Delta Start/Single;13393-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Start/Single LL DALIPhasePulseControl_13394-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13394-402.IES;Notor 65 Delta;aluminium;3100;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;3100;4000;4000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637644;Notor 65 Delta Start/Single;13394-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Start/Single HL DALIPhasePulseControl_13395-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13395-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;100;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637682;Notor 65 Delta Start/Single;13395-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Start/Single LL DALIPhasePulseControl_13396-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13396-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637729;Notor 65 Delta Start/Single;13396-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Start/Single HL DALIPhasePulseControl_13397-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13397-402.IES;Notor 65 Delta;aluminium;9500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;9500;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637767;Notor 65 Delta Start/Single;13397-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Start/Single LL DALIPhasePulseControl_13398-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13398-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637804;Notor 65 Delta Start/Single;13398-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Start/Single HL DALIPhasePulseControl_13399-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13399-402.IES;Notor 65 Delta;aluminium;10000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;10000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046637842;Notor 65 Delta Start/Single;13399-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Start/Single LL DALIPhasePulseControl_13400-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13400-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637880;Notor 65 Delta Start/Single;13400-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Start/Single HL DALIPhasePulseControl_13401-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13401-402.IES;Notor 65 Delta;aluminium;9500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;9500;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046637927;Notor 65 Delta Start/Single;13401-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Start/Single LL DALIPhasePulseControl_13402-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13402-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639136;Notor 65 Delta Start/Single;13402-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Start/Single HL DALIPhasePulseControl_13403-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13403-402.IES;Notor 65 Delta;aluminium;10000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;10000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639174;Notor 65 Delta Start/Single;13403-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 800 Anodised Continuous LL DALIPhasePulseControl_13404-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13404-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639211;Notor 65 Delta Continuous;13404-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 800 Anodised Continuous HL DALIPhasePulseControl_13405-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13405-402.IES;Notor 65 Delta;aluminium;2216;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2216;3000;3000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639259;Notor 65 Delta Continuous;13405-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 Anodised Continuous LL DALIPhasePulseControl_13406-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13406-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639297;Notor 65 Delta Continuous;13406-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 Anodised Continuous HL DALIPhasePulseControl_13407-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13407-402.IES;Notor 65 Delta;aluminium;2333;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2333;4000;4000;20;65;101;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639334;Notor 65 Delta Continuous;13407-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 800 White Continuous LL DALIPhasePulseControl_13408-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13408-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639372;Notor 65 Delta Continuous;13408-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 800 White Continuous HL DALIPhasePulseControl_13409-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13409-402.IES;Notor 65 Delta;aluminium;2216;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2216;3000;3000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639419;Notor 65 Delta Continuous;13409-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 White Continuous LL DALIPhasePulseControl_13410-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13410-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639457;Notor 65 Delta Continuous;13410-402;12;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 800 White Continuous HL DALIPhasePulseControl_13411-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13411-402.IES;Notor 65 Delta;aluminium;2333;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;840;2333;4000;4000;20;65;101;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639495;Notor 65 Delta Continuous;13411-402;23;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Continuous LL DALIPhasePulseControl_13412-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13412-402.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639532;Notor 65 Delta Continuous;13412-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Continuous HL DALIPhasePulseControl_13413-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13413-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639570;Notor 65 Delta Continuous;13413-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Continuous LL DALIPhasePulseControl_13414-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13414-402.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639617;Notor 65 Delta Continuous;13414-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Continuous HL DALIPhasePulseControl_13415-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13415-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639655;Notor 65 Delta Continuous;13415-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Continuous LL DALIPhasePulseControl_13416-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13416-402.IES;Notor 65 Delta;aluminium;1473;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1473;3000;3000;20;65;79;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639693;Notor 65 Delta Continuous;13416-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Continuous HL DALIPhasePulseControl_13417-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13417-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;92;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639730;Notor 65 Delta Continuous;13417-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Continuous LL DALIPhasePulseControl_13418-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13418-402.IES;Notor 65 Delta;aluminium;1550;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;1550;4000;4000;20;65;83;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639778;Notor 65 Delta Continuous;13418-402;19;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Continuous HL DALIPhasePulseControl_13419-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13419-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;97;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046639815;Notor 65 Delta Continuous;13419-402;36;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Continuous LL DALIPhasePulseControl_13420-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13420-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639853;Notor 65 Delta Continuous;13420-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 Anodised Continuous HL DALIPhasePulseControl_13421-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13421-402.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639891;Notor 65 Delta Continuous;13421-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Continuous LL DALIPhasePulseControl_13422-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13422-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639938;Notor 65 Delta Continuous;13422-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 Anodised Continuous HL DALIPhasePulseControl_13423-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13423-402.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046639976;Notor 65 Delta Continuous;13423-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Continuous LL DALIPhasePulseControl_13424-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13424-402.IES;Notor 65 Delta;aluminium;3325;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3325;3000;3000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640019;Notor 65 Delta Continuous;13424-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 1200 White Continuous HL DALIPhasePulseControl_13425-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13425-402.IES;Notor 65 Delta;aluminium;4750;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;4750;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640057;Notor 65 Delta Continuous;13425-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Continuous LL DALIPhasePulseControl_13426-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13426-402.IES;Notor 65 Delta;aluminium;3500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;3500;4000;4000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640095;Notor 65 Delta Continuous;13426-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 1200 White Continuous HL DALIPhasePulseControl_13427-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13427-402.IES;Notor 65 Delta;aluminium;5000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;1256;5000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640132;Notor 65 Delta Continuous;13427-402;43;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Continuous LL DALIPhasePulseControl_13428-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13428-402.IES;Notor 65 Delta;aluminium;2945;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;2945;3000;3000;20;65;91;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640170;Notor 65 Delta Continuous;13428-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Continuous HL DALIPhasePulseControl_13429-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13429-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;95;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640217;Notor 65 Delta Continuous;13429-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Continuous LL DALIPhasePulseControl_13430-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13430-402.IES;Notor 65 Delta;aluminium;3100;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;3100;4000;4000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640255;Notor 65 Delta Continuous;13430-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Continuous HL DALIPhasePulseControl_13431-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13431-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;100;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640293;Notor 65 Delta Continuous;13431-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Continuous LL DALIPhasePulseControl_13432-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13432-402.IES;Notor 65 Delta;aluminium;2945;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;2945;3000;3000;20;65;91;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640330;Notor 65 Delta Continuous;13432-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Continuous HL DALIPhasePulseControl_13433-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13433-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;95;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640378;Notor 65 Delta Continuous;13433-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Continuous LL DALIPhasePulseControl_13434-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13434-402.IES;Notor 65 Delta;aluminium;3100;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;3100;4000;4000;20;65;96;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640415;Notor 65 Delta Continuous;13434-402;32;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Continuous HL DALIPhasePulseControl_13435-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13435-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;100;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640453;Notor 65 Delta Continuous;13435-402;70;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Continuous LL DALIPhasePulseControl_13436-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13436-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640491;Notor 65 Delta Continuous;13436-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 Anodised Continuous HL DALIPhasePulseControl_13437-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13437-402.IES;Notor 65 Delta;aluminium;9500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;9500;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640538;Notor 65 Delta Continuous;13437-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Continuous LL DALIPhasePulseControl_13438-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13438-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640576;Notor 65 Delta Continuous;13438-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 Anodised Continuous HL DALIPhasePulseControl_13439-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13439-402.IES;Notor 65 Delta;aluminium;10000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;10000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640613;Notor 65 Delta Continuous;13439-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Continuous LL DALIPhasePulseControl_13440-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13440-402.IES;Notor 65 Delta;aluminium;6650;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;6650;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640651;Notor 65 Delta Continuous;13440-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 3K 2400 White Continuous HL DALIPhasePulseControl_13441-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13441-402.IES;Notor 65 Delta;aluminium;9500;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;9500;3000;3000;20;65;109;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640699;Notor 65 Delta Continuous;13441-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Continuous LL DALIPhasePulseControl_13442-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13442-402.IES;Notor 65 Delta;aluminium;7000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;7000;4000;4000;20;65;104;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640736;Notor 65 Delta Continuous;13442-402;64;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
Notor 65 Delta 4K 2400 White Continuous HL DALIPhasePulseControl_13443-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13443-402.IES;Notor 65 Delta;aluminium;10000;Fagerhult_Delta_microprisma;Pendant/surface;Pendant/surface;2506;10000;4000;4000;20;65;115;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640774;Notor 65 Delta Continuous;13443-402;87;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;min. 80
