;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ServiceLifeType##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Right or Left##OTHER##
Notor 65 Delta 3K 400x400 Continuous Anodised DALIPhasePulseControl_13548-402;400;2.5;3000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13548-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644635;Notor 65 Delta Continuous;13548-402;12;1
Notor 65 Delta 3K 400x400 Continuous Anodised DALIPhasePulseControl_13549-402;400;2.5;3000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13549-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644659;Notor 65 Delta Continuous;13549-402;12;0
Notor 65 Delta 4K 400x400 Continuous Anodised DALIPhasePulseControl_13550-402;400;2.5;4000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13550-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644673;Notor 65 Delta Continuous;13550-402;12;1
Notor 65 Delta 4K 400x400 Continuous Anodised DALIPhasePulseControl_13551-402;400;2.5;4000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13551-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644697;Notor 65 Delta Continuous;13551-402;12;0
Notor 65 Delta 3K 400x400 Continuous White DALIPhasePulseControl_13552-402;400;2.5;3000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13552-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046644710;Notor 65 Delta Continuous;13552-402;12;1
Notor 65 Delta 3K 400x400 Continuous White DALIPhasePulseControl_13553-402;400;2.5;3000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13553-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046644734;Notor 65 Delta Continuous;13553-402;12;0
Notor 65 Delta 4K 400x400 Continuous White DALIPhasePulseControl_13554-402;400;2.5;4000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13554-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046644758;Notor 65 Delta Continuous;13554-402;12;1
Notor 65 Delta 4K 400x400 Continuous White DALIPhasePulseControl_13555-402;400;2.5;4000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13555-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046644772;Notor 65 Delta Continuous;13555-402;12;0
Notor 65 Delta 3K 400x400 Continuous Anodised DALIPhasePulseControl_13557-402;400;2.5;3000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13557-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644819;Notor 65 Delta StartSingle;13557-402;12;0
Notor 65 Delta 4K 400x400 Continuous Anodised DALIPhasePulseControl_13559-402;400;2.5;4000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13559-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644857;Notor 65 Delta StartSingle;13559-402;12;0
Notor 65 Delta 3K 400x400 Continuous White DALIPhasePulseControl13561-402;400;2.5;3000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13561-402.IES;Notor 65 Delta;aluminium;983;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;983;3000;3000;20;65;82;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046644895;Notor 65 Delta StartSingle;13561-402;12;0
Notor 65 Delta 4K 400x400 Continuous White DALIPhasePulseControl13563-402;400;2.5;4000;400x400;Rectangle;n/a;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish. The indirect light is covered by an opal film which generates a wide beam and acts as a dust cover. End caps are included in the Start/Single-luminaire.;13563-402.IES;Notor 65 Delta;aluminium;1033;Fagerhult_Delta _microprisma;Pendant/surface;Pendant/surface;400;Luminaire in white RAL 9016  in extruded aluminium. Top cover is a lined diffuser for better light distribution and works as a dust cover. Beta louvre.;1033;4000;4000;20;65;86;Created 14/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046644932;Notor 65 Delta StartSingle;13563-402;12;0
