;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Luminaire design##OTHER##
OPALUME D/I HALF SPHERE 400 STD 1500LM E1 740_306200-22868;7.7;4000;1741;1741;4000;4000;66;375;95;Grey;Aluminium - Fagerhult - Grey;7316911015433;306200-22868;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM E2 740_306200-22869;7.7;4000;1741;1741;4000;4000;66;375;94;Grey;Aluminium - Fagerhult - Grey;7316911015471;306200-22869;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1400LM E3 740_306200-22870;7.7;4000;1641;1641;4000;4000;66;375;88;Grey;Aluminium - Fagerhult - Grey;7316911015501;306200-22870;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM E5 740_306200-22871;7.7;4000;1741;1741;4000;4000;66;375;94;Grey;Aluminium - Fagerhult - Grey;7316911015563;306200-22871;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1400LM E6 740_306200-22872;7.7;4000;1641;1641;4000;4000;66;375;88;Grey;Aluminium - Fagerhult - Grey;7316911015594;306200-22872;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1600LM E9 740_306200-22873;7.7;4000;1841;1841;4000;4000;66;375;98;Grey;Aluminium - Fagerhult - Grey;7316911015655;306200-22873;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L2 740_306200-22874;7.7;4000;1741;1741;4000;4000;66;375;95;Grey;Aluminium - Fagerhult - Grey;7316911015693;306200-22874;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L4 740_306200-22875;7.7;4000;1741;1741;4000;4000;66;375;95;Grey;Aluminium - Fagerhult - Grey;7316911015723;306200-22875;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1400LM L5 740_306200-22876;7.7;4000;1641;1641;4000;4000;66;375;88;Grey;Aluminium - Fagerhult - Grey;7316911015754;306200-22876;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L7 740_306200-22877;7.7;4000;1741;1741;4000;4000;66;375;95;Grey;Aluminium - Fagerhult - Grey;7316911015785;306200-22877;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L8 740_306200-22878;7.7;4000;1741;1741;4000;4000;66;375;93;Grey;Aluminium - Fagerhult - Grey;7316911015815;306200-22878;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1400LM F60 740_306200-22879;7.7;4000;1641;1641;4000;4000;66;375;88;Grey;Aluminium - Fagerhult - Grey;7316911015846;306200-22879;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L9 740_306200-22920;7.7;4000;1741;1741;4000;4000;66;375;93;Grey;Aluminium - Fagerhult - Grey;7316911019578;306200-22920;16;16;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 500 STD 17600LM E1 740_306200-22941;14.9;4000;17866;17866;4000;4000;66;375;144;Grey;Aluminium - Fagerhult - Grey;7316911022035;306200-22941;123;123;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17100LM E2 740_306200-22942;14.9;4000;17366;17366;4000;4000;66;375;140;Grey;Aluminium - Fagerhult - Grey;7316911022066;306200-22942;123;123;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16200LM E3 740_306200-22943;14.9;4000;16466;16466;4000;4000;66;375;133;Grey;Aluminium - Fagerhult - Grey;7316911022103;306200-22943;122;122;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17500LM E5 740_306200-22944;14.9;4000;17766;17766;4000;4000;66;375;143;Grey;Aluminium - Fagerhult - Grey;7316911022134;306200-22944;123;123;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16100LM E6 740_306200-22945;14.9;4000;16366;16366;4000;4000;66;375;132;Grey;Aluminium - Fagerhult - Grey;7316911022165;306200-22945;122;122;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17300LM E9 740_306200-22946;14.9;4000;17566;17566;4000;4000;66;375;141;Grey;Aluminium - Fagerhult - Grey;7316911022196;306200-22946;123;123;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17600LM L2 740_306200-22947;14.9;4000;17866;17866;4000;4000;66;375;144;Grey;Aluminium - Fagerhult - Grey;7316911022233;306200-22947;122;122;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17500LM L4 740_306200-22948;14.9;4000;17766;17766;4000;4000;66;375;143;Grey;Aluminium - Fagerhult - Grey;7316911022288;306200-22948;122;122;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16200LM L5 740_306200-22949;14.9;4000;16466;16466;4000;4000;66;375;132;Grey;Aluminium - Fagerhult - Grey;7316911022325;306200-22949;123;123;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17500LM L7 740_306200-22950;14.9;4000;17766;17766;4000;4000;66;375;143;Grey;Aluminium - Fagerhult - Grey;7316911022370;306200-22950;122;122;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17100LM L8 740_306200-22951;14.9;4000;17366;17366;4000;4000;66;375;140;Grey;Aluminium - Fagerhult - Grey;7316911022424;306200-22951;122;122;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17100LM L9 740_306200-22952;14.9;4000;17366;17366;4000;4000;66;375;140;Grey;Aluminium - Fagerhult - Grey;7316911022462;306200-22952;123;123;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16300LM F60 740_306200-22953;14.9;4000;16566;16566;4000;4000;66;375;133;Grey;Aluminium - Fagerhult - Grey;7316911022516;306200-22953;123;123;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 400 STD 1500LM L11 740_306200-24774;7.7;4000;1741;1741;4000;4000;66;375;91;Grey;Aluminium - Fagerhult - Grey;7316912478572;306200-24774;17;17;400;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 500 STD 16900LM L11 740_306200-24788;14.9;4000;17166;17166;4000;4000;66;375;139;Grey;Aluminium - Fagerhult - Grey;7316912492653;306200-24788;122;122;507;Opalume Catenary;Luminaire for wire installation, Ø 6-12 mm. The luminaire can be angled ±25°, in instances where the wire is not suspended horizontally over the roadway, and rotated ±130°, where the wire is not suspended perpendicular to the roadway.;Suspended luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Its specifically optimised light pattern with AGC lenses have been developed for road lighting. Its innovative and smart suspension design ensures efficient installation.;min. 70;D;1;3
