;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Sensor##OTHER##
INDUFLEX 1200 DALI HL WIDE 840_32100-20009;104;3.5;4000;16731;Acrylic - Fagerhult - Lens;1376;16731;4000;4000;23;68;167;Alu-zinc;Aluminium - Fagerhult - Alu-zinc;7316910408137;32100-20009;108.5;108.5;Induflex;Surface mounted or suspended via the integrated bracket. Installation via tube, chain pendent and wall, see accessories.;Reliable and powerful luminaire in alu-zinc with acrylic lens for optimal glare reduction. Narrow, medium or wide beam light distribution.;min. 80;C;1;0
INDUFLEX 1200 DALI HL MEDIUM 840_32100-20010;104;3.5;4000;17101;Acrylic - Fagerhult - Lens;1376;17101;4000;4000;23;68;170;Alu-zinc;Aluminium - Fagerhult - Alu-zinc;7316910408151;32100-20010;108.5;108.5;Induflex;Surface mounted or suspended via the integrated bracket. Installation via tube, chain pendent and wall, see accessories.;Reliable and powerful luminaire in alu-zinc with acrylic lens for optimal glare reduction. Narrow, medium or wide beam light distribution.;min. 80;C;1;0
INDUFLEX 1500 DALI HL WIDE 840_32100-20012;104;4.2;4000;20914;Acrylic - Fagerhult - Lens;1668;20914;4000;4000;23;68;169;Alu-zinc;Aluminium - Fagerhult - Alu-zinc;7316910408199;32100-20012;135;135;Induflex;Surface mounted or suspended via the integrated bracket. Installation via tube, chain pendent and wall, see accessories.;Reliable and powerful luminaire in alu-zinc with acrylic lens for optimal glare reduction. Narrow, medium or wide beam light distribution.;min. 80;C;1;0
INDUFLEX 1200 DALI HL NARROW 840_32100-20011;104;3.5;4000;17186;Acrylic - Fagerhult - Lens;1376;17186;4000;4000;23;68;171;Alu-zinc;Aluminium - Fagerhult - Alu-zinc;7316910408175;32100-20011;108.5;108.5;Induflex;Surface mounted or suspended via the integrated bracket. Installation via tube, chain pendent and wall, see accessories.;Reliable and powerful luminaire in alu-zinc with acrylic lens for optimal glare reduction. Narrow, medium or wide beam light distribution.;min. 80;C;1;0
INDUFLEX 1500 DALI HL MEDIUM 840_32100-20013;104;4.2;4000;21493;Acrylic - Fagerhult - Lens;1668;21493;4000;4000;23;68;174;Alu-zinc;Aluminium - Fagerhult - Alu-zinc;7316910408212;32100-20013;135;135;Induflex;Surface mounted or suspended via the integrated bracket. Installation via tube, chain pendent and wall, see accessories.;Reliable and powerful luminaire in alu-zinc with acrylic lens for optimal glare reduction. Narrow, medium or wide beam light distribution.;min. 80;C;1;0
INDUFLEX 1500 DALI HL NARROW 840_32100-20014;104;4.2;4000;21482;Acrylic - Fagerhult - Lens;1668;21482;4000;4000;23;68;174;Alu-zinc;Aluminium - Fagerhult - Alu-zinc;7316910408236;32100-20014;135;135;Induflex;Surface mounted or suspended via the integrated bracket. Installation via tube, chain pendent and wall, see accessories.;Reliable and powerful luminaire in alu-zinc with acrylic lens for optimal glare reduction. Narrow, medium or wide beam light distribution.;min. 80;C;1;0
