;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;BIM Version##OTHER##;Type Zhaga##OTHER##
EVOLUME 1 G2 STD 3700LM E1 740_550500-20109;350;6.8;4000;3700;Glass - Fagerhult - Clear;538;3700;4000;4000;66;88;154;Grey;Aluminium - Fagerhult - Grey;7316910086335;550500-20109;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3500LM E2 740_550500-20110;350;6.8;4000;3500;Glass - Fagerhult - Clear;538;3500;4000;4000;66;88;146;Grey;Aluminium - Fagerhult - Grey;7316910086397;550500-20110;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3100LM E3 740_550500-20111;350;6.8;4000;3100;Glass - Fagerhult - Clear;538;3100;4000;4000;66;88;129;Grey;Aluminium - Fagerhult - Grey;7316910086458;550500-20111;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3600LM E5 740_550500-20112;350;6.8;4000;3600;Glass - Fagerhult - Clear;538;3600;4000;4000;66;88;150;Grey;Aluminium - Fagerhult - Grey;7316910086519;550500-20112;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3200LM E6 740_550500-20113;350;6.8;4000;3200;Glass - Fagerhult - Clear;538;3200;4000;4000;66;88;133;Grey;Aluminium - Fagerhult - Grey;7316910086571;550500-20113;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3700LM L2 740_550500-20114;350;6.8;4000;3700;Glass - Fagerhult - Clear;538;3700;4000;4000;66;88;154;Grey;Aluminium - Fagerhult - Grey;7316910086632;550500-20114;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3700LM L4 740_550500-20115;350;6.8;4000;3700;Glass - Fagerhult - Clear;538;3700;4000;4000;66;88;154;Grey;Aluminium - Fagerhult - Grey;7316910086663;550500-20115;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3400LM L6 740_550500-20116;350;6.8;4000;3400;Glass - Fagerhult - Clear;538;3400;4000;4000;66;88;142;Grey;Aluminium - Fagerhult - Grey;7316910086694;550500-20116;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3700LM L7 740_550500-20117;350;6.8;4000;3700;Glass - Fagerhult - Clear;538;3700;4000;4000;66;88;150;Grey;Aluminium - Fagerhult - Grey;7316910086762;550500-20117;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 3300LM F60 740_550500-20118;350;6.8;4000;3300;Glass - Fagerhult - Clear;538;3300;4000;4000;66;88;138;Grey;Aluminium - Fagerhult - Grey;7316910086793;550500-20118;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 20400LM E1 740_550500-20119;350;6.8;4000;20400;Glass - Fagerhult - Clear;538;20400;4000;4000;66;88;141;Grey;Aluminium - Fagerhult - Grey;7316910086854;550500-20119;150;150;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 19400LM E2 740_550500-20120;350;6.8;4000;19400;Glass - Fagerhult - Clear;538;19400;4000;4000;66;88;134;Grey;Aluminium - Fagerhult - Grey;7316910086915;550500-20120;150;150;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 17200LM E3 740_550500-20121;350;6.8;4000;17200;Glass - Fagerhult - Clear;538;17200;4000;4000;66;88;119;Grey;Aluminium - Fagerhult - Grey;7316910086991;550500-20121;150;150;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 20000LM E5 740_550500-20122;350;6.8;4000;20000;Glass - Fagerhult - Clear;538;20000;4000;4000;66;88;137;Grey;Aluminium - Fagerhult - Grey;7316910087059;550500-20122;151;151;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 17600LM E6 740_550500-20123;350;6.8;4000;17600;Glass - Fagerhult - Clear;538;17600;4000;4000;66;88;121;Grey;Aluminium - Fagerhult - Grey;7316910087127;550500-20123;151;151;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 20200LM L2 740_550500-20124;350;6.8;4000;20200;Glass - Fagerhult - Clear;538;20200;4000;4000;66;88;139;Grey;Aluminium - Fagerhult - Grey;7316910087189;550500-20124;150;150;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 20300LM L4 740_550500-20125;350;6.8;4000;20300;Glass - Fagerhult - Clear;538;20300;4000;4000;66;88;139;Grey;Aluminium - Fagerhult - Grey;7316910087240;550500-20125;151;151;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 18900LM L6 740_550500-20126;350;6.8;4000;18900;Glass - Fagerhult - Clear;538;18900;4000;4000;66;88;129;Grey;Aluminium - Fagerhult - Grey;7316910087271;550500-20126;151;151;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 20300LM L7 740_550500-20127;350;6.8;4000;20300;Glass - Fagerhult - Clear;538;20300;4000;4000;66;88;140;Grey;Aluminium - Fagerhult - Grey;7316910087332;550500-20127;150;150;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
EVOLUME 1 G2 STD 19000LM F60 740_550500-20128;350;6.8;4000;19000;Glass - Fagerhult - Clear;538;19000;4000;4000;66;88;130;Grey;Aluminium - Fagerhult - Grey;7316910087370;550500-20128;151;151;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º. ;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire.;min. 70;1;0
