;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type Zhaga##OTHER##
EVOLUME 1 G2 STD 3700LM E1 740_550500-20109;350;6.8;4000;3700;538;3700;4000;4000;66;88;154;Grey;Aluminium - Fagerhult - Grey;7316910086335;550500-20109;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3500LM E2 740_550500-20110;350;6.8;4000;3500;538;3500;4000;4000;66;88;146;Grey;Aluminium - Fagerhult - Grey;7316910086397;550500-20110;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3100LM E3 740_550500-20111;350;6.8;4000;3100;538;3100;4000;4000;66;88;129;Grey;Aluminium - Fagerhult - Grey;7316910086458;550500-20111;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3600LM E5 740_550500-20112;350;6.8;4000;3600;538;3600;4000;4000;66;88;150;Grey;Aluminium - Fagerhult - Grey;7316910086519;550500-20112;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3200LM E6 740_550500-20113;350;6.8;4000;3200;538;3200;4000;4000;66;88;133;Grey;Aluminium - Fagerhult - Grey;7316910086571;550500-20113;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3700LM L2 740_550500-20114;350;6.8;4000;3700;538;3700;4000;4000;66;88;154;Grey;Aluminium - Fagerhult - Grey;7316910086632;550500-20114;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3700LM L4 740_550500-20115;350;6.8;4000;3700;538;3700;4000;4000;66;88;154;Grey;Aluminium - Fagerhult - Grey;7316910086663;550500-20115;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3400LM L6 740_550500-20116;350;6.8;4000;3400;538;3400;4000;4000;66;88;142;Grey;Aluminium - Fagerhult - Grey;7316910086694;550500-20116;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3700LM L7 740_550500-20117;350;6.8;4000;3700;538;3700;4000;4000;66;88;150;Grey;Aluminium - Fagerhult - Grey;7316910086762;550500-20117;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3300LM F60 740_550500-20118;350;6.8;4000;3300;538;3300;4000;4000;66;88;138;Grey;Aluminium - Fagerhult - Grey;7316910086793;550500-20118;24;24;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 20400LM E1 740_550500-20119;350;6.8;4000;20400;538;20400;4000;4000;66;88;141;Grey;Aluminium - Fagerhult - Grey;7316910086854;550500-20119;145;145;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 19400LM E2 740_550500-20120;350;6.8;4000;19400;538;19400;4000;4000;66;88;134;Grey;Aluminium - Fagerhult - Grey;7316910086915;550500-20120;145;145;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 17200LM E3 740_550500-20121;350;6.8;4000;17200;538;17200;4000;4000;66;88;119;Grey;Aluminium - Fagerhult - Grey;7316910086991;550500-20121;145;145;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 20000LM E5 740_550500-20122;350;6.8;4000;20000;538;20000;4000;4000;66;88;137;Grey;Aluminium - Fagerhult - Grey;7316910087059;550500-20122;146;146;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 17600LM E6 740_550500-20123;350;6.8;4000;17600;538;17600;4000;4000;66;88;121;Grey;Aluminium - Fagerhult - Grey;7316910087127;550500-20123;146;146;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 20200LM L2 740_550500-20124;350;6.8;4000;20200;538;20200;4000;4000;66;88;139;Grey;Aluminium - Fagerhult - Grey;7316910087189;550500-20124;145;145;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 20300LM L4 740_550500-20125;350;6.8;4000;20300;538;20300;4000;4000;66;88;139;Grey;Aluminium - Fagerhult - Grey;7316910087240;550500-20125;146;146;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 18900LM L6 740_550500-20126;350;6.8;4000;18900;538;18900;4000;4000;66;88;129;Grey;Aluminium - Fagerhult - Grey;7316910087271;550500-20126;146;146;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 20300LM L7 740_550500-20127;350;6.8;4000;20300;538;20300;4000;4000;66;88;140;Grey;Aluminium - Fagerhult - Grey;7316910087332;550500-20127;145;145;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 19000LM F60 740_550500-20128;350;6.8;4000;19000;538;19000;4000;4000;66;88;130;Grey;Aluminium - Fagerhult - Grey;7316910087370;550500-20128;146;146;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3500LM L11 740_550500-35531;350;7.7;4000;3500;538;3500;4000;4000;66;88;143;Grey;Aluminium - Fagerhult - Grey;7316912145740;550500-35531;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 19300LM L11 740_550500-35532;350;9.3;4000;19300;538;19300;4000;4000;66;88;133;Grey;Aluminium - Fagerhult - Grey;7316912145795;550500-35532;146;146;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 3600LM L12 740_550500-38367;350;6.8;4000;3600;538;3600;4000;4000;66;88;145;Grey;Aluminium - Fagerhult - Grey;7316912532847;550500-38367;25;25;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 1 G2 STD 19200LM L12 740_550500-38368;350;6.8;4000;19200;538;19200;4000;4000;66;88;132;Grey;Aluminium - Fagerhult - Grey;7316912532892;550500-38368;145;145;Evolume 1;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
