;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type Zhaga##OTHER##
EVOLUME 75 G2 STD 1300LM E1 740_550500-20088;295;4.8;4000;1300;470;1300;4000;4000;66;77;144;Grey;Aluminium - Fagerhult - Grey;7316910085086;550500-20088;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1300LM E2 740_550500-20089;295;4.8;4000;1300;470;1300;4000;4000;66;77;144;Grey;Aluminium - Fagerhult - Grey;7316910085208;550500-20089;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1100LM E6 740_550500-20092;295;4.8;4000;1100;470;1100;4000;4000;66;77;122;Grey;Aluminium - Fagerhult - Grey;7316910085321;550500-20092;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1100LM E3 740_550500-20091;295;4.8;4000;1100;470;1100;4000;4000;66;77;122;Grey;Aluminium - Fagerhult - Grey;7316910085260;550500-20091;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1300LM L2 740_550500-20093;295;4.8;4000;1300;470;1300;4000;4000;66;77;144;Grey;Aluminium - Fagerhult - Grey;7316910085369;550500-20093;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1300LM L4 740_550500-20094;295;4.8;4000;1300;470;1300;4000;4000;66;77;144;Grey;Aluminium - Fagerhult - Grey;7316910085390;550500-20094;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1300LM E5 740_550500-20095;295;4.8;4000;1300;470;1300;4000;4000;66;77;144;Grey;Aluminium - Fagerhult - Grey;7316910085437;550500-20095;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1200LM L6 740_550500-20096;295;4.8;4000;1200;470;1200;4000;4000;66;77;133;Grey;Aluminium - Fagerhult - Grey;7316910085482;550500-20096;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1300LM L7 740_550500-20097;295;4.8;4000;1300;470;1300;4000;4000;66;77;144;Grey;Aluminium - Fagerhult - Grey;7316910085543;550500-20097;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1200LM F60 740_550500-20098;295;4.8;4000;1200;470;1200;4000;4000;66;77;133;Grey;Aluminium - Fagerhult - Grey;7316910085574;550500-20098;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 10100LM E1 740_550500-20099;295;4.8;4000;10100;470;10100;4000;4000;66;77;144;Grey;Aluminium - Fagerhult - Grey;7316910085635;550500-20099;70;70;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 9700LM E2 740_550500-20100;295;4.8;4000;9700;470;9700;4000;4000;66;77;141;Grey;Aluminium - Fagerhult - Grey;7316910085734;550500-20100;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 10000LM E5 740_550500-20102;295;4.8;4000;10000;470;10000;4000;4000;66;77;145;Grey;Aluminium - Fagerhult - Grey;7316910085895;550500-20102;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 8600LM E3 740_550500-20101;295;4.8;4000;8600;470;8600;4000;4000;66;77;125;Grey;Aluminium - Fagerhult - Grey;7316910085819;550500-20101;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 8400LM E6 740_550500-20103;295;4.8;4000;8400;470;8400;4000;4000;66;77;122;Grey;Aluminium - Fagerhult - Grey;7316910085970;550500-20103;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 9800LM L6 740_550500-20106;295;4.8;4000;9800;470;9800;4000;4000;66;77;140;Grey;Aluminium - Fagerhult - Grey;7316910086113;550500-20106;70;70;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 10100LM L4 740_550500-20105;295;4.8;4000;10100;470;10100;4000;4000;66;77;146;Grey;Aluminium - Fagerhult - Grey;7316910086083;550500-20105;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 10000LM L2 740_550500-20104;295;4.8;4000;10000;470;10000;4000;4000;66;77;145;Grey;Aluminium - Fagerhult - Grey;7316910086052;550500-20104;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 10100LM L7 740_550500-20107;295;4.8;4000;10100;470;10100;4000;4000;66;77;146;Grey;Aluminium - Fagerhult - Grey;7316910086182;550500-20107;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 9500LM F60 740_550500-20108;295;4.8;4000;9500;470;9500;4000;4000;66;77;138;Grey;Aluminium - Fagerhult - Grey;7316910086250;550500-20108;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 1200LM L11 740_550500-35529;295;6.4;4000;1200;470;1200;4000;4000;66;77;136;Grey;Aluminium - Fagerhult - Grey;7316912145535;550500-35529;9;9;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 9500LM L11 740_550500-35530;295;7.1;4000;9500;470;9500;4000;4000;66;77;137;Grey;Aluminium - Fagerhult - Grey;7316912145603;550500-35530;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 2400LM L12 740_550500-38364;295;4.8;4000;2400;470;2400;4000;4000;66;77;146;Grey;Aluminium - Fagerhult - Grey;7316912532748;550500-38364;16;16;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
EVOLUME 75 G2 STD 9600LM L12 740_550500-38366;295;4.8;4000;9600;470;9600;4000;4000;66;77;139;Grey;Aluminium - Fagerhult - Grey;7316912532793;550500-38366;69;69;Evolume 75;Luminaire for installation on Ø48-60 mm post tops or post arms. Accessories for other installation cases are ordered separately: see Accessories. Tiltable ±15º.;Lamppost luminaire with high performance and light comfort. Optimised beam with AGC lenses designed for road lighting. CLO by default for constant luminous flux over the working life of the luminaire. The luminaire has selectable properties to minimise the impact on the environment: Bioinclusive Lighting.;min. 70;D;1;0
