;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
APPAREO G2 RECTANGULAR 3000K WHITE_11083-402;374;4.7;3000;5336;Plastic - Fagerhult - Delta Microprism;1255;5336;3000;3000;20;28;141;White;Aluminium - Fagerhult - White;7320046717384;11083-402;39.5;39.5;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 3000K BLACK_11084-402;374;4.7;3000;5336;Plastic - Fagerhult - Delta Microprism;1255;5336;3000;3000;20;28;140;Black;Aluminium - Fagerhult - Black;7320046717391;11084-402;40;40;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 3000K BLACK_11084-539;374;4.7;3000;5336;Plastic - Fagerhult - Delta Microprism;1255;5336;3000;3000;20;28;140;Black;Aluminium - Fagerhult - Black;7320047915284;11084-539;40;40;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 4000K WHITE_11085-402;374;4.7;4000;5490;Plastic - Fagerhult - Delta Microprism;1255;5490;4000;4000;20;28;145;White;Aluminium - Fagerhult - White;7320046717728;11085-402;39.5;39.5;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 4000K WHITE_11085-539;374;4.7;4000;5490;Plastic - Fagerhult - Delta Microprism;1255;5490;4000;4000;20;28;145;White;Aluminium - Fagerhult - White;7320047651731;11085-539;39.5;39.5;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 4000K BLACK_11086-402;374;4.7;4000;5490;Plastic - Fagerhult - Delta Microprism;1255;5490;4000;4000;20;28;144;Black;Aluminium - Fagerhult - Black;7320046717759;11086-402;40;40;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 4000K WHITE TRANSP CABLE_11090-402;374;4.7;4000;5490;Plastic - Fagerhult - Delta Microprism;1255;5490;4000;4000;20;28;145;White;Aluminium - Fagerhult - White;7320046721152;11090-402;39.5;39.5;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 4000K BLACK TRANSP CABLE_11091-402;374;4.7;4000;5490;Plastic - Fagerhult - Delta Microprism;1255;5490;4000;4000;20;28;144;Black;Aluminium - Fagerhult - Black;7320046721169;11091-402;40;40;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR TW WHITE TRANSP CABLE_11093;374;4.7;4000;5047;Plastic - Fagerhult - Delta Microprism;1255;5047;4000;4000;20;28;122;White;Aluminium - Fagerhult - White;7320048350169;11093;43.5;43.5;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 90;D;1
APPAREO G2 RECTANGULAR TW BLACK TRANSP CABLE_11094;374;4.7;4000;5047;Plastic - Fagerhult - Delta Microprism;1255;5047;4000;4000;20;28;113;Black;Aluminium - Fagerhult - Black;7320048350176;11094;46.5;46.5;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 90;D;1
APPAREO G2 RECTANGULAR 3000K WHITE_11083-539;374;4.7;3000;5336;Plastic - Fagerhult - Delta Microprism;1255;5336;3000;3000;20;28;141;White;Aluminium - Fagerhult - White;7320048150905;11083-539;39.5;39.5;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
APPAREO G2 RECTANGULAR 4000K BLACK_11086-539;374;4.7;4000;5490;Plastic - Fagerhult - Delta Microprism;1255;5490;4000;4000;20;28;144;Black;Aluminium - Fagerhult - Black;7320048150912;11086-539;40;40;Appareo;Two-point wire pendant. Wire suspension and friction lock included with luminaire. Balanced. External ballast box is mounted directly to ceiling or placed loosely above ceiling.;A suspended workplace luminaire with side-emitting LEDs that produce direct/indirect light. Appareo combines uncompromising design with good ergonomics.;min. 80;C;1
