;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Organic Respons##OTHER##;Type##OTHER##
KVISTEN PEND DELTA 50/50 1200 DALI 840_14100-20005;72;2.1;4000;4050;Acrylic - Fagerhult - Delta Microprism;1236;4050;4000;4000;20;75;144;Birch;Wood - Fagerhult - Pine plywood;7316910899881;14100-20005;29.5;29.5;Kvisten;Pendant. Height adjustment of the wire via friction lock in the luminaire.;A suspended workplace luminaire with a strong focus on sustainability. With a wooden frame, recycled reflectors, and reduced plastic components, the luminaire is made up of 77% recycled or renewable material. Beyond its construction, Kvisten offers exceptional operation efficiency and optimal lit experience.;min. 80;C;1;0;2
KVISTEN PEND DELTA 50/50 1200 840_14100-20008;72;2.2;4000;4050;Acrylic - Fagerhult - Delta Microprism;1236;4050;4000;4000;20;75;141;Birch;Wood - Fagerhult - Pine plywood;7316910899911;14100-20008;30.5;30.5;Kvisten;Pendant. Height adjustment of the wire via friction lock in the luminaire.;A suspended workplace luminaire with a strong focus on sustainability. With a wooden frame, recycled reflectors, and reduced plastic components, the luminaire is made up of 77% recycled or renewable material. Beyond its construction, Kvisten offers exceptional operation efficiency and optimal lit experience.;min. 80;C;1;1;2
KVISTEN PEND DELTA D 1200 DALI 840_14100-20009;72;2.1;4000;1820;Acrylic - Fagerhult - Delta Microprism;1236;1820;4000;4000;20;75;138;Birch;Wood - Fagerhult - Pine plywood;7316910899997;14100-20009;14;14;Kvisten;Pendant. Height adjustment of the wire via friction lock in the luminaire.;A suspended workplace luminaire with a strong focus on sustainability. With a wooden frame, recycled reflectors, and reduced plastic components, the luminaire is made up of 77% recycled or renewable material. Beyond its construction, Kvisten offers exceptional operation efficiency and optimal lit experience.;min. 80;C;1;0;1
KVISTEN PEND DELTA D 1200 840_14100-20010;72;2.2;4000;1820;Acrylic - Fagerhult - Delta Microprism;1236;1820;4000;4000;20;75;139;Birch;Wood - Fagerhult - Pine plywood;7316910900020;14100-20010;14.5;14.5;Kvisten;Pendant. Height adjustment of the wire via friction lock in the luminaire.;A suspended workplace luminaire with a strong focus on sustainability. With a wooden frame, recycled reflectors, and reduced plastic components, the luminaire is made up of 77% recycled or renewable material. Beyond its construction, Kvisten offers exceptional operation efficiency and optimal lit experience.;min. 80;C;1;1;1
