;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;BIM Version##OTHER##
OPALUME OVO 400 DALI 2300LM E1 740_306200-21028;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;106;Grey;Steel - Fagerhult - Grey;7320049666283;306200-21028;23;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM E2 740_306200-21029;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;104;Grey;Steel - Fagerhult - Grey;7320049666344;306200-21029;23;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM E3 740_306200-21030;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;98;Grey;Steel - Fagerhult - Grey;7320049666405;306200-21030;24.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM E5 740_306200-21031;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;105;Grey;Steel - Fagerhult - Grey;7320049666467;306200-21031;23;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM E6 740_306200-21032;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;98;Grey;Steel - Fagerhult - Grey;7320049666528;306200-21032;24.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM E9 740_306200-21033;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;106;Grey;Steel - Fagerhult - Grey;7320049666580;306200-21033;23;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM L2 740_306200-21034;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;106;Grey;Steel - Fagerhult - Grey;7320049666641;306200-21034;23;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM L4 740_306200-21035;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;105;Grey;Steel - Fagerhult - Grey;7320049666702;306200-21035;23;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM L5 740_306200-21036;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;99;Grey;Steel - Fagerhult - Grey;7320049666764;306200-21036;24.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM L7 740_306200-21037;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;106;Grey;Steel - Fagerhult - Grey;7320049666832;306200-21037;23;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 2300LM L9 740_306200-21038;390;10.1;4000;2300;Acrylic - Fagerhult - Opal;2300;4000;4000;66;318;103;Grey;Steel - Fagerhult - Grey;7320049666894;306200-21038;23.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM E1 740_306200-21039;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;126;Grey;Steel - Fagerhult - Grey;7320049666955;306200-21039;67.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM E2 740_306200-21040;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;122;Grey;Steel - Fagerhult - Grey;7320049667013;306200-21040;70;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM E3 740_306200-21041;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;114;Grey;Steel - Fagerhult - Grey;7320049667075;306200-21041;75;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM E5 740_306200-21042;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;125;Grey;Steel - Fagerhult - Grey;7320049667136;306200-21042;68.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM E6 740_306200-21043;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;113;Grey;Steel - Fagerhult - Grey;7320049667198;306200-21043;75;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM E9 740_306200-21044;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;125;Grey;Steel - Fagerhult - Grey;7320049667259;306200-21044;68.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM L2 740_306200-21045;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;126;Grey;Steel - Fagerhult - Grey;7320049667310;306200-21045;68;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM L4 740_306200-21046;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;124;Grey;Steel - Fagerhult - Grey;7320049667372;306200-21046;69;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM L5 740_306200-21047;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;116;Grey;Steel - Fagerhult - Grey;7320049667440;306200-21047;73.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM L9 740_306200-21048;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;122;Grey;Steel - Fagerhult - Grey;7320049667518;306200-21048;70;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1
OPALUME OVO 400 DALI 8000LM L7 740_306200-21049;390;10.1;4000;8000;Acrylic - Fagerhult - Opal;8000;4000;4000;66;318;127;Grey;Steel - Fagerhult - Grey;7320049667570;306200-21049;67.5;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;1

