;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
OPALUME D/I OVO 400 STD 1500LM E1 740_306200-22892;390;10.1;4000;1741;1741;4000;4000;66;318;95;Grey;Aluminium - Fagerhult - Grey;7316911016348;306200-22892;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM E2 740_306200-22893;390;10.1;4000;1741;1741;4000;4000;66;318;94;Grey;Aluminium - Fagerhult - Grey;7316911016393;306200-22893;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1400LM E3 740_306200-22894;390;10.1;4000;1641;1641;4000;4000;66;318;88;Grey;Aluminium - Fagerhult - Grey;7316911016423;306200-22894;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1400LM E6 740_306200-22896;390;10.1;4000;1641;1641;4000;4000;66;318;88;Grey;Aluminium - Fagerhult - Grey;7316911016508;306200-22896;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM E5 740_306200-22895;390;10.1;4000;1741;1741;4000;4000;66;318;94;Grey;Aluminium - Fagerhult - Grey;7316911016461;306200-22895;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1600LM E9 740_306200-22897;390;10.1;4000;1841;1841;4000;4000;66;318;98;Grey;Aluminium - Fagerhult - Grey;7316911016539;306200-22897;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM L2 740_306200-22898;390;10.1;4000;1741;1741;4000;4000;66;318;95;Grey;Aluminium - Fagerhult - Grey;7316911016560;306200-22898;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM L4 740_306200-22899;390;10.1;4000;1741;1741;4000;4000;66;318;95;Grey;Aluminium - Fagerhult - Grey;7316911016591;306200-22899;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1400LM L5 740_306200-22900;390;10.1;4000;1641;1641;4000;4000;66;318;88;Grey;Aluminium - Fagerhult - Grey;7316911016621;306200-22900;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM L7 740_306200-22901;390;10.1;4000;1741;1741;4000;4000;66;318;95;Grey;Aluminium - Fagerhult - Grey;7316911016652;306200-22901;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM L8 740_306200-22902;390;10.1;4000;1741;1741;4000;4000;66;318;93;Grey;Aluminium - Fagerhult - Grey;7316911016683;306200-22902;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1400LM F60 740_306200-22903;390;10.1;4000;1641;1641;4000;4000;66;318;88;Grey;Aluminium - Fagerhult - Grey;7316911016713;306200-22903;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM L9 740_306200-22922;390;10.1;4000;1741;1741;4000;4000;66;318;93;Grey;Aluminium - Fagerhult - Grey;7316911019790;306200-22922;16;16;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6800LM E1 740_306200-22954;390;10.1;4000;7046;7046;4000;4000;66;318;132;Grey;Aluminium - Fagerhult - Grey;7316911022554;306200-22954;52;52;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6600LM E2 740_306200-22955;390;10.1;4000;6846;6846;4000;4000;66;318;129;Grey;Aluminium - Fagerhult - Grey;7316911022646;306200-22955;51;51;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6200LM E3 740_306200-22956;390;10.1;4000;6446;6446;4000;4000;66;318;120;Grey;Aluminium - Fagerhult - Grey;7316911022721;306200-22956;52;52;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6700LM E5 740_306200-22957;390;10.1;4000;6946;6946;4000;4000;66;318;131;Grey;Aluminium - Fagerhult - Grey;7316911022790;306200-22957;51;51;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6700LM E9 740_306200-22959;390;10.1;4000;6946;6946;4000;4000;66;318;131;Grey;Aluminium - Fagerhult - Grey;7316911022899;306200-22959;51;51;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6800LM L2 740_306200-22960;390;10.1;4000;7046;7046;4000;4000;66;318;132;Grey;Aluminium - Fagerhult - Grey;7316911022967;306200-22960;52;52;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6700LM L4 740_306200-22961;390;10.1;4000;6946;6946;4000;4000;66;318;130;Grey;Aluminium - Fagerhult - Grey;7316911023032;306200-22961;52;52;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6200LM L5 740_306200-22962;390;10.1;4000;6446;6446;4000;4000;66;318;121;Grey;Aluminium - Fagerhult - Grey;7316911023094;306200-22962;51;51;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6800LM L7 740_306200-22963;390;10.1;4000;7046;7046;4000;4000;66;318;133;Grey;Aluminium - Fagerhult - Grey;7316911023155;306200-22963;51;51;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6600LM L8 740_306200-22964;390;10.1;4000;6846;6846;4000;4000;66;318;128;Grey;Aluminium - Fagerhult - Grey;7316911023223;306200-22964;52;52;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6600LM L9 740_306200-22965;390;10.1;4000;6846;6846;4000;4000;66;318;129;Grey;Aluminium - Fagerhult - Grey;7316911023285;306200-22965;51;51;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6300LM F60 740_306200-22966;390;10.1;4000;6546;6546;4000;4000;66;318;122;Grey;Aluminium - Fagerhult - Grey;7316911023353;306200-22966;52;52;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6200LM E6 740_306200-22958;390;10.1;4000;6446;6446;4000;4000;66;318;120;Grey;Aluminium - Fagerhult - Grey;7316911023551;306200-22958;52;52;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 1500LM L11 740_306200-24775;390;10.1;4000;1741;1741;4000;4000;66;318;91;Grey;Aluminium - Fagerhult - Grey;7316912478671;306200-24775;17;17;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
OPALUME D/I OVO 400 STD 6400LM L11 740_306200-24789;390;10.1;4000;6646;6646;4000;4000;66;318;125;Grey;Aluminium - Fagerhult - Grey;7316912492714;306200-24789;51;51;390;Opalume Ovo;Luminaire for installation on arm, Ø 48 and Ø 60 mm, with or without external Zhaga socket.;Post luminaire with high performance and light comfort. Exciting design language in the form of half ellipse with capability for RGBW. Optimised light pattern with AGC lenses developed for road lighting. CLO for even output.;min. 70;D;1
