;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Description##OTHER##;Color Rendering Index##Other##;Luminaire design##OTHER##
Opalume Half Sphere 400 DALI 8300LM L4 740_306207-486;10.3;4000;8543;Acrylic - Fagerhult - Opal;8543;4000;4000;66;346;128;Grey;Steel - Fagerhult - Grey;7320047562754;306207-486;71;390;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RBGW. Optimised light pattern with AGC lenses developed for road lighting.;min. 80;2
Opalume Cone 400 DALI 8300LM L4 740_306210-486;10.3;4000;8543;Acrylic - Fagerhult - Opal;8543;4000;4000;66;398;128;Grey;Steel - Fagerhult - Grey;7320047562815;306210-486;71;390;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RBGW. Optimised light pattern with AGC lenses developed for road lighting.;min. 80;1
Opalume Half Sphere 400 DALI 8300LM L4 740_306231-486;10.3;4000;8300;Aluminium - Fagerhult - Grey;8300;4000;4000;66;346;132;Grey;Steel - Fagerhult - Grey;7320047589379;306231-486;67;390;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RBGW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;2
Opalume Half Sphere 500 DALI 15300LM L4 740_306213-486;19.9;4000;15566;Acrylic - Fagerhult - Opal;15566;4000;4000;66;405;137;Grey;Steel - Fagerhult - Grey;7320047562877;306213-486;118;507;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RBGW. Optimised light pattern with AGC lenses developed for road lighting.;min. 80;3
Opalume Cone 500 DALI 15300LM L4 740_306216-486;19.9;4000;15566;Acrylic - Fagerhult - Opal;15566;4000;4000;66;473;137;Grey;Steel - Fagerhult - Grey;7320047562938;306216-486;118;507;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RBGW. Optimised light pattern with AGC lenses developed for road lighting.;min. 80;4

