;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Organic Response##OTHER##
MULTILUME RE:THINK 600X600 OR DELTA HL 840 VTB_24100-20022;595;2.8;4000;4300;Polystyrene - Fagerhult - Delta;595;4300;4000;4000;20;27;147;White;Paper - Fagerhult - White;7320049597761;24100-20022;32.5;32.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1
MULTILUME RE:THINK 600X600 DALI DELTA HL T/W VTB_24100-20024;595;2.7;4000;3260;Polystyrene - Fagerhult - Delta;595;3260;4000;4000;20;27;112;White;Paper - Fagerhult - White;7320049597822;24100-20024;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 90;D;1;0
MULTILUME RE:THINK 600X600 DALI DELTA HL 830 VTB_24100-20027;595;2.7;3000;4081;Polystyrene - Fagerhult - Delta;595;4081;3000;3000;20;27;142;White;Paper - Fagerhult - White;7320049759527;24100-20027;32.5;32.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 600X600 OR DELTA HL 830 VTB_24100-20028;595;2.8;3000;4081;Polystyrene - Fagerhult - Delta;595;4081;3000;3000;20;27;140;White;Paper - Fagerhult - White;7320049759589;24100-20028;32.5;32.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1
MULTILUME RE:THINK 600X600 DALI DELTA HL 840 VTB_24100-20029;595;2.7;4000;4300;Polystyrene - Fagerhult - Delta;595;4300;4000;4000;20;27;150;White;Paper - Fagerhult - White;7320049759626;24100-20029;32.5;32.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X600 DALI DELTA HL 830 VTB_24101-20000;295;1.7;3000;1877;Polystyrene - Fagerhult - Delta;595;1877;3000;3000;20;27;110;White;Paper - Fagerhult - White;7316911114174;24101-20000;18.5;18.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X600 OR DELTA HL 840 VTB_24101-20001;295;1.8;4000;1877;Polystyrene - Fagerhult - Delta;595;1877;4000;4000;20;27;104;White;Paper - Fagerhult - White;7316911114204;24101-20001;19.5;19.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1
MULTILUME RE:THINK 300X600 DALI DELTA HL 840 VTB_24101-20003;295;1.7;4000;1877;Polystyrene - Fagerhult - Delta;595;1877;4000;4000;20;27;110;White;Paper - Fagerhult - White;7316911170385;24101-20003;18.5;18.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X600 OR DELTA HL 830 VTB_24101-20004;295;1.8;3000;1877;Polystyrene - Fagerhult - Delta;595;1877;3000;3000;20;27;104;White;Paper - Fagerhult - White;7316911170415;24101-20004;19.5;19.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1
MULTILUME RE:THINK 300X1200 OR DELTA HL 830 VTB_24102-20001;295;3.5;3000;3764;Polystyrene - Fagerhult - Delta;1195;3764;3000;3000;20;27;120;White;Paper - Fagerhult - White;7316911114372;24102-20001;34;34;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;2
MULTILUME RE:THINK 300X1200 DALI DELTA HL 830 VTB_24102-20003;295;3.4;3000;3764;Polystyrene - Fagerhult - Delta;1195;3764;3000;3000;20;27;123;White;Paper - Fagerhult - White;7316911170606;24102-20003;33.5;33.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X1200 DALI DELTA HL 840 VTB_24102-20004;295;3.4;4000;3764;Polystyrene - Fagerhult - Delta;1195;3764;4000;4000;20;27;123;White;Paper - Fagerhult - White;7316911170637;24102-20004;33.5;33.5;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;2;0
MULTILUME RE:THINK 300X1200 OR DELTA HL 840 VTB_24102-20005;295;3.5;4000;3764;Polystyrene - Fagerhult - Delta;1195;3764;4000;4000;20;27;120;White;Paper - Fagerhult - White;7316911170668;24102-20005;34;34;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;3;2
MULTILUME RE:THINK 300X1200 DALI DELTA HL T/W VTB_24102-20010;295;3.5;4000;2765;Polystyrene - Fagerhult - Delta;1195;2765;4000;4000;20;27;96;White;Paper - Fagerhult - White;7316911170835;24102-20010;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 90;D;4;0

