;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Length Lamells##OTHER##
NOTOR36 REC D 303 DALI HL BETA 830_16087-20452;56;0.4;3000;1361;Aluminium - Fagerhult - Beta Opti Nano;310;1361;3000;3000;20;97;112;White;Aluminium - Fagerhult - White;7316911551528;16087-20452;12;12;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;1
NOTOR36 REC D 303 DALI HL BETA 840_16087-20453;56;0.4;4000;1400;Aluminium - Fagerhult - Beta Opti Nano;310;1400;4000;4000;20;97;115;White;Aluminium - Fagerhult - White;7316911551559;16087-20453;12;12;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;1
NOTOR36 REC D 303 DALI HL BETA 830_16087-20454;56;0.4;3000;1361;Aluminium - Fagerhult - Beta Opti Nano;310;1361;3000;3000;20;97;112;Black;Aluminium - Fagerhult - Black;7316911551597;16087-20454;12;12;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;1
NOTOR36 REC D 440 DALI HL BETA 830_16087-20456;56;0.6;3000;1818;Aluminium - Fagerhult - Beta Opti Nano;446;1818;3000;3000;20;97;114;White;Aluminium - Fagerhult - White;7316911551696;16087-20456;16;16;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;2
NOTOR36 REC D 440 DALI HL BETA 840_16087-20457;56;0.6;4000;1870;Aluminium - Fagerhult - Beta Opti Nano;446;1870;4000;4000;20;97;117;White;Aluminium - Fagerhult - White;7316911551726;16087-20457;16;16;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;2
NOTOR36 REC D 440 DALI HL BETA 830_16087-20458;56;0.6;3000;1818;Aluminium - Fagerhult - Beta Opti Nano;446;1818;3000;3000;20;97;114;Black;Aluminium - Fagerhult - Black;7316911551764;16087-20458;16;16;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;2
NOTOR36 REC D 440 DALI HL BETA 840_16087-20459;56;0.6;4000;1870;Aluminium - Fagerhult - Beta Opti Nano;446;1870;4000;4000;20;97;117;Black;Aluminium - Fagerhult - Black;7316911551863;16087-20459;16;16;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;2
