;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Right##OTHER##
NOTOR 36 L LEFT REC D DALI HL OPAL 840_16087-20188;1.4;4000;2683;Acrylic - Fagerhult - Opal;636;20;82;119;White;Aluminium - Fagerhult - White;7320049576704;16087-20188;24;Notor 36 recessed Opal;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Single or series installation. Spot module for continuous installation.;min. 80;C;1;0
NOTOR 36 L RIGHT REC D DALI HL OPAL 840_16087-20189;1.4;4000;2683;Acrylic - Fagerhult - Opal;636;20;82;119;White;Aluminium - Fagerhult - White;7320049576735;16087-20189;24;Notor 36 recessed Opal;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Single or series installation. Spot module for continuous installation.;min. 80;C;1;1
