;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Tilt Angle##ANGLE##DEGREES;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ServiceLifeDuration##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;Optic##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;DiffuserMaterial##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##;Right or Left##OTHER##
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY ANODISED LL_21908;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21908.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1482;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1482;3000;3000;20;100;106;<By Category>;Standard;Anodised;Fagerhult_Alugrey_Aluminium;7320046512170;Notor recessed LED Opal flush ;21908;14;830;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY ANODISED LL_21909;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21909.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1516;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1516;4000;4000;20;100;108;<By Category>;Standard;Anodised;Fagerhult_Alugrey_Aluminium;7320046512217;Notor recessed LED Opal flush ;21909;14;840;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY ANODISED HL_21910;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21910.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2640;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2640;3000;3000;20;100;106;<By Category>;Standard;Anodised;Fagerhult_Alugrey_Aluminium;7320046512255;Notor recessed LED Opal flush ;21910;25;830;1
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY ANODISED HL_21911;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21911.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2700;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2700;4000;4000;20;100;108;<By Category>;Standard;Anodised;Fagerhult_Alugrey_Aluminium;7320046512293;Notor recessed LED Opal flush ;21911;25;840;1
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY WHITE LL_21912;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21912.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1482;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1482;3000;3000;20;100;106;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046512330;Notor recessed LED Opal flush ;21912;14;830;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY WHITE LL_21913;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21913.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1516;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1516;4000;4000;20;100;108;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046512378;Notor recessed LED Opal flush ;21913;14;840;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY WHITE HL_21914;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21914.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2640;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2640;3000;3000;20;100;106;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046512415;Notor recessed LED Opal flush ;21914;25;830;1
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY WHITE HL_21915;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21915.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2700;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2700;4000;4000;20;100;108;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046512453;Notor recessed LED Opal flush ;21915;25;840;1
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY ANODISED LL_21908-402;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21908-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1482;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1482;3000;3000;20;100;106;<By Category>;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046512194;Notor recessed LED Opal flush ;21908-402;14;830;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY ANODISED LL_21909-402;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21909-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1516;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1516;4000;4000;20;100;108;<By Category>;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046512231;Notor recessed LED Opal flush ;21909-402;14;840;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY ANODISED HL_21910-402;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21910-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2640;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2640;3000;3000;20;100;106;<By Category>;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046512279;Notor recessed LED Opal flush ;21910-402;25;830;1
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY ANODISED HL_21911-402;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21911-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2700;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2700;4000;4000;20;100;108;<By Category>;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046512316;Notor recessed LED Opal flush ;21911-402;25;840;1
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY WHITE LL_21912-402;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21912-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1482;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1482;3000;3000;20;100;106;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046512354;Notor recessed LED Opal flush ;21912-402;14;830;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY WHITE LL_21913-402;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21913-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;1516;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;1516;4000;4000;20;100;108;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046512392;Notor recessed LED Opal flush ;21913-402;14;840;0
NOTOR RECESSED L-COUPLER OPAL FLUSH 3K BODY WHITE HL_21914-402;611;3.5;90;3000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21914-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2640;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2640;3000;3000;20;100;106;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046512439;Notor recessed LED Opal flush ;21914-402;25;830;1
NOTOR RECESSED L-COUPLER OPAL FLUSH 4K BODY WHITE HL_21915-402;611;3.5;90;4000;L 647 mm + W 611 mm + H 100 mm;Rectangle;LED 50,000 hrs;A recessed luminaire for all types of suspended ceilings. Single or continuous installation.;21915-402.IES;<By Category>;Notor recessed LED Opal flush ;aluminium;2700;Fagerhult_Opal;Ceiling;Recessed ;647;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;2700;4000;4000;20;100;108;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046512477;Notor recessed LED Opal flush ;21915-402;25;840;1
