;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY ELOX LL_21916;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21916.IES;Notor recessed LED Opal dropped ;aluminium;1594;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1594;3000;3000;20;100;114;Created 15/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046512491;Notor recessed LED Opal dropped ;21916;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY ELOX LL_21917;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21917.IES;Notor recessed LED Opal dropped ;aluminium;1630;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1630;4000;4000;20;100;116;Created 15/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046512538;Notor recessed LED Opal dropped ;21917;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY ELOX HL_21918;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21918.IES;Notor recessed LED Opal dropped ;aluminium;2836;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2836;3000;3000;20;100;113;Created 15/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046512576;Notor recessed LED Opal dropped ;21918;25;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY ELOX HL_21919;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21919.IES;Notor recessed LED Opal dropped ;aluminium;2902;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2902;4000;4000;20;100;116;Created 15/05/2018;Standard;Anodised;Fagerhult_Anodised;7320046512613;Notor recessed LED Opal dropped ;21919;25;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY WHITE LL_21920;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21920.IES;Notor recessed LED Opal dropped ;aluminium;1594;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1594;3000;3000;20;100;114;Created 15/05/2018;Standard;White;Fagerhult_White_aluminium;7320046512651;Notor recessed LED Opal dropped ;21920;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY WHITE LL_21921;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21921.IES;Notor recessed LED Opal dropped ;aluminium;1630;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1630;4000;4000;20;100;116;Created 15/05/2018;Standard;White;Fagerhult_White_aluminium;7320046512699;Notor recessed LED Opal dropped ;21921;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY WHITE HL_21922;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21922.IES;Notor recessed LED Opal dropped ;aluminium;2836;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2836;3000;3000;20;100;113;Created 15/05/2018;Standard;White;Fagerhult_White_aluminium;7320046512736;Notor recessed LED Opal dropped ;21922;25;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY WHITE HL_21923;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21923.IES;Notor recessed LED Opal dropped ;aluminium;2902;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2902;4000;4000;20;100;116;Created 15/05/2018;Standard;White;Fagerhult_White_aluminium;7320046512774;Notor recessed LED Opal dropped ;21923;25;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY ELOX LL_21916-402;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21916-402.IES;Notor recessed LED Opal dropped ;aluminium;1594;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1594;3000;3000;20;100;114;Created 15/05/2018;DaliPhasePulseControl;Anodised;Fagerhult_Anodised;7320046512514;Notor recessed LED Opal dropped ;21916-402;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY ELOX LL_21917-402;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21917-402.IES;Notor recessed LED Opal dropped ;aluminium;1630;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1630;4000;4000;20;100;116;Created 15/05/2018;DaliPhasePulseControl;Anodised;Fagerhult_Anodised;7320046512552;Notor recessed LED Opal dropped ;21917-402;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY ELOX HL_21918-402;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21918-402.IES;Notor recessed LED Opal dropped ;aluminium;2836;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2836;3000;3000;20;100;113;Created 15/05/2018;DaliPhasePulseControl;Anodised;Fagerhult_Anodised;7320046512590;Notor recessed LED Opal dropped ;21918-402;25;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY ELOX HL_21919-402;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21919-402.IES;Notor recessed LED Opal dropped ;aluminium;2902;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2902;4000;4000;20;100;116;Created 15/05/2018;DaliPhasePulseControl;Anodised;Fagerhult_Anodised;7320046512637;Notor recessed LED Opal dropped ;21919-402;25;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY WHITE LL_21920-402;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21920-402.IES;Notor recessed LED Opal dropped ;aluminium;1594;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1594;3000;3000;20;100;114;Created 15/05/2018;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046512675;Notor recessed LED Opal dropped ;21920-402;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY WHITE LL_21921-402;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21921-402.IES;Notor recessed LED Opal dropped ;aluminium;1630;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;1630;4000;4000;20;100;116;Created 15/05/2018;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046512712;Notor recessed LED Opal dropped ;21921-402;14;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 3K BODY WHITE HL_21922-402;611;3.5;3000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21922-402.IES;Notor recessed LED Opal dropped ;aluminium;2836;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2836;3000;3000;20;100;113;Created 15/05/2018;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046512750;Notor recessed LED Opal dropped ;21922-402;25;min. 80
NOTOR RECESSED L-COUPLER OPAL DROPPED 4K BODY WHITE HL_21923-402;611;3.5;4000;L 647 mm + W 611 mm + H 100 mm;L shape;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;21923-402.IES;Notor recessed LED Opal dropped ;aluminium;2902;Fagerhult_Opal;Ceiling;Recessed ;470;A recessed luminaire for all types of suspended ceilings. The opal louvre lowers the suspended ceiling's surface and creates ambient light on the ceiling. Single or continuous installation.;2902;4000;4000;20;100;116;Created 15/05/2018;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046512798;Notor recessed LED Opal dropped ;21923-402;25;min. 80
