;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
RONDO G3 WALL TWIN NARROW 840 CLO_308045-402;75;4.7;4000;1600;Polycarbonate - Fagerhult - Opal;205;1600;4000;4000;66;244;61;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581793;308045-402;26;26;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE 830 CLO_308040;75;4.7;3000;2604;Polycarbonate - Fagerhult - Opal;205;2604;3000;3000;66;244;100;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581571;308040;26;26;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE 830 CLO_308040-402;75;4.7;3000;2604;Polycarbonate - Fagerhult - Opal;205;2604;3000;3000;66;244;100;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581595;308040-402;26;26;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE 840 CLO_308041;75;4.7;4000;2800;Polycarbonate - Fagerhult - Opal;205;2800;4000;4000;66;244;107;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581618;308041;26;26;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE 840 CLO_308041-402;75;4.7;4000;2800;Polycarbonate - Fagerhult - Opal;205;2800;4000;4000;66;244;107;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581632;308041-402;26;26;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE/NARROW 830 CLO_308042;75;4.7;3000;1488;Polycarbonate - Fagerhult - Opal;205;1488;3000;3000;66;244;89;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581656;308042;17;17;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE/NARROW 830 CLO_308042-402;75;4.7;3000;1488;Polycarbonate - Fagerhult - Opal;205;1488;3000;3000;66;244;89;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581670;308042-402;17;17;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE/NARROW 840 CLO_308043;75;4.7;4000;1600;Polycarbonate - Fagerhult - Opal;205;1600;4000;4000;66;244;96;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581694;308043;17;17;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN WIDE/NARROW 840 CLO_308043-402;75;4.7;4000;1600;Polycarbonate - Fagerhult - Opal;205;1600;4000;4000;66;244;96;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581717;308043-402;17;17;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN NARROW 830 CLO_308044;75;4.7;3000;1488;Polycarbonate - Fagerhult - Opal;205;1488;3000;3000;66;244;55;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581731;308044;27;27;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN NARROW 830 CLO_308044-402;75;4.7;3000;1488;Polycarbonate - Fagerhult - Opal;205;1488;3000;3000;66;244;56;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581755;308044-402;26;26;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
RONDO G3 WALL TWIN NARROW 840 CLO_308045;75;4.7;4000;1600;Polycarbonate - Fagerhult - Opal;205;1600;4000;4000;66;244;59;Anthracite;Aluminium - Fagerhult - Anthracite;7320047581779;308045;27;27;Rondo G3 Twin wall;Luminaire for wall mounting.;Efficient robust wall luminaire in classic cylinder form with up and down lights where the up light is directed inward wall for effect lighting. Wide or narrow beam angle. CLO as standard.;min. 80;E;1
