;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
Notor 65 Opal Start/Single 800 3000K DALIPhasePulseControl Anodised_13445-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13445-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;840;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640811;Notor 65 Opal Start/Single;13445-402;15;min. 80
Notor 65 Opal Start/Single 800 4000K DALIPhasePulseControl Anodised_13447-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13447-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;840;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640859;Notor 65 Opal Start/Single;13447-402;15;min. 80
Notor 65 Opal Start/Single 800 3000K DALIPhasePulseControl White_13449-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13449-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;840;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640897;Notor 65 Opal Start/Single;13449-402;15;min. 80
Notor 65 Opal Start/Single 800 4000K DALIPhasePulseControl White_13451-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13451-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;840;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046640934;Notor 65 Opal Start/Single;13451-402;15;min. 80
Notor 65 Opal Start/Single 1200 3000K DALIPhasePulseControl Anodised_13453-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13453-402.IES;Notor 65 Opal;aluminium;2375;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1256;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2375;3000;3000;20;65;103;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046640972;Notor 65 Opal Start/Single;13453-402;23;min. 80
Notor 65 Opal Start/Single 1200 4000K DALIPhasePulseControl Anodised_13455-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13455-402.IES;Notor 65 Opal;aluminium;2500;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1256;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2500;4000;4000;20;65;109;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641016;Notor 65 Opal Start/Single;13455-402;23;min. 80
Notor 65 Opal Start/Single 1200 3000K DALIPhasePulseControl White_13457-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13457-402.IES;Notor 65 Opal;aluminium;2375;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1256;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2375;3000;3000;20;65;103;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641054;Notor 65 Opal Start/Single;13457-402;23;min. 80
Notor 65 Opal Start/Single 1200 4000K DALIPhasePulseControl White_13459-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13459-402.IES;Notor 65 Opal;aluminium;2500;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1256;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2500;4000;4000;20;65;109;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641092;Notor 65 Opal Start/Single;13459-402;23;min. 80
Notor 65 Opal Start/Single 2400 3000K DALIPhasePulseControl Anodised_13461-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13461-402.IES;Notor 65 Opal;aluminium;4750;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2506;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;4750;3000;3000;20;65;101;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641139;Notor 65 Opal Start/Single;13461-402;47;min. 80
Notor 65 Opal Start/Single 2400 4000K DALIPhasePulseControl Anodised_13463-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13463-402.IES;Notor 65 Opal;aluminium;5000;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2506;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;5000;4000;4000;20;65;106;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641177;Notor 65 Opal Start/Single;13463-402;47;min. 80
Notor 65 Opal Start/Single 2400 3000K DALIPhasePulseControl White_13465-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13465-402.IES;Notor 65 Opal;aluminium;4750;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2506;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;4750;3000;3000;20;65;101;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641214;Notor 65 Opal Start/Single;13465-402;47;min. 80
Notor 65 Opal Start/Single 2400 4000K DALIPhasePulseControl White_13467-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13467-402.IES;Notor 65 Opal;aluminium;5000;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2506;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;5000;4000;4000;20;65;106;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641252;Notor 65 Opal Start/Single;13467-402;47;min. 80
Notor 65 Opal Continuous 800 3000K DALIPhasePulseControl Anodised_13469-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13469-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;836;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641290;Notor 65 Opal Continuous;13469-402;15;min. 80
Notor 65 Opal Continuous 800 4000K DALIPhasePulseControl Anodised_13471-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13471-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;836;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641337;Notor 65 Opal Continuous;13471-402;15;min. 80
Notor 65 Opal Continuous 800 3000K DALIPhasePulseControl White_13473-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13473-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;836;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641375;Notor 65 Opal Continuous;13473-402;15;min. 80
Notor 65 Opal Continuous 800 4000K DALIPhasePulseControl White_13475-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13475-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;836;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641412;Notor 65 Opal Continuous;13475-402;15;min. 80
Notor 65 Opal Continuous 1200 3000K DALIPhasePulseControl Anodised_13477-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13477-402.IES;Notor 65 Opal;aluminium;2375;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1252;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2375;3000;3000;20;65;103;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641450;Notor 65 Opal Continuous;13477-402;23;min. 80
Notor 65 Opal Continuous 1200 4000K DALIPhasePulseControl Anodised_13479-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13479-402.IES;Notor 65 Opal;aluminium;2500;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1252;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2500;4000;4000;20;65;109;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641498;Notor 65 Opal Continuous;13479-402;23;min. 80
Notor 65 Opal Continuous 1200 3000K DALIPhasePulseControl White_13481-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13481-402.IES;Notor 65 Opal;aluminium;2375;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1252;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2375;3000;3000;20;65;103;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641535;Notor 65 Opal Continuous;13481-402;23;min. 80
Notor 65 Opal Continuous 1200 4000K DALIPhasePulseControl White_13483-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13483-402.IES;Notor 65 Opal;aluminium;2500;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1252;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2500;4000;4000;20;65;109;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641573;Notor 65 Opal Continuous;13483-402;23;min. 80
Notor 65 Opal Continuous 2400 3000K DALIPhasePulseControl Anodised_13485-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13485-402.IES;Notor 65 Opal;aluminium;4750;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2502;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;4750;3000;3000;20;65;101;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641610;Notor 65 Opal Continuous;13485-402;47;min. 80
Notor 65 Opal Continuous 2400 4000K DALIPhasePulseControl Anodised_13487-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13487-402.IES;Notor 65 Opal;aluminium;5000;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2502;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;5000;4000;4000;20;65;106;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641658;Notor 65 Opal Continuous;13487-402;47;min. 80
Notor 65 Opal Continuous 2400 3000K DALIPhasePulseControl White_13489-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13489-402.IES;Notor 65 Opal;aluminium;4750;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2502;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;4750;3000;3000;20;65;101;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641696;Notor 65 Opal Continuous;13489-402;47;min. 80
Notor 65 Opal Continuous 2400 4000K DALIPhasePulseControl White_13491-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13491-402.IES;Notor 65 Opal;aluminium;5000;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2502;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;5000;4000;4000;20;65;106;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046641733;Notor 65 Opal Continuous;13491-402;47;min. 80
Notor 65 Opal Start/Single 800 4000K DALIPhasePulseControl Black_13517-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13517-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;840;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643751;Notor 65 Opal Start/Single;13517-402;15;min. 80
Notor 65 Opal Start/Single 800 3000K DALIPhasePulseControl Black_13519-402;65;2.0;3000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13519-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;840;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643775;Notor 65 Opal Start/Single;13519-402;15;min. 80
Notor 65 Opal Start/Single 1200 4000K DALIPhasePulseControl Black_13521-402;65;3.0;4000;L 1200 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13521-402.IES;Notor 65 Opal;aluminium;2375;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1256;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2375;3000;3000;20;65;103;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643799;Notor 65 Opal Start/Single;13521-402;23;min. 80
Notor 65 Opal Start/Single 1200 3000K DALIPhasePulseControl Black_13523-402;65;3.0;3000;L 1200 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13523-402.IES;Notor 65 Opal;aluminium;2500;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1256;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2500;4000;4000;20;65;109;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643812;Notor 65 Opal Start/Single;13523-402;23;min. 80
Notor 65 Opal Start/Single 2400 4000K DALIPhasePulseControl Black_13525-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13525-402.IES;Notor 65 Opal;aluminium;4750;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2506;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;4750;3000;3000;20;65;101;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643836;Notor 65 Opal Start/Single;13525-402;47;min. 80
Notor 65 Opal Start/Single 2400 3000K DALIPhasePulseControl Black_13527-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13527-402.IES;Notor 65 Opal;aluminium;5000;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2506;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;5000;4000;4000;20;65;106;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643850;Notor 65 Opal Start/Single;13527-402;47;min. 80
Notor 65 Opal Continuous 800 4000K DALIPhasePulseControl Black_13529-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13529-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;836;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643874;Notor 65 Opal Continuous;13529-402;15;min. 80
Notor 65 Opal Continuous 800 4000K DALIPhasePulseControl Black_13531-402;65;2.0;4000;L 800 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13531-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;836;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643898;Notor 65 Opal Continuous;13531-402;15;min. 80
Notor 65 Opal Continuous 1200 3000K DALIPhasePulseControl Black_13533-402;65;3.0;3000;L 1200 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13533-402.IES;Notor 65 Opal;aluminium;2375;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1252;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2375;3000;3000;20;65;103;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643911;Notor 65 Opal Continuous;13533-402;23;min. 80
Notor 65 Opal Continuous 1200 3000K DALIPhasePulseControl Black_13535-402;65;3.0;3000;L 1200 mm + W 90,5 mm + H 100 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13535-402.IES;Notor 65 Opal;aluminium;2500;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;1252;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;2500;4000;4000;20;65;109;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643935;Notor 65 Opal Continuous;13535-402;23;min. 80
Notor 65 Opal Continuous 2400 4000K DALIPhasePulseControl Black_13537-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13537-402.IES;Notor 65 Opal;aluminium;4750;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2502;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;4750;3000;3000;20;65;101;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643959;Notor 65 Opal Continuous;13537-402;47;min. 80
Notor 65 Opal Continuous 2400 3000K DALIPhasePulseControl Black_13539-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13539-402.IES;Notor 65 Opal;aluminium;5000;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;2502;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;5000;4000;4000;20;65;106;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643973;Notor 65 Opal Continuous;13539-402;47;min. 80
