;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Right or Left##OTHER##
Notor 65 Opal Illuminated corner, continuous, left 400x400 3000K DALIPhasePulseControl Anodised_13492-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13492-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641771;Notor 65 Opal Illuminated corner, continuous, left;13492-402;15;0
Notor 65 Opal Illuminated corner, continuous, right 400x400 3000K DALIPhasePulseControl Anodised_13493-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13493-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641818;Notor 65 Opal Illuminated corner, continuous, right;13493-402;15;1
Notor 65 Opal Illuminated corner, continuous, left 400x400 4000K DALIPhasePulseControl Anodised_13494-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13494-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641856;Notor 65 Opal Illuminated corner, continuous, left;13494-402;15;0
Notor 65 Opal Illuminated corner, continuous, right 400x400 4000K DALIPhasePulseControl Anodised_13495-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13495-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046641894;Notor 65 Opal Illuminated corner, continuous, right;13495-402;15;1
Notor 65 Opal Illuminated corner, continuous, left 400x400 3000K DALIPhasePulseControl White_13496-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13496-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_Aluminium;7320046641931;Notor 65 Opal Illuminated corner, continuous, left;13496-402;15;0
Notor 65 Opal Illuminated corner, continuous, right 400x400 3000K DALIPhasePulseControl White_13497-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13497-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_Aluminium;7320046641979;Notor 65 Opal Illuminated corner, continuous, right;13497-402;15;1
Notor 65 Opal Illuminated corner, continuous, left 400x400 4000K DALIPhasePulseControl White_13498-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13498-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_Aluminium;7320046642013;Notor 65 Opal Illuminated corner, continuous, left;13498-402;15;0
Notor 65 Opal Illuminated corner, continuous, right 400x400 4000K DALIPhasePulseControl White_13499-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13499-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_Aluminium;7320046642051;Notor 65 Opal Illuminated corner, continuous, right;13499-402;15;1
Notor 65 Opal Illuminated corner, continuous, right 400x400 3000K DALIPhasePulseControl Anodised_13541-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13541-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644178;Notor 65 Opal Illuminated corner, continuous, right;13541-402;15;1
Notor 65 Opal Illuminated corner, continuous, right 400x400 4000K DALIPhasePulseControl Anodised_13543-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13543-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046644215;Notor 65 Opal Illuminated corner, continuous, right;13543-402;15;1
Notor 65 Opal Illuminated corner, continuous, right 400x400 3000K DALIPhasePulseControl White_13545-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13545-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_Aluminium;7320046644253;Notor 65 Opal Illuminated corner, continuous, right;13545-402;15;1
Notor 65 Opal Illuminated corner, continuous, right 400x400 4000K DALIPhasePulseControl White_13547-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13547-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;White;Fagerhult_White_Aluminium;7320046644291;Notor 65 Opal Illuminated corner, continuous, right;13547-402;15;1
Notor 65 Opal Illuminated corner, continuous, right 400x400 3000K DALIPhasePulseControl Black_13565-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13565-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643232;Notor 65 Opal Illuminated corner, continuous, right;13565-402;15;1
Notor 65 Opal Illuminated corner, continuous, right 400x400 4000K DALIPhasePulseControl Black_13567-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13567-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643317;Notor 65 Opal Illuminated corner, continuous, right;13567-402;15;1
Notor 65 Opal Illuminated corner, continuous, left 400x400 3000K DALIPhasePulseControl Black_13568-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13568-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643355;Notor 65 Opal Illuminated corner, continuous, left;13568-402;15;0
Notor 65 Opal Illuminated corner, continuous, right 400x400 3000K DALIPhasePulseControl Black_13569-402;400;2.5;3000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13569-402.IES;Notor 65 Opal;aluminium;1582;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1582;3000;3000;20;65;105;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643393;Notor 65 Opal Illuminated corner, continuous, right;13569-402;15;1
Notor 65 Opal Illuminated corner, continuous, left 400x400 4000K DALIPhasePulseControl Black_13570-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13570-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643430;Notor 65 Opal Illuminated corner, continuous, left;13570-402;15;0
Notor 65 Opal Illuminated corner, continuous, right 400x400 4000K DALIPhasePulseControl Black_13571-402;400;2.5;4000;400x400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;13571-402.IES;Notor 65 Opal;aluminium;1666;Fagerhult_Opal_glass;Pendant/surface;Pendant/surface;400;Luminaire body enameled in white (RAL 9016) alternatively black (RAL 9005) or natural anodised extruded aluminium finish.;1666;4000;4000;20;65;111;Created 19/06/2017;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046643478;Notor 65 Opal Illuminated corner, continuous, right;13571-402;15;1
