;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Size##OTHER##
TERSO LED D250 WHITE 3K _54540-402;2.5;3000;1680;1680;3000;3000;20;300;80;White;Aluminium - Fagerhult - White;7320046849511;54540-402;21;21;250;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;1
TERSO LED D250 WHITE 4K  _54541-402;2.5;4000;1680;1680;4000;4000;20;300;84;White;Aluminium - Fagerhult - White;7320046849528;54541-402;20;20;250;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;1
TERSO LED D250 BLACK 3K  _54542-402;2.5;3000;1680;1680;3000;3000;20;300;80;Black;Aluminium - Fagerhult - Black;7320046849535;54542-402;21;21;250;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;1
TERSO LED D250 BLACK 4K_54543-402;2.5;4000;1680;1680;4000;4000;20;300;84;Black;Aluminium - Fagerhult - Black;7320046849566;54543-402;20;20;250;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;1
TERSO LED D400 WHITE 3K  _54544-402;3.9;3000;2370;2370;3000;3000;20;475;76;White;Aluminium - Fagerhult - White;7320046849573;54544-402;31;31;400;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;2
TERSO LED D400 WHITE 4K_54545-402;3.9;4000;2370;2370;4000;4000;20;475;82;White;Aluminium - Fagerhult - White;7320046849580;54545-402;29;29;400;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;2
TERSO LED D400 BLACK 3K_54546-402;3.9;3000;2370;2370;3000;3000;20;475;76;Black;Aluminium - Fagerhult - Black;7320046849597;54546-402;31;31;400;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;2
TERSO LED D400 BLACK 4K  _54547-402;3.9;4000;2370;2370;4000;4000;20;475;82;Black;Aluminium - Fagerhult - Black;7320046849603;54547-402;29;29;400;Terso;Two point suspension c/c 55–78 mm.;A decorative suspended luminaire in different colours and two sizes for all types of conference/entertainment rooms. Fabric cord and white finish inside.;min. 80;N/A;1;2
