;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Description##OTHER##;Color Rendering Index##Other##
DTI TYPE2 3100LM 1200 WHITE 3K Standard_29470;141;3.0;3000;2900;Aluminium - Fagerhult - BetaOpti;1365;2900;3000;3000;20;58;145;White;Aluminium - Fagerhult - White;7320046221003;29470;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K Standard_29471;141;3.0;3000;4740;Aluminium - Fagerhult - BetaOpti;1365;4740;3000;3000;20;58;144;White;Aluminium - Fagerhult - White;7320046221102;29471;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K Standard_29472;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046221201;29472;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K Standard_29473;141;3.0;3000;6390;Aluminium - Fagerhult - BetaOpti;1365;6390;3000;3000;20;58;139;White;Aluminium - Fagerhult - White;7320046221362;29473;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 4K Standard_29474;141;3.0;4000;3040;Aluminium - Fagerhult - BetaOpti;1365;3040;4000;4000;20;58;152;White;Aluminium - Fagerhult - White;7320046221508;29474;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K Standard_29475;141;3.0;4000;4990;Aluminium - Fagerhult - BetaOpti;1365;4990;4000;4000;20;58;151;White;Aluminium - Fagerhult - White;7320046221607;29475;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K Standard_29476;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046221706;29476;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K Standard_29477;141;3.0;4000;6730;Aluminium - Fagerhult - BetaOpti;1365;6730;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046221867;29477;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 3100LM 1200 WHITE 3K Standard_29480;141;3.0;3000;2890;Aluminium - Fagerhult - BetaOpti;1365;2890;3000;3000;20;58;145;White;Aluminium - Fagerhult - White;7320046222000;29480;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 4800LM 1200 WHITE 3K Standard_29481;141;3.0;3000;4740;Aluminium - Fagerhult - BetaOpti;1365;4740;3000;3000;20;58;144;White;Aluminium - Fagerhult - White;7320046222048;29481;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 5600LM 1200 WHITE 3K Standard_29482;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046222086;29482;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 6500LM 1200 WHITE 3K Standard_29483;141;3.0;3000;6390;Aluminium - Fagerhult - BetaOpti;1365;6390;3000;3000;20;58;139;White;Aluminium - Fagerhult - White;7320046222123;29483;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 3100LM 1200 WHITE 4K Standard_29484;141;3.0;4000;3040;Aluminium - Fagerhult - BetaOpti;1365;3040;4000;4000;20;58;152;White;Aluminium - Fagerhult - White;7320046222161;29484;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 4800LM 1200 WHITE 4K Standard_29485;141;3.0;4000;4990;Aluminium - Fagerhult - BetaOpti;1365;4990;4000;4000;20;58;151;White;Aluminium - Fagerhult - White;7320046222208;29485;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 5600LM 1200 WHITE 4K Standard_29486;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046222246;29486;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 6500LM 1200 WHITE 4K Standard_29487;141;3.0;4000;6730;Aluminium - Fagerhult - BetaOpti;1365;6730;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046222284;29487;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K PLUS Standard_29490;141;3.0;3000;4740;Aluminium - Fagerhult - BetaOpti;1365;4740;3000;3000;20;58;144;White;Aluminium - Fagerhult - White;7320046220686;29490;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS Standard_29491;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046220761;29491;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K PLUS Standard_29492;141;3.0;4000;4990;Aluminium - Fagerhult - BetaOpti;1365;4990;4000;4000;20;58;151;White;Aluminium - Fagerhult - White;7320046220846;29492;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS Standard_29493;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046220921;29493;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1500 WHITE 4K Standard_29668;141;3.2;4000;6020;Aluminium - Fagerhult - BetaOpti;1665;6020;4000;4000;20;58;151;White;Aluminium - Fagerhult - White;7320046415761;29668;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6000LM 1500 WHITE 3K Standard_29670;141;3.2;3000;5720;Aluminium - Fagerhult - BetaOpti;1665;5720;3000;3000;20;58;143;White;Aluminium - Fagerhult - White;7320046600433;29670;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7500LM 1500 WHITE 3K Standard_29671;141;3.2;3000;7350;Aluminium - Fagerhult - BetaOpti;1665;7350;3000;3000;20;58;141;White;Aluminium - Fagerhult - White;7320046600839;29671;52;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7500LM 1500 WHITE 4K Standard_29672;141;3.2;4000;7730;Aluminium - Fagerhult - BetaOpti;1665;7730;4000;4000;20;58;149;White;Aluminium - Fagerhult - White;7320046600891;29672;52;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 3K StandardOnePullCord_29470-16;141;3.0;3000;2900;Aluminium - Fagerhult - BetaOpti;1365;2900;3000;3000;20;58;145;White;Aluminium - Fagerhult - White;7320046221027;29470-16;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 3K DALIPhasePulseControl_29470-402;141;3;3000;2890;Aluminium - Fagerhult - BetaOpti;1365;2890;3000;3000;20;82;145;White;Aluminium - Fagerhult - White;7320046221041;29470-402;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 3K eSenseActiLumeWithSingleLuminaire1pullDimcord_29470-448;141;3;3000;2890;Aluminium - Fagerhult - BetaOpti;1365;2890;3000;3000;20;82;145;White;Aluminium - Fagerhult - White;7320046221065;29470-448;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 3K PhasepulseControlOnePullDimCord_29470-449;141;3;3000;2890;Aluminium - Fagerhult - BetaOpti;1365;2890;3000;3000;20;82;145;White;Aluminium - Fagerhult - White;7320046221089;29470-449;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 3K eSenseSmartSWITCHonOff_29470-515;141;3.0;3000;2900;Aluminium - Fagerhult - BetaOpti;1365;2900;3000;3000;20;58;145;White;Aluminium - Fagerhult - White;7320046688868;29470-515;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 3K ESenseActive_29470-538;141;3.2;3000;2890;Aluminium - Fagerhult - BetaOpti;1365;2890;3000;3000;20;82;144;White;Aluminium - Fagerhult - White;7320047651991;29470-538;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K StandardOnePullCord_29471-16;141;3.0;3000;4740;Aluminium - Fagerhult - BetaOpti;1365;4740;3000;3000;20;58;144;White;Aluminium - Fagerhult - White;7320046221140;29471-16;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K DALIPhasePulseControl_29471-402;141;3.0;3000;4740;Aluminium - Fagerhult - BetaOpti;1365;4740;3000;3000;20;58;144;White;Aluminium - Fagerhult - White;7320046221164;29471-402;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K eSenseActiLumeWithSingleLuminaire1pullDimcord_29471-448;141;3;3000;4742;Aluminium - Fagerhult - BetaOpti;1365;4742;3000;3000;20;82;144;White;Aluminium - Fagerhult - White;7320046221164;29471-448;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K PhasepulseControlOnePullDimCord_29471-449;141;3;3000;4742;Aluminium - Fagerhult - BetaOpti;1365;4742;3000;3000;20;82;144;White;Aluminium - Fagerhult - White;7320046221188;29471-449;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K eSenseSmartSWITCHonOff_29471-515;141;3.0;3000;4740;Aluminium - Fagerhult - BetaOpti;1365;4740;3000;3000;20;58;144;White;Aluminium - Fagerhult - White;7320046688882;29471-515;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K StandardOnePullCord_29472-16;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046221225;29472-16;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K DALIPhasePulseControl_29472-402;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046221249;29472-402;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K eSenseActiLumeWithSingleLuminaire1pullDimcord_29472-448;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046221263;29472-448;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PhasepulseControlOnePullDimCord_29472-449;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046221287;29472-449;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K eSenseConnectWithSensor_29472-457;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046221300;29472-457;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K eSenseConnect_29472-458;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046221324;29472-458;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K eSenseActiLumeMasterLuminaire_29472-459;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046221348;29472-459;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K ESenseOrganic_29472-492;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320047211249;29472-492;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K eSenseSmartSWITCHonOff_29472-515;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046688899;29472-515;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K ESenseOrganic_29472-533;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320047806292;29472-533;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K ESenseActiveMaster_29472-537;141;3.2;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320047652219;29472-537;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K ESenseActive_29472-538;141;3.2;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320047652189;29472-538;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K DALIPhasePulseControl_29473-402;141;3;3000;6391;Aluminium - Fagerhult - BetaOpti;1365;6391;3000;3000;20;82;139;White;Aluminium - Fagerhult - White;7320046221386;29473-402;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K eSenseActiLumeWithSingleLuminaire1pullDimcord_29473-448;141;3;3000;6391;Aluminium - Fagerhult - BetaOpti;1365;6391;3000;3000;20;82;139;White;Aluminium - Fagerhult - White;7320046221409;29473-448;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K PhasepulseControlOnePullDimCord_29473-449;141;3;3000;6391;Aluminium - Fagerhult - BetaOpti;1365;6391;3000;3000;20;82;139;White;Aluminium - Fagerhult - White;7320046221423;29473-449;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K eSenseConnectWithSensor_29473-457;141;3;3000;6391;Aluminium - Fagerhult - BetaOpti;1365;6391;3000;3000;20;82;139;White;Aluminium - Fagerhult - White;7320046221447;29473-457;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K eSenseConnect_29473-458;141;3;3000;6391;Aluminium - Fagerhult - BetaOpti;1365;6391;3000;3000;20;82;139;White;Aluminium - Fagerhult - White;7320046221461;29473-458;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K eSenseActiLumeMasterLuminaire_29473-459;141;3;3000;6391;Aluminium - Fagerhult - BetaOpti;1365;6391;3000;3000;20;82;139;White;Aluminium - Fagerhult - White;7320046221485;29473-459;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K PhasePulse_29473-474;141;3.0;3000;6390;Aluminium - Fagerhult - BetaOpti;1365;6390;3000;3000;20;58;139;White;Aluminium - Fagerhult - White;7320046534639;29473-474;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K ESenseOrganic_29473-492;141;3.0;3000;6390;Aluminium - Fagerhult - BetaOpti;1365;6390;3000;3000;20;58;139;White;Aluminium - Fagerhult - White;7320047213557;29473-492;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K eSenseSmartSWITCHonOff_29473-515;141;3.0;3000;6390;Aluminium - Fagerhult - BetaOpti;1365;6390;3000;3000;20;58;139;White;Aluminium - Fagerhult - White;7320046688912;29473-515;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K ESenseOrganic_29473-533;141;3.0;3000;6390;Aluminium - Fagerhult - BetaOpti;1365;6390;3000;3000;20;58;139;White;Aluminium - Fagerhult - White;7320047806315;29473-533;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 3K ESenseActiveMaster_29473-537;141;3.0;3000;6390;Aluminium - Fagerhult - BetaOpti;1365;6390;3000;3000;;58;139;White;Aluminium - Fagerhult - White;7320047652257;29473-537;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 4K StandardOnePullCord_29474-16;141;3.0;4000;3040;Aluminium - Fagerhult - BetaOpti;1365;3040;4000;4000;20;58;152;White;Aluminium - Fagerhult - White;7320046221522;29474-16;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 4K DALIPhasePulseControl_29474-402;141;3;4000;3042;Aluminium - Fagerhult - BetaOpti;1365;3042;4000;4000;20;82;152;White;Aluminium - Fagerhult - White;7320046221546;29474-402;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 4K eSenseActiLumeWithSingleLuminaire1pullDimcord_29474-448;141;3;4000;3042;Aluminium - Fagerhult - BetaOpti;1365;3042;4000;4000;20;82;152;White;Aluminium - Fagerhult - White;7320046221560;29474-448;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 4K PhasepulseControlOnePullDimCord_29474-449;141;3;4000;3042;Aluminium - Fagerhult - BetaOpti;1365;3042;4000;4000;20;82;152;White;Aluminium - Fagerhult - White;7320046221584;29474-449;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 3100LM 1200 WHITE 4K eSenseSmartSWITCHonOff_29474-515;141;3.0;4000;3040;Aluminium - Fagerhult - BetaOpti;1365;3040;4000;4000;20;58;152;White;Aluminium - Fagerhult - White;7320046688929;29474-515;20;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K StandardOnePullCord_29475-16;141;3.0;4000;4800;Aluminium - Fagerhult - BetaOpti;1365;4800;4000;4000;20;58;137;White;Aluminium - Fagerhult - White;7320046221621;29475-16;36;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K DALIPhasePulseControl_29475-402;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320046221645;29475-402;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K eSenseActiLumeWithSingleLuminaire1pullDimcord_29475-448;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320046221669;29475-448;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K PhasepulseControlOnePullDimCord_29475-449;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320046221683;29475-449;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K eSenseSmartSWITCHonOff_29475-515;141;3.0;4000;4800;Aluminium - Fagerhult - BetaOpti;1365;4800;4000;4000;20;58;137;White;Aluminium - Fagerhult - White;7320046688943;29475-515;36;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K ESenseActive_29475-538;141;3.2;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320047652011;29475-538;35;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K StandardOnePullCord_29476-16;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046221720;29476-16;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K DALIPhasePulseControl_29476-402;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221744;29476-402;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K eSenseActiLumeWithSingleLuminaire1pullDimcord_29476-448;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221768;29476-448;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PhasepulseControlOnePullDimCord_29476-449;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221782;29476-449;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K eSenseConnectWithSensor_29476-457;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221805;29476-457;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K eSenseConnect_29476-458;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221829;29476-458;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K eSenseActiLumeMasterLuminaire_29476-459;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221843;29476-459;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K ESenseOrganic_29476-492;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320047213519;29476-492;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K eSenseSmartSWITCHonOff_29476-515;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046688967;29476-515;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K ESenseOrganic_29476-533;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320047806308;29476-533;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K ESenseActiveMaster_29476-537;141;3.2;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320047652233;29476-537;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K DALIPhasePulseControl_29477-402;141;3.0;4000;6730;Aluminium - Fagerhult - BetaOpti;1365;6730;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046221881;29477-402;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K eSenseActiLumeWithSingleLuminaire1pullDimcord_29477-448;141;3;4000;6727;Aluminium - Fagerhult - BetaOpti;1365;6727;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221904;29477-448;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K PhasepulseControlOnePullDimCord_29477-449;141;3;4000;6727;Aluminium - Fagerhult - BetaOpti;1365;6727;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221928;29477-449;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K eSenseConnectWithSensor_29477-457;141;3;4000;6727;Aluminium - Fagerhult - BetaOpti;1365;6727;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221942;29477-457;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K eSenseConnect_29477-458;141;3;4000;6727;Aluminium - Fagerhult - BetaOpti;1365;6727;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221966;29477-458;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K eSenseActiLumeMasterLuminaire_29477-459;141;3;4000;6727;Aluminium - Fagerhult - BetaOpti;1365;6727;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046221980;29477-459;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K ESenseOrganic_29477-492;141;3.0;4000;6730;Aluminium - Fagerhult - BetaOpti;1365;6730;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320047213564;29477-492;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K eSenseSmartSWITCHonOff_29477-515;141;3.0;4000;6730;Aluminium - Fagerhult - BetaOpti;1365;6730;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046688974;29477-515;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K ESenseOrganic_29477-533;141;3.0;4000;6730;Aluminium - Fagerhult - BetaOpti;1365;6730;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320047806322;29477-533;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K ESenseActiveMaster_29477-537;141;3.0;4000;6730;Aluminium - Fagerhult - BetaOpti;1365;6730;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320047652271;29477-537;46;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6400LM 1200 WHITE 4K ESenseActive_29477-538;141;3.2;4000;6727;Aluminium - Fagerhult - BetaOpti;1365;6727;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320047652134;29477-538;48;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 3100LM 1200 WHITE 3K DALIPhasePulseControl_29480-402;141;3;3000;2890;Aluminium - Fagerhult - BetaOpti;1365;2890;3000;3000;20;82;145;White;Aluminium - Fagerhult - White;7320046222024;29480-402;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 4800LM 1200 WHITE 3K DALIPhasePulseControl_29481-402;141;3;3000;4742;Aluminium - Fagerhult - BetaOpti;1365;4742;3000;3000;20;82;144;White;Aluminium - Fagerhult - White;7320046222062;29481-402;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 5600LM 1200 WHITE 3K DALIPhasePulseControl_29482-402;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046222109;29482-402;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 6500LM 1200 WHITE 3K DALIPhasePulseControl_29483-402;141;3;3000;6391;Aluminium - Fagerhult - BetaOpti;1365;6391;3000;3000;20;82;139;White;Aluminium - Fagerhult - White;7320046222147;29483-402;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 3100LM 1200 WHITE 4K DALIPhasePulseControl_29484-402;141;3;4000;3042;Aluminium - Fagerhult - BetaOpti;1365;3042;4000;4000;20;82;152;White;Aluminium - Fagerhult - White;7320046222185;29484-402;21;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 4800LM 1200 WHITE 4K DALIPhasePulseControl_29485-402;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320046222222;29485-402;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 5600LM 1200 WHITE 4K DALIPhasePulseControl_29486-402;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046222260;29486-402;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 CONT 6500LM 1200 WHITE 4K DALIPhasePulseControl_29487-402;141;3;4000;6727;Aluminium - Fagerhult - BetaOpti;1365;6727;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046222307;29487-402;47.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K PLUS StandardOnePullCord_29490-16;141;3.0;3000;4740;Aluminium - Fagerhult - BetaOpti;1365;4740;3000;3000;20;58;144;White;Aluminium - Fagerhult - White;7320046220709;29490-16;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K PLUS eSenseActiLumeWithSingleLuminaire1pullDimcord_29490-448;141;3;3000;4742;Aluminium - Fagerhult - BetaOpti;1365;4742;3000;3000;20;82;144;White;Aluminium - Fagerhult - White;7320046220723;29490-448;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 3K PLUS PhasepulseControlOnePullDimCord_29490-449;141;3;3000;4742;Aluminium - Fagerhult - BetaOpti;1365;4742;3000;3000;20;82;144;White;Aluminium - Fagerhult - White;7320046220747;29490-449;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS StandardOnePullCord_29491-16;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046220785;29491-16;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS StandardOnePullCord_29491-402;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046285012;29491-402;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS eSenseActiLumeWithSingleLuminaire1pullDimcord_29491-448;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046220808;29491-448;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS PhasepulseControlOnePullDimCord_29491-449;141;3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320046220822;29491-449;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS PhasePulse_29491-474;141;3.0;3000;5530;Aluminium - Fagerhult - BetaOpti;1365;5530;3000;3000;20;58;138;White;Aluminium - Fagerhult - White;7320046274085;29491-474;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS ESenseBrightSWITCHOnOff_29491-535;151;3.3;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;58;135;White;Aluminium - Fagerhult - White;7320047625961;29491-535;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS ESenseActiveMaster_29491-537;141;3.2;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320047652110;29491-537;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 3K PLUS ESenseActive_29491-538;141;3.2;3000;5532;Aluminium - Fagerhult - BetaOpti;1365;5532;3000;3000;20;82;138;White;Aluminium - Fagerhult - White;7320047652103;29491-538;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K PLUS StandardOnePullCord_29492-16;141;3.0;4000;4990;Aluminium - Fagerhult - BetaOpti;1365;4990;4000;4000;20;58;151;White;Aluminium - Fagerhult - White;7320046220860;29492-16;33;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K PLUS eSenseActiLumeWithSingleLuminaire1pullDimcord_29492-448;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320046220884;29492-448;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K PLUS PhasepulseControlOnePullDimCord_29492-449;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320046220907;29492-449;34.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 4800LM 1200 WHITE 4K PLUS ESenseActive_29492-538;141;3.2;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;82;151;White;Aluminium - Fagerhult - White;7320047652004;29492-538;35;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS StandardOnePullCord_29493-16;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046220945;29493-16;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS eSenseActiLumeWithSingleLuminaire1pullDimcord_29493-448;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046220969;29493-448;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS PhasepulseControlOnePullDimCord_29493-449;141;3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320046220983;29493-449;41.5;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS PhasePulse_29493-474;141;3.0;4000;5820;Aluminium - Fagerhult - BetaOpti;1365;5820;4000;4000;20;58;146;White;Aluminium - Fagerhult - White;7320046485177;29493-474;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS ESenseBrightSWITCHOnOff_29493-535;151;3.3;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;58;142;White;Aluminium - Fagerhult - White;7320047625978;29493-535;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS ESenseActive_29493-537;141;3.0;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;58;142;White;Aluminium - Fagerhult - White;7320047652240;29493-537;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1200 WHITE 4K PLUS ESenseActive_29493-538;141;3.2;4000;5823;Aluminium - Fagerhult - BetaOpti;1365;5823;4000;4000;20;82;146;White;Aluminium - Fagerhult - White;7320047652127;29493-538;42;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS DaliPhasePulseControl_29496-402;141;3.3;3000;7237;Aluminium - Fagerhult - BetaOpti;1200;7237;3000;3000;20;82;133;White;Aluminium - Fagerhult - White;7320047377679;29496-402;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS ESenseActive_29496-448;141;3.3;3000;7237;Aluminium - Fagerhult - BetaOpti;1200;7237;3000;3000;20;82;133;White;Aluminium - Fagerhult - White;7320047377693;29496-448;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS PhasePulse_29496-474;141;3.3;3000;7237;Aluminium - Fagerhult - BetaOpti;1200;7237;3000;3000;20;82;133;White;Aluminium - Fagerhult - White;7320047377716;29496-474;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS ESenseBrightSWITCHOnOff_29496-531;141;3.3;3000;7237;Aluminium - Fagerhult - BetaOpti;1200;7237;3000;3000;20;82;133;White;Aluminium - Fagerhult - White;7320047377730;29496-531;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS ESenseActive_29496-538;141;3.3;3000;7237;Aluminium - Fagerhult - BetaOpti;1200;7237;3000;3000;20;82;133;White;Aluminium - Fagerhult - White;7320047652288;29496-538;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS DaliPhasePulseControl_29497-402;141;3.3;4000;7618;Aluminium - Fagerhult - BetaOpti;1200;7618;4000;4000;20;82;141;White;Aluminium - Fagerhult - White;7320047377754;29497-402;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS ESenseActive_29497-448;141;3.3;4000;7618;Aluminium - Fagerhult - BetaOpti;1200;7618;4000;4000;20;82;141;White;Aluminium - Fagerhult - White;7320047377778;29497-448;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS PhasePulse_29497-474;141;3.3;4000;7618;Aluminium - Fagerhult - BetaOpti;1200;7618;4000;4000;20;82;141;White;Aluminium - Fagerhult - White;7320047377792;29497-474;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS ESenseBrightSWITCHOnOff_29497-531;141;3.3;4000;7618;Aluminium - Fagerhult - BetaOpti;1200;7618;4000;4000;20;82;141;White;Aluminium - Fagerhult - White;7320047377815;29497-531;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS ESenseActive_29497-538;141;3.3;4000;7618;Aluminium - Fagerhult - BetaOpti;1200;7618;4000;4000;20;82;141;White;Aluminium - Fagerhult - White;7320047652295;29497-538;56;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1500 WHITE 4K DALIPhasePulseControl_29668-402;141;3.2;4000;6020;Aluminium - Fagerhult - BetaOpti;1665;6020;4000;4000;20;58;151;White;Aluminium - Fagerhult - White;7320046600822;29668-402;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 5600LM 1500 WHITE 4K PhasepulseControlOnePullDimCord_29668-449;141;3.2;4000;6020;Aluminium - Fagerhult - BetaOpti;1665;6020;4000;4000;20;58;151;White;Aluminium - Fagerhult - White;7320046415792;29668-449;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6000LM 1500 WHITE 3K DALIPhasePulseControl_29670-402;141;3.2;3000;5720;Aluminium - Fagerhult - BetaOpti;1665;5720;3000;3000;20;58;143;White;Aluminium - Fagerhult - White;7320046600457;29670-402;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 6000LM 1500 WHITE 3K PhasepulseControlOnePullDimCord_29670-449;141;3.2;3000;5720;Aluminium - Fagerhult - BetaOpti;1665;5720;3000;3000;20;58;143;White;Aluminium - Fagerhult - White;7320046600815;29670-449;40;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7500LM 1500 WHITE 3K DALIPhasePulseControl_29671-402;141;3.2;3000;7350;Aluminium - Fagerhult - BetaOpti;1665;7350;3000;3000;20;58;141;White;Aluminium - Fagerhult - White;7320046600877;29671-402;52;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
DTI TYPE2 7500LM 1500 WHITE 4K DALIPhasePulseControl_29672-402;141;3.2;4000;7730;Aluminium - Fagerhult - BetaOpti;1665;7730;4000;4000;20;58;149;White;Aluminium - Fagerhult - White;7320046600907;29672-402;52;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.   ;min. 80
