;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Description##OTHER##;Color Rendering Index##Other##;Luminaire type##OTHER##;Louvre type##OTHER##;Light distribution##OTHER##
NOTOR36 PEND D 1200 DALI HL 840_16085-20015;36;1.7;4000;2800;Acrylic - Fagerhult - Opal;1249;2800;4000;4000;20;36;117;White;Aluminium - Fagerhult - White;7320048598516;16085-20015;25.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;3;0
NOTOR36 PEND D 2400 DALI HL 840_16085-20016;36;2.9;4000;5600;Acrylic - Fagerhult - Opal;2488;5600;4000;4000;20;36;122;White;Aluminium - Fagerhult - White;7320048598547;16085-20016;47.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;3;0
NOTOR36 PEND D 1200 DALI LL 840_16085-20021;36;1.9;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1255;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048598691;16085-20021;14.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;1;0
NOTOR36 PEND D 2400 DALI LL 840_16085-20022;36;3.2;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2507;3500;4000;4000;20;36;132;White;Aluminium - Fagerhult - White;7320048598721;16085-20022;28.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;2;0
NOTOR36 PEND D 1200 DALI HL 840_16085-20023;36;1.9;4000;2800;Aluminium - Fagerhult - Beta Opti Nano;1255;2800;4000;4000;20;36;135;White;Aluminium - Fagerhult - White;7320048598752;16085-20023;22.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;1;0
NOTOR36 PEND D 2400 DALI HL 840_16085-20024;36;3.2;4000;5600;Aluminium - Fagerhult - Beta Opti Nano;2507;5600;4000;4000;20;36;134;White;Aluminium - Fagerhult - White;7320048598783;16085-20024;44;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;2;0
NOTOR36 PEND D/I 1200 DALI  840_16085-20026;36;1.7;4000;4800;Aluminium - Fagerhult - Beta Opti Nano;1255;4800;4000;4000;20;36;133;White;Aluminium - Fagerhult - White;7320048598851;16085-20026;38;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;1;1
NOTOR36 PEND D 1200 DALI LL 840_16085-20029;36;1.7;4000;1800;Acrylic - Fagerhult - Opal;1249;1800;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320048600073;16085-20029;16.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;3;0
NOTOR36 PEND D 2400 DALI LL 840_16085-20030;36;2.9;4000;3600;Acrylic - Fagerhult - Opal;2488;3600;4000;4000;20;36;119;White;Aluminium - Fagerhult - White;7320048600103;16085-20030;31.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;1;3;0
NOTOR36 PEND D 1200 DALI LL 840_16085-20065;36;1.9;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1268;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048855053;16085-20065;14.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;3;1;0
NOTOR36 PEND D 1200 DALI LL 840_16085-20074;36;1.7;4000;1800;Acrylic - Fagerhult - Opal;1260;1800;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320048855084;16085-20074;16;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;3;3;0
NOTOR36 PEND D 2400 DALI LL 840_16085-20075;36;3.2;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2520;3500;4000;4000;20;36;136;White;Aluminium - Fagerhult - White;7320048855114;16085-20075;27;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;3;2;0
NOTOR36 PEND D 2400 DALI LL 840_16085-20076;36;2.9;4000;3600;Acrylic - Fagerhult - Opal;2499;3600;4000;4000;20;36;119;White;Aluminium - Fagerhult - White;7320048855145;16085-20076;30.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;3;3;0
NOTOR36 PEND D 1200 DALI LL 840_16085-20077;36;1.9;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1254;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048855176;16085-20077;14.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;2;1;0
NOTOR36 PEND D 1200 DALI LL 840_16085-20078;36;1.7;4000;1800;Acrylic - Fagerhult - Opal;1284;1800;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320048855206;16085-20078;16;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;4;3;0
NOTOR36 PEND D 2400 DALI LL 840_16085-20079;36;2.9;4000;3600;Acrylic - Fagerhult - Opal;2523;3600;4000;4000;20;36;119;White;Aluminium - Fagerhult - White;7320048855275;16085-20079;30.5;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;4;3;0
NOTOR36 PEND D 2400 DALI LL 840_16085-20064;36;3.2;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2506;3500;4000;4000;20;36;136;White;Aluminium - Fagerhult - White;7320048855244;16085-20064;27;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 4000;2;2;0

