;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Temperature Color##COLOR_TEMPERATURE##KELVIN;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;BIM Version##OTHER##
NOTOR36 3-SPOT MODULE PEND NARROW BEAM 930_16085-20386;36;1;1548;603;3000;20;107;85;White;Aluminium - Fagerhult - White;7320049980600;16085-20386;18;Notor 36 Spot module;Individual or system installation by means of wire suspension. Can also be wall mounted using the wall bracket. Wire brackets and friction locks are included in the delivery. Use Configure for wire suspension and mounting options.;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 90;1
NOTOR36 3-SPOT MODULE PEND MEDIUM BEAM 930_16085-20387;36;1;1404;603;3000;20;107;77;White;Aluminium - Fagerhult - White;7320049980631;16085-20387;18;Notor 36 Spot module;Individual or system installation by means of wire suspension. Can also be wall mounted using the wall bracket. Wire brackets and friction locks are included in the delivery. Use Configure for wire suspension and mounting options.;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 90;1
NOTOR36 3-SPOT MODULE PEND MEDIUM BEAM 930_16085-20388;36;1;1404;603;3000;20;107;77;White;Aluminium - Fagerhult - White;7320049980655;16085-20388;18;Notor 36 Spot module;Individual or system installation by means of wire suspension. Can also be wall mounted using the wall bracket. Wire brackets and friction locks are included in the delivery. Use Configure for wire suspension and mounting options.;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 90;1
NOTOR36 3-SPOT MODULE PEND NARROW BEAM 930_16085-20385;36;1;1548;603;3000;20;107;85;White;Aluminium - Fagerhult - White;7320049980587;16085-20385;18;Notor 36 Spot module;Individual or system installation by means of wire suspension. Can also be wall mounted using the wall bracket. Wire brackets and friction locks are included in the delivery. Use Configure for wire suspension and mounting options.;Luminaire for pendent installation, individually or in a system. Opal or Beta Opti Nano louvre. Can also be wall mounted using the wall bracket. Available with both direct and direct/indirect light distribution.;min. 90;1
