;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Model##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Description##OTHER##;Color Rendering Index##Other##;SENSOR##OTHER##
INDIGO LED OPAL VTB 3K 1 HL_24650;596;4,9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;596;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043446843;24650;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-111;596;4.9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;596;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043446881;24650-111;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-3;596;4.9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;596;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043446867;24650-3;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-340;596;4.9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;596;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043446904;24650-340;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-402;596;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;596;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043446874;24650-402;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-454;596;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;596;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043446935;24650-454;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-456;596;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;596;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043446898;24650-456;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-492;596;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;596;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043578902;24650-492;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 1 HL_24650-533;596;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;596;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320047815225;24650-533;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;1
INDIGO LED OPAL VTB 4K 1 HL_24651;596;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;596;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043446966;24651;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 1 HL_24651-111;596;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;596;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043447017;24651-111;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 1 HL_24651-3;596;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;596;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043446973;24651-3;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 1 HL_24651-340;596;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;596;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043447109;24651-340;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 1 HL_24651-402;596;4.9;4000;Indigo LED;3448;Acrylic - Fagerhult - Opal;596;3448;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043446997;24651-402;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 1 HL_24651-454;596;4.9;4000;Indigo LED;3448;Acrylic - Fagerhult - Opal;596;3448;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447123;24651-454;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 1 HL_24651-456;596;4.9;4000;Indigo LED;3448;Acrylic - Fagerhult - Opal;596;3448;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447093;24651-456;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 1 HL_24651-533;596;4,9;4000;Indigo LED;4181;Acrylic - Fagerhult - Opal;596;4181;4000;4000;40;152;95;White;Aluminium - Fagerhult - White;7320047815232;24651-533;44;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;1
INDIGO LED OPAL HB 3K 1 HL_24652;599;4.9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;599;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043447208;24652;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 1 HL_24652-111;599;4.9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;599;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043447246;24652-111;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 1 HL_24652-3;599;4.9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;599;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043447222;24652-3;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 1 HL_24652-340;599;4.9;3000;Indigo LED;3604;Acrylic - Fagerhult - Opal;599;3604;3000;3000;20;152;92;White;Aluminium - Fagerhult - White;7320043447291;24652-340;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 1 HL_24652-402;599;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;599;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043447239;24652-402;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 1 HL_24652-454;599;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;599;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043447307;24652-454;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 1 HL_24652-456;599;4.9;3000;Indigo LED;3276;Acrylic - Fagerhult - Opal;599;3276;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043447277;24652-456;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 1 HL_24653;599;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;599;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043447369;24653;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 1 HL_24653-111;599;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;599;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043447390;24653-111;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 1 HL_24653-3;599;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;599;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043447376;24653-3;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 1 HL_24653-340;599;4.9;4000;Indigo LED;3793;Acrylic - Fagerhult - Opal;599;3793;4000;4000;20;152;97;White;Aluminium - Fagerhult - White;7320043447413;24653-340;39;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 1 HL_24653-402;599;4.9;4000;Indigo LED;3448;Acrylic - Fagerhult - Opal;599;3448;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447383;24653-402;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 1 HL_24653-454;599;4.9;4000;Indigo LED;3448;Acrylic - Fagerhult - Opal;599;3448;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447420;24653-454;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 1 HL_24653-456;599;4.9;4000;Indigo LED;3448;Acrylic - Fagerhult - Opal;599;3448;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447406;24653-456;37;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 2 LL_24654;596;4.9;3000;Indigo LED;2595;Acrylic - Fagerhult - Opal;596;2595;3000;3000;20;152;93;White;Aluminium - Fagerhult - White;7320043447444;24654;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 2 LL_24654-111;596;4.9;3000;Indigo LED;2595;Acrylic - Fagerhult - Opal;596;2595;3000;3000;20;152;93;White;Aluminium - Fagerhult - White;7320043447499;24654-111;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 2 LL_24654-3;596;4.9;3000;Indigo LED;2595;Acrylic - Fagerhult - Opal;596;2595;3000;3000;20;152;93;White;Aluminium - Fagerhult - White;7320043447475;24654-3;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 2 LL_24654-340;596;4.9;3000;Indigo LED;2595;Acrylic - Fagerhult - Opal;596;2595;3000;3000;20;152;93;White;Aluminium - Fagerhult - White;7320043447512;24654-340;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 2 LL_24654-402;596;4.9;3000;Indigo LED;2359;Acrylic - Fagerhult - Opal;596;2359;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043447482;24654-402;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 2 LL_24654-454;596;4.9;3000;Indigo LED;2359;Acrylic - Fagerhult - Opal;596;2359;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043447529;24654-454;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 3K 2 LL_24654-456;596;4.9;3000;Indigo LED;2359;Acrylic - Fagerhult - Opal;596;2359;3000;3000;20;152;94;White;Aluminium - Fagerhult - White;7320043447505;24654-456;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 2 LL_24655;596;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;596;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447536;24655;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 2 LL_24655-111;596;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;596;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447574;24655-111;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 2 LL_24655-3;596;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;596;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447550;24655-3;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 2 LL_24655-340;596;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;596;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447598;24655-340;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 2 LL_24655-402;596;4.9;4000;Indigo LED;2483;Acrylic - Fagerhult - Opal;596;2483;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447567;24655-402;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 2 LL_24655-454;596;4.9;4000;Indigo LED;2483;Acrylic - Fagerhult - Opal;596;2483;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447604;24655-454;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL VTB 4K 2 LL_24655-456;596;4.9;4000;Indigo LED;2483;Acrylic - Fagerhult - Opal;596;2483;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447581;24655-456;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 2 LL_24656;599;4,9;3000;Indigo LED;2750;Acrylic - Fagerhult - Opal;599;2750;3000;3000;40;152;98;White;Aluminium - Fagerhult - White;7320043447611;24656;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 2 LL_24656-111;599;4,9;3000;Indigo LED;2750;Acrylic - Fagerhult - Opal;599;2750;3000;3000;40;152;98;White;Aluminium - Fagerhult - White;7320043447642;24656-111;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 2 LL_24656-3;599;4,9;3000;Indigo LED;2750;Acrylic - Fagerhult - Opal;599;2750;3000;3000;40;152;98;White;Aluminium - Fagerhult - White;7320043447628;24656-3;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 2 LL_24656-340;599;4,9;3000;Indigo LED;2750;Acrylic - Fagerhult - Opal;599;2750;3000;3000;40;152;98;White;Aluminium - Fagerhult - White;7320043447666;24656-340;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 2 LL_24656-402;599;4,9;3000;Indigo LED;2750;Acrylic - Fagerhult - Opal;599;2750;3000;3000;40;152;98;White;Aluminium - Fagerhult - White;7320043447635;24656-402;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 2 LL_24656-454;599;4,9;3000;Indigo LED;2750;Acrylic - Fagerhult - Opal;599;2750;3000;3000;40;152;98;White;Aluminium - Fagerhult - White;7320043447673;24656-454;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 3K 2 LL_24656-456;599;4,9;3000;Indigo LED;2750;Acrylic - Fagerhult - Opal;599;2750;3000;3000;40;152;98;White;Aluminium - Fagerhult - White;7320043447659;24656-456;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 2 LL_24657;599;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;599;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447680;24657;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 2 LL_24657-111;599;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;599;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447710;24657-111;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 2 LL_24657-3;599;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;599;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447697;24657-3;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 2 LL_24657-340;599;4.9;4000;Indigo LED;2731;Acrylic - Fagerhult - Opal;599;2731;4000;4000;20;152;98;White;Aluminium - Fagerhult - White;7320043447734;24657-340;28;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 2 LL_24657-402;599;4.9;4000;Indigo LED;2483;Acrylic - Fagerhult - Opal;599;2483;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447703;24657-402;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 2 LL_24657-454;599;4.9;4000;Indigo LED;2483;Acrylic - Fagerhult - Opal;599;2483;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447741;24657-454;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
INDIGO LED OPAL HB 4K 2 LL_24657-456;599;4.9;4000;Indigo LED;2483;Acrylic - Fagerhult - Opal;599;2483;4000;4000;20;152;99;White;Aluminium - Fagerhult - White;7320043447727;24657-456;26;A recessed luminaire for most types of suspended ceilings. Combination of direct and indirect light creates comfortable and glare-free working environments, ambient light on the wall.;min. 80;0
