;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Organic Response##OTHER##;Opening##OTHER##
MULTILUME RE:THINK 600X600 OR DELTA HL 840 VTB_24100-20022;595;2.8;4000;4388;Fagerhult_Delta_microprisma;595;4388;4000;4000;20;27;142;White;Aluminium - Fagerhult - White;7320049597761;24100-20022;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 600X600 DALI DELTA HL T/W VTB_24100-20024;595;2.7;4000;3213;Fagerhult_Delta_microprisma;595;3213;4000;4000;20;27;111;White;Aluminium - Fagerhult - White;7320049597822;24100-20024;29;29;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 90;D;1;0;1
MULTILUME RE:THINK 600X600 DALI DELTA HL 830 VTB_24100-20027;595;2.7;3000;4388;Fagerhult_Delta_microprisma;595;4388;3000;3000;20;27;146;White;Aluminium - Fagerhult - White;7320049759527;24100-20027;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 600X600 OR DELTA HL 830 VTB_24100-20028;595;2.8;3000;4388;Fagerhult_Delta_microprisma;595;4388;3000;3000;20;27;142;White;Aluminium - Fagerhult - White;7320049759589;24100-20028;29;29;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 600X600 DALI DELTA HL 840 VTB_24100-20029;595;2.7;4000;4388;Fagerhult_Delta_microprisma;595;4388;4000;4000;20;27;146;White;Aluminium - Fagerhult - White;7320049759626;24100-20029;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X600 DALI DELTA HL 830 VTB_24101-20000;295;1.7;3000;1877;Fagerhult_Delta_microprisma;595;1877;3000;3000;20;27;110;White;Aluminium - Fagerhult - White;7316911114174;24101-20000;17;17;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X600 OR DELTA HL 840 VTB_24101-20001;295;1.8;4000;1877;Fagerhult_Delta_microprisma;595;1877;4000;4000;20;27;105;White;Aluminium - Fagerhult - White;7316911114204;24101-20001;18;18;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 300X600 DALI DELTA HL 840 VTB_24101-20003;295;1.7;4000;1877;Fagerhult_Delta_microprisma;595;1877;4000;4000;20;27;110;White;Aluminium - Fagerhult - White;7316911170385;24101-20003;17;17;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X600 OR DELTA HL 830 VTB_24101-20004;295;1.8;3000;1877;Fagerhult_Delta_microprisma;595;1877;3000;3000;20;27;105;White;Aluminium - Fagerhult - White;7316911170415;24101-20004;18;18;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 300X1200 OR DELTA HL 830 VTB_24102-20001;295;3.5;3000;3802;Fagerhult_Delta_microprisma;1195;3802;3000;3000;20;27;117;White;Aluminium - Fagerhult - White;7316911114372;24102-20001;33;33;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 300X1200 DALI DELTA HL 830 VTB_24102-20003;295;3.4;3000;3802;Fagerhult_Delta_microprisma;1195;3802;3000;3000;20;27;123;White;Aluminium - Fagerhult - White;7316911170606;24102-20003;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X1200 DALI DELTA HL 840 VTB_24102-20004;295;3.4;4000;3802;Fagerhult_Delta_microprisma;1195;3802;4000;4000;20;27;123;White;Aluminium - Fagerhult - White;7316911170637;24102-20004;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X1200 OR DELTA HL 840 VTB_24102-20005;295;3.5;4000;3802;Fagerhult_Delta_microprisma;1195;3802;4000;4000;20;27;117;White;Aluminium - Fagerhult - White;7316911170668;24102-20005;33;33;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 300X1200 DALI DELTA HL T/W VTB_24102-20010;295;3.5;4000;2958;Fagerhult_Delta_microprisma;1195;2958;4000;4000;20;27;102;White;Aluminium - Fagerhult - White;7316911170835;24102-20010;29;29;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 90;D;1;0;1
MULTILUME RE:THINK 600X600 OR DELTA HL T/W VTB_24100-20122;595;2.8;4000;3213;Fagerhult_Delta_microprisma;595;3213;4000;4000;20;27;108;White;Aluminium - Fagerhult - White;7316910531279;24100-20122;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 90;D;1;1;1
MULTILUME RE:THINK 300X1200 OR DELTA HL T/W VTB_24102-20002;295;3.6;4000;2958;Fagerhult_Delta_microprisma;1195;2958;4000;4000;20;27;100;White;Aluminium - Fagerhult - White;7316911114310;24102-20002;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 90;D;1;2;1
MULTILUME RE:THINK 625X625 OR DELTA HL 840 VTB_24104-20001;620;3.2;4000;4358;Fagerhult_Delta_microprisma;620;4358;4000;4000;20;25;141;White;Aluminium - Fagerhult - White;7316911788719;24104-20001;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 625X625 DALI DELTA HL 830 VTB_24104-20004;620;3.2;3000;4358;Fagerhult_Delta_microprisma;620;4358;3000;3000;20;25;145;White;Aluminium - Fagerhult - White;7316911949882;24104-20004;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 625X625 DALI DELTA HL 840 VTB_24104-20005;620;3.2;4000;4358;Fagerhult_Delta_microprisma;620;4358;4000;4000;20;25;145;White;Aluminium - Fagerhult - White;7316911949912;24104-20005;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 625X625 OR DELTA HL 830 VTB_24104-20006;620;3.2;3000;4358;Fagerhult_Delta_microprisma;620;4358;3000;3000;20;25;141;White;Aluminium - Fagerhult - White;7316911949943;24104-20006;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 312,5X1250 OR DELTA HL 840 VTB_24106-20003;308;3.2;4000;3365;Fagerhult_Delta_microprisma;1245;3365;4000;4000;20;27;103;White;Aluminium - Fagerhult - White;7316911838049;24106-20003;33;33;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 312,5X1250 DALI DELTA HL 830 VTB_24106-20005;308;3.2;3000;3365;Fagerhult_Delta_microprisma;1245;3365;3000;3000;20;27;109;White;Aluminium - Fagerhult - White;7316911949974;24106-20005;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 312,5X1250 DALI DELTA HL 840 VTB_24106-20006;309;3.2;4000;3365;Fagerhult_Delta_microprisma;1246;3365;4000;4000;20;28;109;White;Aluminium - Fagerhult - White;7316911950000;24106-20006;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 312,5X1250 OR DELTA HL 830 VTB_24106-20007;308;3.2;3000;3365;Fagerhult_Delta_microprisma;1245;3365;3000;3000;20;27;103;White;Aluminium - Fagerhult - White;7316911950031;24106-20007;33;33;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 600X600 CIRC DALI DELTA HL 830 VTB_24103-20008;595;2.7;3000;3996;Fagerhult_Delta_microprisma;595;3996;3000;3000;20;27;133;White;Aluminium - Fagerhult - White;7316911490766;24103-20008;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;2
MULTILUME RE:THINK 600X600 CIRC DALI DELTA HL 840 VTB_24103-20013;595;2.7;4000;3996;Fagerhult_Delta_microprisma;595;3996;4000;4000;20;27;133;White;Aluminium - Fagerhult - White;7316911535177;24103-20013;30;30;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;0;2
MULTILUME RE:THINK 600X600 CIRC OR DELTA HL 830 VTB_24103-20017;595;2.8;3000;3996;Fagerhult_Delta_microprisma;595;3996;3000;3000;20;27;129;White;Aluminium - Fagerhult - White;7316911522177;24103-20017;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;2
MULTILUME RE:THINK 600X600 CIRC OR DELTA HL 840 VTB_24103-20015;595;2.8;4000;3996;Fagerhult_Delta_microprisma;595;3996;4000;4000;20;27;129;White;Aluminium - Fagerhult - White;7316911517418;24103-20015;31;31;Multilume Re:Think Delta;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Delta louvre provides efficient and optimal light comfort.;min. 80;C;1;1;2
