;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Organic Response##OTHER##;Opening##OTHER##
MULTILUME RE:THINK 600X600 DALI OPAL HL 830 VTB_24100-20030;595;2.7;3000;4508;Polystyrene - Fagerhult - Opal;595;4508;3000;3000;20;27;150;White;Aluminium - Fagerhult - White;7320049759657;24100-20030;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 600X600 DALI OPAL HL 840 VTB_24100-20031;595;2.7;4000;4508;Polystyrene - Fagerhult - Opal;595;4508;4000;4000;20;27;150;White;Aluminium - Fagerhult - White;7320049759688;24100-20031;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X600 DALI OPAL HL 830 VTB_24101-20005;295;1.4;3000;2121;Polystyrene - Fagerhult - Opal;595;2121;3000;3000;20;27;124;White;Aluminium - Fagerhult - White;7316911170446;24101-20005;17;17;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X600 DALI OPAL HL 840 VTB_24101-20006;295;1.4;4000;2121;Polystyrene - Fagerhult - Opal;595;2121;4000;4000;20;27;124;White;Aluminium - Fagerhult - White;7316911170477;24101-20006;17;17;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X600 OR OPAL HL 830 VTB_24101-20007;295;1.5;3000;2121;Polystyrene - Fagerhult - Opal;595;2121;3000;3000;20;27;118;White;Aluminium - Fagerhult - White;7316911170507;24101-20007;18;18;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 300X600 OR OPAL HL 840 VTB_24101-20008;295;1.5;4000;2121;Polystyrene - Fagerhult - Opal;595;2121;4000;4000;20;27;118;White;Aluminium - Fagerhult - White;7316911170538;24101-20008;18;18;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 300X1200 DALI OPAL HL 830 VTB_24102-20006;295;3;3000;3791;Polystyrene - Fagerhult - Opal;1195;3791;3000;3000;20;27;122;White;Aluminium - Fagerhult - White;7316911170699;24102-20006;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X1200 DALI OPAL HL 840 VTB_24102-20007;295;3;4000;3791;Polystyrene - Fagerhult - Opal;1195;3791;4000;4000;20;27;122;White;Aluminium - Fagerhult - White;7316911170736;24102-20007;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 300X1200 OR OPAL HL 830 VTB_24102-20008;295;3.1;3000;3791;Polystyrene - Fagerhult - Opal;1195;3791;3000;3000;20;27;116;White;Aluminium - Fagerhult - White;7316911170767;24102-20008;33;33;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 300X1200 OR OPAL HL 840 VTB_24102-20009;295;3.1;4000;3791;Polystyrene - Fagerhult - Opal;1195;3791;4000;4000;20;27;116;White;Aluminium - Fagerhult - White;7316911170798;24102-20009;33;33;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 300X1200 DALI OPAL HL T/W VTB_24102-20011;295;3.1;4000;2949;Polystyrene - Fagerhult - Opal;1195;2949;4000;4000;20;27;102;White;Aluminium - Fagerhult - White;7316911170866;24102-20011;29;29;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 90;D;1;0;1
MULTILUME RE:THINK 600X600 OR OPAL HL T/W VTB_24100-20177;595;2.8;4000;3294;Polystyrene - Fagerhult - Opal;595;3294;4000;4000;20;27;111;White;Aluminium - Fagerhult - White;7316911425751;24100-20177;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 90;D;1;1;1
MULTILUME RE:THINK 625X625 DALI OPAL HL 830 VTB_24104-20007;620;3;3000;4531;Polystyrene - Fagerhult - Opal;620;4531;3000;3000;20;25;151;White;Aluminium - Fagerhult - White;7316911950147;24104-20007;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 625X625 DALI OPAL HL 840 VTB_24104-20008;620;3;4000;4531;Polystyrene - Fagerhult - Opal;620;4531;4000;4000;20;25;151;White;Aluminium - Fagerhult - White;7316911950185;24104-20008;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 625X625 OR OPAL HL 830 VTB_24104-20009;620;3;3000;4531;Polystyrene - Fagerhult - Opal;620;4531;3000;3000;20;25;146;White;Aluminium - Fagerhult - White;7316911950215;24104-20009;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 625X625 OR OPAL HL 840 VTB_24104-20010;620;3;4000;4531;Polystyrene - Fagerhult - Opal;620;4531;4000;4000;20;25;146;White;Aluminium - Fagerhult - White;7316911950253;24104-20010;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1;1
MULTILUME RE:THINK 312,5X1250 DALI OPAL HL 830 VTB_24106-20008;308;3.3;3000;3296;Polystyrene - Fagerhult - Opal;1245;3296;3000;3000;20;27;106;White;Aluminium - Fagerhult - White;7316911950284;24106-20008;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 312,5X1250 OR OPAL HL 840 VTB_24106-20002;308;3.4;4000;3296;Polystyrene - Fagerhult - Opal;1245;3296;4000;4000;20;27;101;White;Aluminium - Fagerhult - White;7316911788979;24106-20002;33;33;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 312,5X1250 DALI OPAL HL 840 VTB_24106-20009;308;3.3;4000;3296;Polystyrene - Fagerhult - Opal;1245;3296;4000;4000;20;27;106;White;Aluminium - Fagerhult - White;7316911950314;24106-20009;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;1
MULTILUME RE:THINK 312,5X1250 OR OPAL HL 830 VTB_24106-20010;308;3.4;3000;3296;Polystyrene - Fagerhult - Opal;1245;3296;3000;3000;20;27;101;White;Aluminium - Fagerhult - White;7316911950345;24106-20010;33;33;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;2;1
MULTILUME RE:THINK 600X600 CIRC DALI OPAL HL 830 VTB_24103-20002;595;2.7;3000;4058;Polystyrene - Fagerhult - Opal;595;4058;3000;3000;20;27;135;White;Aluminium - Fagerhult - White;7316911445513;24103-20002;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;2
MULTILUME RE:THINK 600X600 CIRC DALI OPAL HL 840 VTB_24103-20012;595;2.7;4000;4058;Polystyrene - Fagerhult - Opal;595;4058;4000;4000;20;27;135;White;Aluminium - Fagerhult - White;7316911506702;24103-20012;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0;2
MULTILUME RE:THINK 600X600 CIRC OR OPAL HL 830 VTB_24103-20001;595;2.8;3000;4058;Polystyrene - Fagerhult - Opal;595;4058;3000;3000;20;27;131;White;Aluminium - Fagerhult - White;7316911445537;24103-20001;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1;2
MULTILUME RE:THINK 600X600 CIRC OR OPAL HL 840 VTB_24103-20022;595;2.8;4000;4058;Polystyrene - Fagerhult - Opal;595;4058;4000;4000;20;27;131;White;Aluminium - Fagerhult - White;7316912111639;24103-20022;31;31;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB 24 mm. Unventilated or ventilated building elements.;A recessed general luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1;2
