;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Organic Response##OTHER##
MULTILUME RE:THINK 600X600 DALI OPAL HL 830 VTB_24100-20030;595;2.7;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;20;27;146;White;Paper - Fagerhult - White;7320049759657;24100-20030;32.5;32.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 600X600 DALI OPAL HL 840 VTB_24100-20031;595;2.7;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;20;27;154;White;Paper - Fagerhult - White;7320049759688;24100-20031;32.5;32.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X600 DALI OPAL HL 830 VTB_24101-20005;295;1.4;3000;2121;Polystyrene - Fagerhult - Opal;595;2121;3000;3000;20;27;124;White;Paper - Fagerhult - White;7316911170446;24101-20005;18.5;18.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X600 DALI OPAL HL 840 VTB_24101-20006;295;1.4;4000;2121;Polystyrene - Fagerhult - Opal;595;2121;4000;4000;20;27;124;White;Paper - Fagerhult - White;7316911170477;24101-20006;18.5;18.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X600 OR OPAL HL 830 VTB_24101-20007;295;1.5;3000;2121;Polystyrene - Fagerhult - Opal;595;2121;3000;3000;20;27;118;White;Paper - Fagerhult - White;7316911170507;24101-20007;19.5;19.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1
MULTILUME RE:THINK 300X600 OR OPAL HL 840 VTB_24101-20008;295;1.5;4000;2121;Polystyrene - Fagerhult - Opal;595;2121;4000;4000;20;27;118;White;Paper - Fagerhult - White;7316911170538;24101-20008;19.5;19.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;1
MULTILUME RE:THINK 300X1200 DALI OPAL HL 830 VTB_24102-20006;295;3;3000;4253;Polystyrene - Fagerhult - Opal;1195;4253;3000;3000;20;27;139;White;Paper - Fagerhult - White;7316911170699;24102-20006;33.5;33.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X1200 DALI OPAL HL 840 VTB_24102-20007;295;3;4000;4253;Polystyrene - Fagerhult - Opal;1195;4253;4000;4000;20;27;139;White;Paper - Fagerhult - White;7316911170736;24102-20007;33.5;33.5;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;0
MULTILUME RE:THINK 300X1200 OR OPAL HL 830 VTB_24102-20008;295;3.1;3000;4253;Polystyrene - Fagerhult - Opal;1195;4253;3000;3000;20;27;135;White;Paper - Fagerhult - White;7316911170767;24102-20008;34;34;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;2
MULTILUME RE:THINK 300X1200 OR OPAL HL 840 VTB_24102-20009;295;3.1;4000;4253;Polystyrene - Fagerhult - Opal;1195;4253;4000;4000;20;27;135;White;Paper - Fagerhult - White;7316911170798;24102-20009;34;34;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 80;C;1;2
MULTILUME RE:THINK 300X1200 DALI OPAL HL T/W VTB_24102-20011;295;3.1;4000;3124;Polystyrene - Fagerhult - Opal;1195;3124;4000;4000;20;27;93;White;Paper - Fagerhult - White;7316911170866;24102-20011;30;30;Multilume Re:Think Opal;Recessed in suspended ceilings with visible T-bars, VTB (15 or 24 mm). Unventilated or ventilated building elements.;A recessed workplace luminaire with a strong focus on sustainability. Body in Solid Board. Installation in ceiling with visible T-bars – VTB. Opal louvre provides efficient and optimal light comfort.;min. 90;D;1;0

