;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Sensor##OTHER##
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199;599;4;3000;3919;Polystyrene - Fagerhult - Opal;599;3919;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046711535;23199;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-3;599;4;3000;3919;Polystyrene - Fagerhult - Opal;599;3919;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046711559;23199-3;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-111;599;4;3000;3919;Polystyrene - Fagerhult - Opal;599;3919;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260858;23199-111;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-340;599;4;3000;3919;Polystyrene - Fagerhult - Opal;599;3919;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260896;23199-340;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-402;599;4;3000;3553;Polystyrene - Fagerhult - Opal;599;3553;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046711573;23199-402;27;27;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-519;599;4;3000;3919;Polystyrene - Fagerhult - Opal;599;3919;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260933;23199-519;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-520;599;4;3000;3553;Polystyrene - Fagerhult - Opal;599;3553;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260957;23199-520;25;25;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-528;599;4;3000;3553;Polystyrene - Fagerhult - Opal;599;3553;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260872;23199-528;25;25;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 830 HB WHITE_23199-529;599;4;3000;3553;Polystyrene - Fagerhult - Opal;599;3553;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260919;23199-529;25;25;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200;599;4;4000;4129;Polystyrene - Fagerhult - Opal;599;4129;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320046711597;23200;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-3;599;4;4000;4129;Polystyrene - Fagerhult - Opal;599;4129;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320046711610;23200-3;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-111;599;4;4000;4129;Polystyrene - Fagerhult - Opal;599;4129;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047260971;23200-111;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-340;599;4;4000;4129;Polystyrene - Fagerhult - Opal;599;4129;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047261015;23200-340;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-402;599;4;4000;3788;Polystyrene - Fagerhult - Opal;599;3788;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320046711634;23200-402;27;27;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-519;599;4;4000;4129;Polystyrene - Fagerhult - Opal;599;4129;4000;4000;44;23;142;White;Steel - Fagerhult - White;7320047261053;23200-519;28;28;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-520;599;4;4000;3788;Polystyrene - Fagerhult - Opal;599;3788;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047261077;23200-520;25;25;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-528;599;4;4000;3788;Polystyrene - Fagerhult - Opal;599;3788;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047260995;23200-528;25;25;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 840 HB WHITE_23200-529;599;4;4000;3788;Polystyrene - Fagerhult - Opal;599;3788;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047261039;23200-529;25;25;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207;599;4;3000;3718;Polystyrene - Fagerhult - Opal;599;3718;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320046712013;23207;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-3;599;4;3000;3718;Polystyrene - Fagerhult - Opal;599;3718;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320046712037;23207-3;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-111;599;4;3000;3718;Polystyrene - Fagerhult - Opal;599;3718;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261336;23207-111;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-340;599;4;3000;3718;Polystyrene - Fagerhult - Opal;599;3718;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261374;23207-340;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-402;599;4;3000;3421;Polystyrene - Fagerhult - Opal;599;3421;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320046712051;23207-402;35;35;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-519;599;4;3000;3718;Polystyrene - Fagerhult - Opal;599;3718;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261411;23207-519;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-520;599;4;3000;3421;Polystyrene - Fagerhult - Opal;599;3421;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261435;23207-520;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-528;599;4;3000;3421;Polystyrene - Fagerhult - Opal;599;3421;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261350;23207-528;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 930 HB WHITE_23207-529;599;4;3000;3421;Polystyrene - Fagerhult - Opal;599;3421;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261398;23207-529;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208;599;4;4000;3959;Polystyrene - Fagerhult - Opal;599;3959;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320046712075;23208;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-3;599;4;4000;3959;Polystyrene - Fagerhult - Opal;599;3959;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320046712099;23208-3;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-111;599;4;4000;3959;Polystyrene - Fagerhult - Opal;599;3959;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320047261459;23208-111;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-340;599;4;4000;3959;Polystyrene - Fagerhult - Opal;599;3959;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320047261497;23208-340;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-402;599;4;4000;3642;Polystyrene - Fagerhult - Opal;599;3642;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320046712112;23208-402;35;35;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-519;599;4;4000;3949;Polystyrene - Fagerhult - Opal;599;3949;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320047261534;23208-519;31;31;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-520;599;4;4000;3642;Polystyrene - Fagerhult - Opal;599;3642;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320047261558;23208-520;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-528;599;4;4000;3642;Polystyrene - Fagerhult - Opal;599;3642;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320047261473;23208-528;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 HL 940 HB WHITE_23208-529;599;4;4000;3642;Polystyrene - Fagerhult - Opal;599;3642;4000;4000;44;23;127;White;Steel - Fagerhult - White;7320047261510;23208-529;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;118;White;Steel - Fagerhult - White;7320047264764;23217;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-3;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;118;White;Steel - Fagerhult - White;7320047264832;23217-3;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-111;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;118;White;Steel - Fagerhult - White;7320047265013;23217-111;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-340;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;118;White;Steel - Fagerhult - White;7320047265037;23217-340;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-402;595;4;3000;3503;Polystyrene - Fagerhult - Opal;595;3503;3000;3000;44;23;122;White;Steel - Fagerhult - White;7320047264849;23217-402;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-519;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;118;White;Steel - Fagerhult - White;7320047265051;23217-519;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-520;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;122;White;Steel - Fagerhult - White;7320047265068;23217-520;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-528;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;122;White;Steel - Fagerhult - White;7320047265020;23217-528;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 930 WHITE_23217-529;595;4;3000;3583;Polystyrene - Fagerhult - Opal;595;3583;3000;3000;44;23;122;White;Steel - Fagerhult - White;7320047265044;23217-529;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218;595;4;4000;3816;Polystyrene - Fagerhult - Opal;595;3816;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047265075;23218;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-3;595;4;4000;3816;Polystyrene - Fagerhult - Opal;595;3816;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047265082;23218-3;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-111;595;4;4000;3816;Polystyrene - Fagerhult - Opal;595;3816;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047265105;23218-111;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-340;595;4;4000;3816;Polystyrene - Fagerhult - Opal;595;3816;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047265129;23218-340;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-402;595;4;4000;3731;Polystyrene - Fagerhult - Opal;595;3731;4000;4000;44;23;130;White;Steel - Fagerhult - White;7320047265099;23218-402;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-519;595;4;4000;3816;Polystyrene - Fagerhult - Opal;595;3816;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047265143;23218-519;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-520;595;4;4000;3731;Polystyrene - Fagerhult - Opal;595;3731;4000;4000;44;23;130;White;Steel - Fagerhult - White;7320047265167;23218-520;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-528;595;4;4000;3731;Polystyrene - Fagerhult - Opal;595;3731;4000;4000;44;23;130;White;Steel - Fagerhult - White;7320047265112;23218-528;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL 600X600 VTB 940 WHITE_23218-529;595;4;4000;3731;Polystyrene - Fagerhult - Opal;595;3731;4000;4000;44;23;130;White;Steel - Fagerhult - White;7320047265136;23218-529;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404;599;4;3000;2624;Polystyrene - Fagerhult - Opal;599;2624;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320046596965;23404;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-3;599;4;3000;2624;Polystyrene - Fagerhult - Opal;599;2624;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320046711139;23404-3;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-111;599;4;3000;2624;Polystyrene - Fagerhult - Opal;599;2624;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261817;23404-111;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-340;599;4;3000;2624;Polystyrene - Fagerhult - Opal;599;2624;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261855;23404-340;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-402;599;4;3000;2445;Polystyrene - Fagerhult - Opal;599;2445;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320046711153;23404-402;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-519;599;4;3000;2624;Polystyrene - Fagerhult - Opal;599;2624;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261893;23404-519;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-520;599;4;3000;2445;Polystyrene - Fagerhult - Opal;599;2445;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261916;23404-520;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-528;599;4;3000;2445;Polystyrene - Fagerhult - Opal;599;2445;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261831;23404-528;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 930 HB WHITE_23404-529;599;4;3000;2445;Polystyrene - Fagerhult - Opal;599;2445;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047261879;23404-529;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405;599;4;4000;2795;Polystyrene - Fagerhult - Opal;599;2795;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320046596972;23405;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-3;599;4;4000;2795;Polystyrene - Fagerhult - Opal;599;2795;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320046711177;23405-3;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-111;599;4;4000;2795;Polystyrene - Fagerhult - Opal;599;2795;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047261930;23405-111;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-340;599;4;4000;2795;Polystyrene - Fagerhult - Opal;599;2795;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047261978;23405-340;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-402;599;4;4000;2603;Polystyrene - Fagerhult - Opal;599;2603;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320046711191;23405-402;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-519;599;4;4000;2795;Polystyrene - Fagerhult - Opal;599;2795;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047262012;23405-519;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-520;599;4;4000;2603;Polystyrene - Fagerhult - Opal;599;2603;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047262036;23405-520;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-528;599;4;4000;2603;Polystyrene - Fagerhult - Opal;599;2603;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047261954;23405-528;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 940 HB WHITE_23405-529;599;4;4000;2603;Polystyrene - Fagerhult - Opal;599;2603;4000;4000;44;23;126;White;Steel - Fagerhult - White;7320047261992;23405-529;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491;599;4;3000;2874;Polystyrene - Fagerhult - Opal;599;2874;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046596859;23491;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-3;599;4;3000;2874;Polystyrene - Fagerhult - Opal;599;2874;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046710811;23491-3;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-111;599;4;3000;2874;Polystyrene - Fagerhult - Opal;599;2874;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047262296;23491-111;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-340;599;4;3000;2874;Polystyrene - Fagerhult - Opal;599;2874;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047262333;23491-340;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-402;599;4;3000;2586;Polystyrene - Fagerhult - Opal;599;2586;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320046710835;23491-402;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-519;599;4;3000;2874;Polystyrene - Fagerhult - Opal;599;2874;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047262371;23491-519;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-520;599;4;3000;2586;Polystyrene - Fagerhult - Opal;599;2586;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320047262395;23491-520;18;18;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-528;599;4;3000;2586;Polystyrene - Fagerhult - Opal;599;2586;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320047262319;23491-528;18;18;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 830 HB WHITE_23491-529;599;4;3000;2586;Polystyrene - Fagerhult - Opal;599;2586;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320047262357;23491-529;18;18;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492;599;4;4000;3028;Polystyrene - Fagerhult - Opal;599;3028;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320046596866;23492;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-3;599;4;4000;3028;Polystyrene - Fagerhult - Opal;599;3028;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320046710859;23492-3;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-111;599;4;4000;3028;Polystyrene - Fagerhult - Opal;599;3028;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047262418;23492-111;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-340;599;4;4000;3028;Polystyrene - Fagerhult - Opal;599;3028;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047262456;23492-340;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-402;599;4;4000;2725;Polystyrene - Fagerhult - Opal;599;2725;4000;4000;44;23;148;White;Steel - Fagerhult - White;7320046710873;23492-402;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-519;599;4;4000;3028;Polystyrene - Fagerhult - Opal;599;3028;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047262494;23492-519;19;19;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-520;599;4;4000;2725;Polystyrene - Fagerhult - Opal;599;2725;4000;4000;44;23;148;White;Steel - Fagerhult - White;7320047262517;23492-520;18;18;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-528;599;4;4000;3028;Polystyrene - Fagerhult - Opal;599;3028;4000;4000;44;23;148;White;Steel - Fagerhult - White;7320047262432;23492-528;18;18;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM OPAL REC 600X600 LL 840 HB WHITE_23492-529;599;4;4000;3028;Polystyrene - Fagerhult - Opal;599;3028;4000;4000;44;23;148;White;Steel - Fagerhult - White;7320047262470;23492-529;18;18;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505;595;4;3000;4282;Polystyrene - Fagerhult - Opal;595;4282;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320046213107;23505;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-3;595;4;3000;4282;Polystyrene - Fagerhult - Opal;595;4282;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320046200268;23505-3;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-111;595;4;3000;4282;Polystyrene - Fagerhult - Opal;595;4282;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320047262531;23505-111;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-340;595;4;3000;4282;Polystyrene - Fagerhult - Opal;595;4282;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320047262579;23505-340;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-402;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;44;23;146;White;Steel - Fagerhult - White;7320046213114;23505-402;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-519;595;4;3000;4282;Polystyrene - Fagerhult - Opal;595;4282;3000;3000;44;23;141;White;Steel - Fagerhult - White;7320047262616;23505-519;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-520;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;44;23;146;White;Steel - Fagerhult - White;7320047262630;23505-520;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-528;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;44;23;146;White;Steel - Fagerhult - White;7320047262555;23505-528;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB HL_23505-529;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;44;23;146;White;Steel - Fagerhult - White;7320047262593;23505-529;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506;595;4;4000;4512;Polystyrene - Fagerhult - Opal;595;4512;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320046213138;23506;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-3;595;4;4000;4512;Polystyrene - Fagerhult - Opal;595;4512;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320046213145;23506-3;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-111;595;4;4000;4512;Polystyrene - Fagerhult - Opal;595;4512;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047262654;23506-111;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-340;595;4;4000;4512;Polystyrene - Fagerhult - Opal;595;4512;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047262692;23506-340;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-402;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;44;23;154;White;Steel - Fagerhult - White;7320046213152;23506-402;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-519;595;4;4000;4512;Polystyrene - Fagerhult - Opal;595;4512;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047262739;23506-519;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-520;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;44;23;154;White;Steel - Fagerhult - White;7320047262753;23506-520;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-528;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;44;23;154;White;Steel - Fagerhult - White;7320047262678;23506-528;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB HL_23506-529;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;44;23;154;White;Steel - Fagerhult - White;7320047262715;23506-529;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510;595;4;3000;3211;Polystyrene - Fagerhult - Opal;595;3211;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320046282370;23510;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-3;595;4;3000;3211;Polystyrene - Fagerhult - Opal;595;3211;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320046282387;23510-3;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-111;595;4;3000;3211;Polystyrene - Fagerhult - Opal;595;3211;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320047262777;23510-111;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-340;595;4;3000;3211;Polystyrene - Fagerhult - Opal;595;3211;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320047262814;23510-340;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-402;595;4;3000;2992;Polystyrene - Fagerhult - Opal;595;2992;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320046282394;23510-402;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-519;595;4;3000;3211;Polystyrene - Fagerhult - Opal;595;3211;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320047262852;23510-519;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-520;595;4;3000;2992;Polystyrene - Fagerhult - Opal;595;2992;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320047262876;23510-520;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-528;595;4;3000;2992;Polystyrene - Fagerhult - Opal;595;2992;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320047262791;23510-528;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 3K VTB LL_23510-529;595;4;3000;2992;Polystyrene - Fagerhult - Opal;595;2992;3000;3000;44;23;145;White;Steel - Fagerhult - White;7320047262838;23510-529;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511;595;4;4000;3384;Polystyrene - Fagerhult - Opal;595;3384;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320046282899;23511;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-3;595;4;4000;3384;Polystyrene - Fagerhult - Opal;595;3384;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320046282905;23511-3;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-111;595;4;4000;3384;Polystyrene - Fagerhult - Opal;595;3384;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320047262890;23511-111;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-340;595;4;4000;3384;Polystyrene - Fagerhult - Opal;595;3384;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320047262937;23511-340;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-402;595;4;4000;3153;Polystyrene - Fagerhult - Opal;595;3153;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320046282912;23511-402;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-519;595;4;4000;3384;Polystyrene - Fagerhult - Opal;595;3384;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320047262975;23511-519;22;22;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-520;595;4;4000;3153;Polystyrene - Fagerhult - Opal;595;3153;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320047262999;23511-520;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-528;595;4;4000;3153;Polystyrene - Fagerhult - Opal;595;3153;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320047262913;23511-528;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 4K VTB LL_23511-529;595;4;4000;3153;Polystyrene - Fagerhult - Opal;595;3153;4000;4000;44;23;153;White;Steel - Fagerhult - White;7320047262951;23511-529;21;21;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 OPAL 830 ORGANIC RESP. VTB_27970;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;20;23;144;White;Steel - Fagerhult - White;7316911651099;27970;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 830 ORGANIC RESP. VTB_27970-3;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;20;23;144;White;Steel - Fagerhult - White;7316911651112;27970-3;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 830 ORGANIC RESP. VTB_27970-340;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;20;23;141;White;Steel - Fagerhult - White;7316911651150;27970-340;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 830 ORGANIC RESP. VTB_27970-519;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;20;23;141;White;Steel - Fagerhult - White;7316911651174;27970-519;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 830 ORGANIC RESP. VTB_27970-111;595;4;3000;4186;Polystyrene - Fagerhult - Opal;595;4186;3000;3000;20;23;141;White;Steel - Fagerhult - White;7316911651136;27970-111;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 840 ORGANIC RESP. VTB_27971;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;20;23;152;White;Steel - Fagerhult - White;7316911651198;27971;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 840 ORGANIC RESP. VTB_27971-3;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;20;23;152;White;Steel - Fagerhult - White;7316911651211;27971-3;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 840 ORGANIC RESP. VTB_27971-111;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;20;23;148;White;Steel - Fagerhult - White;7316911651235;27971-111;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 840 ORGANIC RESP. VTB_27971-340;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;20;23;148;White;Steel - Fagerhult - White;7316911651259;27971-340;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 840 ORGANIC RESP. VTB_27971-519;595;4;4000;4410;Polystyrene - Fagerhult - Opal;595;4410;4000;4000;20;23;148;White;Steel - Fagerhult - White;7316911651273;27971-519;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 OPAL 930 ORGANIC RESP. VTB_27978-111;595;4;3000;3503;Polystyrene - Fagerhult - Opal;595;3503;3000;3000;20;23;120;White;Steel - Fagerhult - White;7316911685193;27978-111;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 OPAL 930 ORGANIC RESP. VTB_27978;595;4;3000;3503;Polystyrene - Fagerhult - Opal;595;3503;3000;3000;20;23;120;White;Steel - Fagerhult - White;7316911685179;27978;29;29;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 OPAL 930 ORGANIC RESP. VTB_27978-3;595;4;3000;3503;Polystyrene - Fagerhult - Opal;595;3503;3000;3000;20;23;118;White;Steel - Fagerhult - White;7316911685186;27978-3;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 OPAL 930 ORGANIC RESP. VTB_27978-340;595;4;3000;3503;Polystyrene - Fagerhult - Opal;595;3503;3000;3000;20;23;118;White;Steel - Fagerhult - White;7316911685209;27978-340;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 OPAL 930 ORGANIC RESP. VTB_27978-519;595;4;3000;3503;Polystyrene - Fagerhult - Opal;595;3503;3000;3000;20;23;118;White;Steel - Fagerhult - White;7316911685230;27978-519;30;30;Multilume Slim Opal;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel. Recessed depth 23 mm.;min. 90;E;1;2
