;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Temperature Color##COLOR_TEMPERATURE##KELVIN;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;BIM Version##OTHER##
NOTOR36 3-SPOT MODULE REC NARROW BEAM 930_16087-20296;56;1.2;1548;600;3000;20;122;85;White;Aluminium - Fagerhult - White;7320049981577;16087-20296;18;Notor 36 Spot module;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Opal or Beta Opti Nano louvre. Single or series installation.;min. 90;1
NOTOR36 3-SPOT MODULE REC MEDIUM BEAM 930_16087-20297;56;1.2;1404;621;3000;20;122;77;White;Aluminium - Fagerhult - White;7320049981591;16087-20297;18;Notor 36 Spot module;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Opal or Beta Opti Nano louvre. Single or series installation.;min. 90;1
NOTOR36 3-SPOT MODULE REC NARROW BEAM 930_16087-20288;56;1.2;1548;600;3000;20;122;85;White;Aluminium - Fagerhult - White;7320049981218;16087-20288;18;Notor 36 Spot module;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Opal or Beta Opti Nano louvre. Single or series installation.;min. 90;1
NOTOR36 3-SPOT MODULE REC MEDIUM BEAM 930_16087-20289;56;1.2;1404;600;3000;20;122;77;White;Aluminium - Fagerhult - White;7320049981232;16087-20289;18;Notor 36 Spot module;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Opal or Beta Opti Nano louvre. Single or series installation.;min. 90;1
NOTOR36 3-SPOT MODULE REC NARROW BEAM 930_16087-20290;56;1.2;1548;600;3000;20;122;85;Black;Aluminium - Fagerhult - Black;7320049981256;16087-20290;18;Notor 36 Spot module;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Opal or Beta Opti Nano louvre. Single or series installation.;min. 90;1
NOTOR36 3-SPOT MODULE REC MEDIUM BEAM 930_16087-20291;56;1.2;1404;600;3000;20;122;77;Black;Aluminium - Fagerhult - Black;7320049981270;16087-20291;18;Notor 36 Spot module;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Opal or Beta Opti Nano louvre. Single or series installation.;min. 90;1
