;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;MODEL##OTHER##;End Cap 1##OTHER##
NOTOR REC DELTA 4K 2400 WHITE HL SINGLE _22225;90.5;9.4;4000;5306;Plastic - Fagerhult - Delta Microprism;2366;5306;4000;4000;20;102;117;White;Aluminium - Fagerhult - White;7320047934094;22225;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 2400 WHITE HL SINGLE _22225-402;90.5;9.4;4000;5003;Plastic - Fagerhult - Delta Microprism;2366;5003;4000;4000;20;102;115;White;Aluminium - Fagerhult - White;7320047934117;22225-402;43,5;43,5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 WHITE HL SINGLE_22226;90.5;9.4;3000;5035;Plastic - Fagerhult - Delta Microprism;2366;5035;3000;3000;20;102;111;White;Aluminium - Fagerhult - White;7320047934131;22226;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 WHITE HL SINGLE_22226-402;90.5;9.4;3000;5003;Plastic - Fagerhult - Delta Microprism;2366;5003;3000;3000;20;102;109;White;Aluminium - Fagerhult - White;7320047934155;22226-402;45,9;45,9;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 2400 ELOX HL SINGLE_22227;90.5;9.4;4000;5306;Plastic - Fagerhult - Delta Microprism;2366;5306;4000;4000;20;102;117;Anodised;Aluminium - Fagerhult - Anodised;7320047934179;22227;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 2400 ELOX HL SINGLE_22227-402;90.5;9.4;4000;5003;Plastic - Fagerhult - Delta Microprism;2366;5003;4000;4000;20;102;115;Anodised;Aluminium - Fagerhult - Anodised;7320047934193;22227-402;43,5;43,5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 ELOX HL SINGLE_22228;90.5;9.4;3000;5035;Plastic - Fagerhult - Delta Microprism;2366;5035;3000;3000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320047934216;22228;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 ELOX HL SINGLE_22228-402;90.5;9.4;3000;5003;Plastic - Fagerhult - Delta Microprism;2366;5003;3000;3000;20;102;109;Anodised;Aluminium - Fagerhult - Anodised;7320047934230;22228-402;45,9;45,9;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 2400 WHITE LL SINGLE_22229;90.5;9.4;4000;2648;Plastic - Fagerhult - Delta Microprism;2366;2648;4000;4000;20;102;112;White;Aluminium - Fagerhult - White;7320047934254;22229;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 2400 WHITE LL SINGLE_22229-402;90.5;9.4;4000;2526;Plastic - Fagerhult - Delta Microprism;2366;2526;4000;4000;20;102;108;White;Aluminium - Fagerhult - White;7320047934278;22229-402;23,4;23,4;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 WHITE LL SINGLE_22230;90.5;9.4;3000;2512;Plastic - Fagerhult - Delta Microprism;2366;2512;3000;3000;20;102;106;White;Aluminium - Fagerhult - White;7320047934292;22230;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 WHITE LL SINGLE_22230-402;90.5;9.4;3000;2526;Plastic - Fagerhult - Delta Microprism;2366;2526;3000;3000;20;102;108;White;Aluminium - Fagerhult - White;7320047934315;22230-402;23,4;23,4;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 2400 ELOX LL SINGLE_22231;90.5;9.4;4000;2648;Plastic - Fagerhult - Delta Microprism;2366;2648;4000;4000;20;102;112;Anodised;Aluminium - Fagerhult - Anodised;7320047934339;22231;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 2400 ELOX LL SINGLE_22231-402;90.5;9.4;4000;2526;Plastic - Fagerhult - Delta Microprism;2366;2526;4000;4000;20;102;108;Anodised;Aluminium - Fagerhult - Anodised;7320047934353;22231-402;23,4;23,4;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 ELOX LL SINGLE_22232;90.5;7.1;3000;2752;Plastic - Fagerhult - Delta Microprism;2366;2752;3000;3000;20;102;110;Anodised;Aluminium - Fagerhult - Anodised;7320047934377;22232;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 2400 ELOX LL SINGLE_22232-402;90.5;9.4;3000;2526;Plastic - Fagerhult - Delta Microprism;2366;2526;3000;3000;20;102;108;Anodised;Aluminium - Fagerhult - Anodised;7320047934391;22232-402;45,9;45,9;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 ELOX LL SINGLE_23515;90.5;1.9;3000;667;Plastic - Fagerhult - Delta Microprism;585;667;3000;3000;20;102;83;Anodised;Aluminium - Fagerhult - Anodised;7320046502409;23515;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 ELOX LL SINGLE_23515-402;90.5;2.4;3000;584;Plastic - Fagerhult - Delta Microprism;585;584;3000;3000;20;102;85;Anodised;Aluminium - Fagerhult - Anodised;7320046502423;23515-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 ELOX LL SINGLE_23516;90.5;4.8;3000;1285;Plastic - Fagerhult - Delta Microprism;1170;1285;3000;3000;20;102;98;Anodised;Aluminium - Fagerhult - Anodised;7320046502447;23516;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 ELOX LL SINGLE_23516-402;90.5;4.8;3000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046502461;23516-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 ELOX LL SINGLE_23518;90.5;2.4;4000;660;Plastic - Fagerhult - Delta Microprism;585;660;4000;4000;20;102;86;Anodised;Aluminium - Fagerhult - Anodised;7320046502522;23518;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 ELOX LL SINGLE_23518-402;90.5;2.4;4000;615;Plastic - Fagerhult - Delta Microprism;585;615;4000;4000;20;102;89;Anodised;Aluminium - Fagerhult - Anodised;7320046502546;23518-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 ELOX LL SINGLE_23519;90.5;4.8;4000;1356;Plastic - Fagerhult - Delta Microprism;1170;1356;4000;4000;20;102;103;Anodised;Aluminium - Fagerhult - Anodised;7320046502560;23519;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 ELOX LL SINGLE_23519-402;90.5;4.8;4000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;4000;4000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046502584;23519-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 WHITE LL SINGLE_23521;90.5;2.4;3000;627;Plastic - Fagerhult - Delta Microprism;585;627;3000;3000;20;102;81;White;Aluminium - Fagerhult - White;7320046502645;23521;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 WHITE LL SINGLE_23521-402;90.5;2.4;3000;584;Plastic - Fagerhult - Delta Microprism;585;584;3000;3000;20;102;85;White;Aluminium - Fagerhult - White;7320046502669;23521-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 WHITE LL SINGLE_23522;90.5;4.8;3000;1285;Plastic - Fagerhult - Delta Microprism;1170;1285;3000;3000;20;102;98;White;Aluminium - Fagerhult - White;7320046502683;23522;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 WHITE LL SINGLE_23522-402;90.5;4.8;3000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;3000;3000;20;102;107;White;Aluminium - Fagerhult - White;7320046502706;23522-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 WHITE LL SINGLE_23524;90.5;2.4;4000;660;Plastic - Fagerhult - Delta Microprism;585;660;4000;4000;20;102;86;White;Aluminium - Fagerhult - White;7320046502768;23524;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 WHITE LL SINGLE_23524-402;90.5;2.4;4000;615;Plastic - Fagerhult - Delta Microprism;585;615;4000;4000;20;102;89;White;Aluminium - Fagerhult - White;7320046502782;23524-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 WHITE LL SINGLE_23525;90.5;4.8;4000;1356;Plastic - Fagerhult - Delta Microprism;1170;1356;4000;4000;20;102;103;White;Aluminium - Fagerhult - White;7320046502805;23525;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 WHITE LL SINGLE_23525-402;90.5;4.8;4000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;4000;4000;20;102;107;White;Aluminium - Fagerhult - White;7320046502829;23525-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 ELOX HL SINGLE_23527;90.5;1.9;3000;1188;Plastic - Fagerhult - Delta Microprism;585;1188;3000;3000;20;102;91;Anodised;Aluminium - Fagerhult - Anodised;7320046504588;23527;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 ELOX HL SINGLE_23527-402;90.5;2.4;3000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;3000;3000;20;102;95;Anodised;Aluminium - Fagerhult - Anodised;7320046504601;23527-402;14.5;14.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 ELOX HL SINGLE_23528;90.5;4.8;3000;2515;Plastic - Fagerhult - Delta Microprism;1170;2515;3000;3000;20;102;104;Anodised;Aluminium - Fagerhult - Anodised;7320046504625;23528;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 ELOX HL SINGLE_23528-402;90.5;4.8;3000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046504649;23528-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 ELOX HL SINGLE_23530;90.5;2.4;4000;1289;Plastic - Fagerhult - Delta Microprism;585;1289;4000;4000;20;102;101;Anodised;Aluminium - Fagerhult - Anodised;7320046504700;23530;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 ELOX HL SINGLE_23530-402;90.5;2.4;4000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;4000;4000;20;102;100;Anodised;Aluminium - Fagerhult - Anodised;7320046504724;23530-402;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 ELOX HL SINGLE_23531;90.5;4.8;4000;2653;Plastic - Fagerhult - Delta Microprism;1170;2653;4000;4000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046504748;23531;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 ELOX HL SINGLE_23531-402;90.5;4.8;4000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;4000;4000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046504762;23531-402;24.5;24.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 WHITE HL SINGLE_23533;90.5;2.4;3000;1223;Plastic - Fagerhult - Delta Microprism;585;1223;3000;3000;20;102;96;White;Aluminium - Fagerhult - White;7320046502904;23533;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 WHITE HL SINGLE_23533-402;90.5;2.4;3000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;3000;3000;20;102;95;White;Aluminium - Fagerhult - White;7320046502928;23533-402;14.5;14.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 WHITE HL SINGLE_23534;90.5;3.7;3000;2450;Plastic - Fagerhult - Delta Microprism;1170;2450;3000;3000;20;102;98;White;Aluminium - Fagerhult - White;7320046502942;23534;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 1200 WHITE HL SINGLE_23534-402;90.5;4.8;3000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;3000;3000;20;102;107;White;Aluminium - Fagerhult - White;7320046502966;23534-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 WHITE HL SINGLE_23536;90.5;2.4;4000;1289;Plastic - Fagerhult - Delta Microprism;585;1289;4000;4000;20;102;101;White;Aluminium - Fagerhult - White;7320046503024;23536;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 600 WHITE HL SINGLE_23536-402;90.5;2.4;4000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;4000;4000;20;102;100;White;Aluminium - Fagerhult - White;7320046503048;23536-402;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 WHITE HL SINGLE_23537;90.5;4.8;4000;2653;Plastic - Fagerhult - Delta Microprism;1170;2653;4000;4000;20;102;111;White;Aluminium - Fagerhult - White;7320046504809;23537;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 4K 1200 WHITE HL SINGLE_23537-402;90.5;4.8;4000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;4000;4000;20;102;111;White;Aluminium - Fagerhult - White;7320046504823;23537-402;24.5;24.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;2;0
NOTOR REC DELTA 3K 600 ELOX LL START_23539;90.5;1.9;3000;667;Plastic - Fagerhult - Delta Microprism;585;667;3000;3000;20;102;83;Anodised;Aluminium - Fagerhult - Anodised;7320046504885;23539;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 ELOX LL START_23539-402;90.5;2.4;3000;584;Plastic - Fagerhult - Delta Microprism;585;584;3000;3000;20;102;85;Anodised;Aluminium - Fagerhult - Anodised;7320046504908;23539-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 ELOX LL START_23540;90.5;4.8;3000;1285;Plastic - Fagerhult - Delta Microprism;1170;1285;3000;3000;20;102;98;Anodised;Aluminium - Fagerhult - Anodised;7320046504922;23540;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 ELOX LL START_23540-402;90.5;4.8;3000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046504946;23540-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 ELOX LL START_23541;90.5;7.4;3000;2752;Plastic - Fagerhult - Delta Microprism;2339;2752;3000;3000;20;102;110;Anodised;Aluminium - Fagerhult - Anodised;7320046503062;23541;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 ELOX LL START_23541-402;90.5;9.4;3000;2526;Plastic - Fagerhult - Delta Microprism;2339;2526;3000;3000;20;102;108;Anodised;Aluminium - Fagerhult - Anodised;7320046503086;23541-402;23.5;23.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 ELOX LL START_23542;90.5;2.4;4000;660;Plastic - Fagerhult - Delta Microprism;585;660;4000;4000;20;102;86;Anodised;Aluminium - Fagerhult - Anodised;7320046503109;23542;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 ELOX LL START_23542-402;90.5;2.4;4000;615;Plastic - Fagerhult - Delta Microprism;585;615;4000;4000;20;102;89;Anodised;Aluminium - Fagerhult - Anodised;7320046503123;23542-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 ELOX LL START_23543;90.5;4.8;4000;1356;Plastic - Fagerhult - Delta Microprism;1170;1356;4000;4000;20;102;103;Anodised;Aluminium - Fagerhult - Anodised;7320046503147;23543;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 ELOX LL START_23543-402;90.5;4.8;4000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;4000;4000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046503161;23543-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 ELOX LL START_23544;90.5;9.4;4000;2648;Plastic - Fagerhult - Delta Microprism;2339;2648;4000;4000;20;102;112;Anodised;Aluminium - Fagerhult - Anodised;7320046503185;23544;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 ELOX LL START_23544-402;90.5;9.4;4000;2526;Plastic - Fagerhult - Delta Microprism;2339;2526;4000;4000;20;102;108;Anodised;Aluminium - Fagerhult - Anodised;7320046503208;23544-402;23.5;23.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 WHITE LL START_23545;90.5;2.4;3000;627;Plastic - Fagerhult - Delta Microprism;585;627;3000;3000;20;102;81;White;Aluminium - Fagerhult - White;7320046503222;23545;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 WHITE LL START_23545-402;90.5;2.4;3000;584;Plastic - Fagerhult - Delta Microprism;585;584;3000;3000;20;102;85;White;Aluminium - Fagerhult - White;7320046503246;23545-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 WHITE LL START_23546;90.5;4.8;3000;1285;Plastic - Fagerhult - Delta Microprism;1170;1285;3000;3000;20;102;98;White;Aluminium - Fagerhult - White;7320046503260;23546;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 WHITE LL START_23546-402;90.5;4.8;3000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;3000;3000;20;102;107;White;Aluminium - Fagerhult - White;7320046503284;23546-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 WHITE LL START_23547;90.5;9.4;3000;2512;Plastic - Fagerhult - Delta Microprism;2339;2512;3000;3000;20;102;106;White;Aluminium - Fagerhult - White;7320046503307;23547;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 WHITE LL START_23547-402;90.5;9.4;3000;2526;Plastic - Fagerhult - Delta Microprism;2339;2526;3000;3000;20;102;108;White;Aluminium - Fagerhult - White;7320046503321;23547-402;23.5;23.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 WHITE LL START_23548;90.5;2.4;4000;660;Plastic - Fagerhult - Delta Microprism;585;660;4000;4000;20;102;86;White;Aluminium - Fagerhult - White;7320046503345;23548;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 WHITE LL START_23548-402;90.5;2.4;4000;615;Plastic - Fagerhult - Delta Microprism;585;615;4000;4000;20;102;89;White;Aluminium - Fagerhult - White;7320046503369;23548-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 WHITE LL START_23549;90.5;4.8;4000;1356;Plastic - Fagerhult - Delta Microprism;1170;1356;4000;4000;20;102;103;White;Aluminium - Fagerhult - White;7320046503383;23549;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 WHITE LL START_23549-402;90.5;4.8;4000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;4000;4000;20;102;107;White;Aluminium - Fagerhult - White;7320046503406;23549-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 WHITE LL START_23550;90.5;9.4;4000;2648;Plastic - Fagerhult - Delta Microprism;2339;2648;4000;4000;20;102;112;White;Aluminium - Fagerhult - White;7320046503420;23550;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 WHITE LL START_23550-402;90.5;9.4;4000;2526;Plastic - Fagerhult - Delta Microprism;2339;2526;4000;4000;20;102;108;White;Aluminium - Fagerhult - White;7320046503444;23550-402;23.5;23.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 ELOX HL START_23551;90.5;1.9;3000;1188;Plastic - Fagerhult - Delta Microprism;585;1188;3000;3000;20;102;91;Anodised;Aluminium - Fagerhult - Anodised;7320046503468;23551;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 ELOX HL START_23551-402;90.5;2.4;3000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;3000;3000;20;102;95;Anodised;Aluminium - Fagerhult - Anodised;7320046503482;23551-402;14.5;14.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 ELOX HL START_23552;90.5;4.8;3000;2515;Plastic - Fagerhult - Delta Microprism;1170;2515;3000;3000;20;102;104;Anodised;Aluminium - Fagerhult - Anodised;7320046503505;23552;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 ELOX HL START_23552-402;90.5;4.8;3000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046503529;23552-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 ELOX HL START_23553;90.5;9.4;3000;5035;Plastic - Fagerhult - Delta Microprism;2339;5035;3000;3000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046503543;23553;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 ELOX HL START_23553-402;90.5;7.4;3000;4900;Plastic - Fagerhult - Delta Microprism;2339;4900;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046503567;23553-402;46;46;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 ELOX HL START_23554;90.5;2.4;4000;1289;Plastic - Fagerhult - Delta Microprism;585;1289;4000;4000;20;102;101;Anodised;Aluminium - Fagerhult - Anodised;7320046503581;23554;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 ELOX HL START_23554-402;90.5;2.4;4000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;4000;4000;20;102;100;Anodised;Aluminium - Fagerhult - Anodised;7320046503604;23554-402;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 ELOX HL START_23555;90.5;4.8;4000;2653;Plastic - Fagerhult - Delta Microprism;1170;2653;4000;4000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046503628;23555;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 ELOX HL START_23555-402;90.5;4.8;4000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;4000;4000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046503642;23555-402;24.5;24.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 ELOX HL START_23556;90.5;9.4;4000;5306;Plastic - Fagerhult - Delta Microprism;2339;5306;4000;4000;20;102;117;Anodised;Aluminium - Fagerhult - Anodised;7320046503666;23556;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 ELOX HL START_23556-402;90.5;9.4;4000;5003;Plastic - Fagerhult - Delta Microprism;2339;5003;4000;4000;20;102;115;Anodised;Aluminium - Fagerhult - Anodised;7320046503680;23556-402;47;47;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 WHITE HL START_23557;90.5;2.4;3000;1223;Plastic - Fagerhult - Delta Microprism;585;1223;3000;3000;20;102;96;White;Aluminium - Fagerhult - White;7320046503703;23557;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 WHITE HL START_23557-402;90.5;2.4;3000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;3000;3000;20;102;95;White;Aluminium - Fagerhult - White;7320046503727;23557-402;14.5;14.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 WHITE HL START_23558;90.5;4.8;3000;2515;Plastic - Fagerhult - Delta Microprism;1170;2515;3000;3000;20;102;104;White;Aluminium - Fagerhult - White;7320046503741;23558;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 1200 WHITE HL START_23558-402;90.5;4.8;3000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;3000;3000;20;102;107;White;Aluminium - Fagerhult - White;7320046503765;23558-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 WHITE HL START_23559;90.5;9.4;3000;5035;Plastic - Fagerhult - Delta Microprism;2339;5035;3000;3000;20;102;111;White;Aluminium - Fagerhult - White;7320046503789;23559;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 2400 WHITE HL START_23559-402;90.5;9.4;3000;5003;Plastic - Fagerhult - Delta Microprism;2339;5003;3000;3000;20;102;109;White;Aluminium - Fagerhult - White;7320046503802;23559-402;49.5;49.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 WHITE HL START_23560;90.5;2.4;4000;1289;Plastic - Fagerhult - Delta Microprism;585;1289;4000;4000;20;102;101;White;Aluminium - Fagerhult - White;7320046503826;23560;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 600 WHITE HL START_23560-402;90.5;2.4;4000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;4000;4000;20;102;100;White;Aluminium - Fagerhult - White;7320046503840;23560-402;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 WHITE HL START_23561;90.5;4.8;4000;2653;Plastic - Fagerhult - Delta Microprism;1170;2653;4000;4000;20;102;111;White;Aluminium - Fagerhult - White;7320046503864;23561;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 1200 WHITE HL START_23561-402;90.5;4.8;4000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;4000;4000;20;102;111;White;Aluminium - Fagerhult - White;7320046503888;23561-402;24.5;24.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 WHITE HL START_23562;90.5;9.4;4000;5306;Plastic - Fagerhult - Delta Microprism;2339;5306;4000;4000;20;102;117;White;Aluminium - Fagerhult - White;7320046503901;23562;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 4K 2400 WHITE HL START_23562-402;90.5;9.4;4000;5003;Plastic - Fagerhult - Delta Microprism;2339;5003;4000;4000;20;102;115;White;Aluminium - Fagerhult - White;7320046503925;23562-402;47;47;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;1;1
NOTOR REC DELTA 3K 600 ELOX LL CONT._23563;90.5;1.9;3000;667;Plastic - Fagerhult - Delta Microprism;585;667;3000;3000;20;102;83;Anodised;Aluminium - Fagerhult - Anodised;7320046503949;23563;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 600 ELOX LL CONT._23563-402;90.5;2.4;3000;584;Plastic - Fagerhult - Delta Microprism;585;584;3000;3000;20;102;85;Anodised;Aluminium - Fagerhult - Anodised;7320046503963;23563-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 ELOX LL CONT._23564;90.5;4.8;3000;1285;Plastic - Fagerhult - Delta Microprism;1170;1285;3000;3000;20;102;98;Anodised;Aluminium - Fagerhult - Anodised;7320046503987;23564;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 ELOX LL CONT._23564-402;90.5;4.8;3000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046504007;23564-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 ELOX LL CONT._23565;90.5;7.4;3000;2752;Plastic - Fagerhult - Delta Microprism;2339;2752;3000;3000;20;102;110;Anodised;Aluminium - Fagerhult - Anodised;7320046504021;23565;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 ELOX LL CONT._23565-402;90.5;9.4;3000;2526;Plastic - Fagerhult - Delta Microprism;2339;2526;3000;3000;20;102;108;Anodised;Aluminium - Fagerhult - Anodised;7320046504045;23565-402;23.5;23.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 ELOX LL CONT._23566;90.5;2.4;4000;660;Plastic - Fagerhult - Delta Microprism;585;660;4000;4000;20;102;86;Anodised;Aluminium - Fagerhult - Anodised;7320046504069;23566;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 ELOX LL CONT._23566-402;90.5;2.4;4000;615;Plastic - Fagerhult - Delta Microprism;585;615;4000;4000;20;102;89;Anodised;Aluminium - Fagerhult - Anodised;7320046504083;23566-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 ELOX LL CONT._23567;90.5;4.8;4000;1356;Plastic - Fagerhult - Delta Microprism;1170;1356;4000;4000;20;102;103;Anodised;Aluminium - Fagerhult - Anodised;7320046504106;23567;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 ELOX LL CONT._23567-402;90.5;4.8;4000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;4000;4000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046504120;23567-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 ELOX LL CONT._23568;90.5;9.4;4000;2648;Plastic - Fagerhult - Delta Microprism;2339;2648;4000;4000;20;102;112;Anodised;Aluminium - Fagerhult - Anodised;7320046504144;23568;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 ELOX LL CONT._23568-402;90.5;7.4;4000;2805;Plastic - Fagerhult - Delta Microprism;2339;2805;4000;4000;20;102;112;Anodised;Aluminium - Fagerhult - Anodised;7320046504168;23568-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 600 WHITE LL CONT._23569;90.5;2.4;3000;627;Plastic - Fagerhult - Delta Microprism;585;627;3000;3000;20;102;81;White;Aluminium - Fagerhult - White;7320046504182;23569;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 600 WHITE LL CONT._23569-402;90.5;2.4;3000;584;Plastic - Fagerhult - Delta Microprism;585;584;3000;3000;20;102;85;White;Aluminium - Fagerhult - White;7320046504205;23569-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 WHITE LL CONT._23570;90.5;4.8;3000;1285;Plastic - Fagerhult - Delta Microprism;1170;1285;3000;3000;20;102;98;White;Aluminium - Fagerhult - White;7320046504229;23570;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 WHITE LL CONT._23570-402;90.5;4.8;3000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;3000;3000;20;102;107;White;Aluminium - Fagerhult - White;7320046504243;23570-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 WHITE LL CONT._23571;90.5;9.4;3000;2512;Plastic - Fagerhult - Delta Microprism;2339;2512;3000;3000;20;102;106;White;Aluminium - Fagerhult - White;7320046504267;23571;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 WHITE LL CONT._23571-402;90.5;9.4;3000;2526;Plastic - Fagerhult - Delta Microprism;2339;2526;3000;3000;20;102;108;White;Aluminium - Fagerhult - White;7320046504281;23571-402;23.5;23.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 WHITE LL CONT._23572;90.5;2.4;4000;660;Plastic - Fagerhult - Delta Microprism;585;660;4000;4000;20;102;86;White;Aluminium - Fagerhult - White;7320046504304;23572;8;8;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 WHITE LL CONT._23572-402;90.5;2.4;4000;615;Plastic - Fagerhult - Delta Microprism;585;615;4000;4000;20;102;89;White;Aluminium - Fagerhult - White;7320046504328;23572-402;7.5;7.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 WHITE LL CONT._23573;90.5;4.8;4000;1356;Plastic - Fagerhult - Delta Microprism;1170;1356;4000;4000;20;102;103;White;Aluminium - Fagerhult - White;7320046504342;23573;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 WHITE LL CONT._23573-402;90.5;4.8;4000;1263;Plastic - Fagerhult - Delta Microprism;1170;1263;4000;4000;20;102;107;White;Aluminium - Fagerhult - White;7320046504366;23573-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 WHITE LL CONT._23574;90.5;9.4;4000;2648;Plastic - Fagerhult - Delta Microprism;2339;2648;4000;4000;20;102;112;White;Aluminium - Fagerhult - White;7320046504380;23574;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 WHITE LL CONT._23574-402;90.5;9.4;4000;2526;Plastic - Fagerhult - Delta Microprism;2339;2526;4000;4000;20;102;108;White;Aluminium - Fagerhult - White;7320046504403;23574-402;23.5;23.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 600 ELOX HL CONT._23575;90.5;1.9;3000;1188;Plastic - Fagerhult - Delta Microprism;585;1188;3000;3000;20;102;91;Anodised;Aluminium - Fagerhult - Anodised;7320046504427;23575;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 600 ELOX HL CONT._23575-402;90.5;2.4;3000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;3000;3000;20;102;95;Anodised;Aluminium - Fagerhult - Anodised;7320046504441;23575-402;14.5;14.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 ELOX HL CONT._23576;90.5;4.8;3000;2515;Plastic - Fagerhult - Delta Microprism;1170;2515;3000;3000;20;102;104;Anodised;Aluminium - Fagerhult - Anodised;7320046504465;23576;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 ELOX HL CONT._23576-402;90.5;4.8;3000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046504489;23576-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 ELOX HL CONT._23577;90.5;9.4;3000;5035;Plastic - Fagerhult - Delta Microprism;2339;5035;3000;3000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046504502;23577;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 ELOX HL CONT._23577-402;90.5;7.4;3000;4900;Plastic - Fagerhult - Delta Microprism;2339;4900;3000;3000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046504526;23577-402;46;46;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 ELOX HL CONT._23578;90.5;2.4;4000;1289;Plastic - Fagerhult - Delta Microprism;585;1289;4000;4000;20;102;101;Anodised;Aluminium - Fagerhult - Anodised;7320046504540;23578;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 ELOX HL CONT._23578-402;90.5;2.4;4000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;4000;4000;20;102;100;Anodised;Aluminium - Fagerhult - Anodised;7320046504564;23578-402;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 ELOX HL CONT._23579;90.5;4.8;4000;2653;Plastic - Fagerhult - Delta Microprism;1170;2653;4000;4000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046504960;23579;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 ELOX HL CONT._23579-402;90.5;4.8;4000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;4000;4000;20;102;111;Anodised;Aluminium - Fagerhult - Anodised;7320046504984;23579-402;24.5;24.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 ELOX HL CONT._23580;90.5;9.4;4000;5306;Plastic - Fagerhult - Delta Microprism;2339;5306;4000;4000;20;102;117;Anodised;Aluminium - Fagerhult - Anodised;7320046505004;23580;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 ELOX HL CONT._23580-402;90.5;9.4;4000;5003;Plastic - Fagerhult - Delta Microprism;2339;5003;4000;4000;20;102;115;Anodised;Aluminium - Fagerhult - Anodised;7320046505028;23580-402;47;47;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 600 WHITE HL CONT._23581;90.5;2.4;3000;1223;Plastic - Fagerhult - Delta Microprism;585;1223;3000;3000;20;102;96;White;Aluminium - Fagerhult - White;7320046505042;23581;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 600 WHITE HL CONT._23581-402;90.5;2.4;3000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;3000;3000;20;102;95;White;Aluminium - Fagerhult - White;7320046505066;23581-402;14.5;14.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 WHITE HL CONT._23582;90.5;4.8;3000;2515;Plastic - Fagerhult - Delta Microprism;1170;2515;3000;3000;20;102;104;White;Aluminium - Fagerhult - White;7320046505080;23582;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 1200 WHITE HL CONT._23582-402;90.5;4.8;3000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;3000;3000;20;102;107;White;Aluminium - Fagerhult - White;7320046505103;23582-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 WHITE HL CONT._23583;90.5;9.4;3000;5035;Plastic - Fagerhult - Delta Microprism;2339;5035;3000;3000;20;102;111;White;Aluminium - Fagerhult - White;7320046505127;23583;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 3K 2400 WHITE HL CONT._23583-402;90.5;9.4;3000;5003;Plastic - Fagerhult - Delta Microprism;2339;5003;3000;3000;20;102;109;White;Aluminium - Fagerhult - White;7320046505141;23583-402;49.5;49.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 WHITE HL CONT._23584;90.5;2.4;4000;1289;Plastic - Fagerhult - Delta Microprism;585;1289;4000;4000;20;102;101;White;Aluminium - Fagerhult - White;7320046505165;23584;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 600 WHITE HL CONT._23584-402;90.5;2.4;4000;1215;Plastic - Fagerhult - Delta Microprism;585;1215;4000;4000;20;102;100;White;Aluminium - Fagerhult - White;7320046505189;23584-402;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 WHITE HL CONT._23585;90.5;4.8;4000;2653;Plastic - Fagerhult - Delta Microprism;1170;2653;4000;4000;20;102;111;White;Aluminium - Fagerhult - White;7320046505202;23585;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 1200 WHITE HL CONT._23585-402;90.5;4.8;4000;2501;Plastic - Fagerhult - Delta Microprism;1170;2501;4000;4000;20;102;111;White;Aluminium - Fagerhult - White;7320046505226;23585-402;24.5;24.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 WHITE HL CONT._23586;90.5;9.4;4000;5306;Plastic - Fagerhult - Delta Microprism;2339;5306;4000;4000;20;102;117;White;Aluminium - Fagerhult - White;7320046505240;23586;45;45;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 4K 2400 WHITE HL CONT._23586-402;90.5;9.4;4000;5003;Plastic - Fagerhult - Delta Microprism;2339;5003;4000;4000;20;102;115;White;Aluminium - Fagerhult - White;7320046505264;23586-402;47;47;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;3;0
NOTOR REC DELTA 1200 TW ELOX SINGLE_24068;90.5;3.7;3000;2200;Plastic - Fagerhult - Delta Microprism;1170;2200;3000;3000;20;102;86;Anodised;Aluminium - Fagerhult - Anodised;7320047629174;24068;25,6;25,6;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;2;0
NOTOR REC DELTA 2400 TW ELOX SINGLE_24069;90.5;7.4;3000;4400;Plastic - Fagerhult - Delta Microprism;2339;4400;3000;3000;20;102;93;Anodised;Aluminium - Fagerhult - Anodised;7320047629198;24069;47,3;47,3;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;2;0
NOTOR REC DELTA 1200 TW ELOX START_24071;90.5;3.7;3000;2200;Plastic - Fagerhult - Delta Microprism;1170;2200;3000;3000;20;102;86;Anodised;Aluminium - Fagerhult - Anodised;7320047629235;24071;25,6;25,6;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;1;1
NOTOR REC DELTA 2400 TW ELOX START_24072;90.5;7.4;3000;4400;Plastic - Fagerhult - Delta Microprism;2339;4400;3000;3000;20;102;93;Anodised;Aluminium - Fagerhult - Anodised;7320047629259;24072;47,3;47,3;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;1;1
NOTOR REC DELTA 1200 TW ELOX CON/END_24074;90.5;3.7;3000;2200;Plastic - Fagerhult - Delta Microprism;1170;2200;3000;3000;20;102;86;Anodised;Aluminium - Fagerhult - Anodised;7320047629297;24074;25,6;25,6;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;3;0
NOTOR REC DELTA 2400 TW ELOX CON/END_24075;90.5;7.4;3000;4400;Plastic - Fagerhult - Delta Microprism;2339;4400;3000;3000;20;102;93;Anodised;Aluminium - Fagerhult - Anodised;7320047629310;24075;47,3;47,3;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;3;0
NOTOR REC DELTA 1200 TW WHITE SINGLE_24089;90.5;3.7;3000;2200;Plastic - Fagerhult - Delta Microprism;1170;2200;3000;3000;20;102;86;White;Aluminium - Fagerhult - White;7320047629358;24089;25,6;25,6;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;2;0
NOTOR REC DELTA 2400 TW WHITE SINGLE_24090;90.5;7.4;3000;4400;Plastic - Fagerhult - Delta Microprism;2366;4400;3000;3000;20;102;93;White;Aluminium - Fagerhult - White;7320047629372;24090;47,3;47,3;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;2;0
NOTOR REC DELTA 1200 TW WHITE START_24092;90.5;3.7;3000;2200;Plastic - Fagerhult - Delta Microprism;1170;2200;3000;3000;20;102;86;White;Aluminium - Fagerhult - White;7320047629419;24092;25,6;25,6;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;1;1
NOTOR REC DELTA 2400 TW WHITE START_24093;90.5;7.4;3000;4400;Plastic - Fagerhult - Delta Microprism;2339;4400;3000;3000;20;102;93;White;Aluminium - Fagerhult - White;7320047629433;24093;47,3;47,3;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;1;1
NOTOR REC DELTA 1200 TW WHITE CON/END_24095;90.5;3.7;3000;2200;Plastic - Fagerhult - Delta Microprism;1170;2200;3000;3000;20;102;86;White;Aluminium - Fagerhult - White;7320047629471;24095;25,6;25,6;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;3;0
NOTOR REC DELTA 2400 TW WHITE CON/END_24096;90.5;7.4;3000;4400;Plastic - Fagerhult - Delta Microprism;2339;4400;3000;3000;20;102;93;White;Aluminium - Fagerhult - White;7320047629495;24096;47,3;47,3;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 90;E;2;3;0
