;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Springs Size##OTHER##
POZZO 345 DALI DELTA 830_24300-20005;1.7;3000;1329;Polystyrene - Fagerhult - Delta Microprism;1329;3000;3000;20;114;117;White;Aluminium - Fagerhult - White;7316910633461;24300-20005;13;13;360;Pozzo Delta;"Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. Stable assembly springs included. When installing in soft tile ceilings, mounting plates must be used, see accessories. The ballast housing is separate for flexible and quick installation.
<br>Do not cover with insulation. For detailed information, see the installation instructions.";A recessed luminaire in three different sizes. Adjustable Delta louvre shutters with two positions and the possibility of creating a well feel. High level of efficiency and optimal light comfort with different looks. A bevelled outer edge that provides a soft luminance transition to the ceiling.;min. 80;C;1;1
POZZO 345 DALI DELTA 840_24300-20006;1.7;4000;1400;Polystyrene - Fagerhult - Delta Microprism;1400;4000;4000;20;114;123;White;Aluminium - Fagerhult - White;7316910633492;24300-20006;13;13;360;Pozzo Delta;"Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. Stable assembly springs included. When installing in soft tile ceilings, mounting plates must be used, see accessories. The ballast housing is separate for flexible and quick installation.
<br>Do not cover with insulation. For detailed information, see the installation instructions.";A recessed luminaire in three different sizes. Adjustable Delta louvre shutters with two positions and the possibility of creating a well feel. High level of efficiency and optimal light comfort with different looks. A bevelled outer edge that provides a soft luminance transition to the ceiling.;min. 80;C;1;1
POZZO 445 DALI DELTA 830_24301-20001;2.5;3000;2278;Polystyrene - Fagerhult - Delta Microprism;2278;3000;3000;20;114;129;White;Aluminium - Fagerhult - White;7316910740527;24301-20001;19;19;460;Pozzo Delta;"Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. Stable assembly springs included. When installing in soft tile ceilings, mounting plates must be used, see accessories. The ballast housing is separate for flexible and quick installation.
<br>Do not cover with insulation. For detailed information, see the installation instructions.";A recessed luminaire in three different sizes. Adjustable Delta louvre shutters with two positions and the possibility of creating a well feel. High level of efficiency and optimal light comfort with different looks. A bevelled outer edge that provides a soft luminance transition to the ceiling.;min. 80;C;1;2
POZZO 445 DALI DELTA 840_24301-20002;2.5;4000;2400;Polystyrene - Fagerhult - Delta Microprism;2400;4000;4000;20;114;136;White;Aluminium - Fagerhult - White;7316910740688;24301-20002;19;19;460;Pozzo Delta;"Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. Stable assembly springs included. When installing in soft tile ceilings, mounting plates must be used, see accessories. The ballast housing is separate for flexible and quick installation.
<br>Do not cover with insulation. For detailed information, see the installation instructions.";A recessed luminaire in three different sizes. Adjustable Delta louvre shutters with two positions and the possibility of creating a well feel. High level of efficiency and optimal light comfort with different looks. A bevelled outer edge that provides a soft luminance transition to the ceiling.;min. 80;C;1;2
POZZO 545 DALI DELTA 840_24302-20000;3.2;4000;4000;Polystyrene - Fagerhult - Delta Microprism;4000;4000;4000;20;114;141;White;Aluminium - Fagerhult - White;7316910633614;24302-20000;31.5;31.5;560;Pozzo Delta;"Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. Stable assembly springs included. When installing in soft tile ceilings, mounting plates must be used, see accessories. The ballast housing is separate for flexible and quick installation.
<br>Do not cover with insulation. For detailed information, see the installation instructions.";A recessed luminaire in three different sizes. Adjustable Delta louvre shutters with two positions and the possibility of creating a well feel. High level of efficiency and optimal light comfort with different looks. A bevelled outer edge that provides a soft luminance transition to the ceiling.;min. 80;C;1;3
POZZO 545 DALI DELTA 830_24302-20001;3.2;3000;3796;Polystyrene - Fagerhult - Delta Microprism;3796;3000;3000;20;114;134;White;Aluminium - Fagerhult - White;7316910740879;24302-20001;31.5;31.5;560;Pozzo Delta;"Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. Stable assembly springs included. When installing in soft tile ceilings, mounting plates must be used, see accessories. The ballast housing is separate for flexible and quick installation.
<br>Do not cover with insulation. For detailed information, see the installation instructions.";A recessed luminaire in three different sizes. Adjustable Delta louvre shutters with two positions and the possibility of creating a well feel. High level of efficiency and optimal light comfort with different looks. A bevelled outer edge that provides a soft luminance transition to the ceiling.;min. 80;C;1;3
