;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Temperature Color##COLOR_TEMPERATURE##KELVIN;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;BIM Version##OTHER##
NOTOR36 3-SPOT MODULE CEIL NARROW BEAM 930_16086-20503;36;1;1548;603;3000;20;107;85;White;Aluminium - Fagerhult - White;7320049980617;16086-20503;18;Notor 36 Spot module;Keyhole slots permit individual or system surface-mounted installation.;Luminaire for surface-mounted installation, individually or in a system. Opal or Beta Opti Nano louvre.;min. 90;1
NOTOR36 3-SPOT MODULE CEIL NARROW BEAM 930_16086-20504;36;1;1548;603;3000;20;107;85;White;Aluminium - Fagerhult - White;7320049980624;16086-20504;18;Notor 36 Spot module;Keyhole slots permit individual or system surface-mounted installation.;Luminaire for surface-mounted installation, individually or in a system. Opal or Beta Opti Nano louvre.;min. 90;1
NOTOR36 3-SPOT MODULE CEIL MEDIUM BEAM 930_16086-20505;36;1;1404;603;3000;20;107;77;White;Aluminium - Fagerhult - White;7320049980662;16086-20505;18;Notor 36 Spot module;Keyhole slots permit individual or system surface-mounted installation.;Luminaire for surface-mounted installation, individually or in a system. Opal or Beta Opti Nano louvre.;min. 90;1
NOTOR36 3-SPOT MODULE CEIL MEDIUM BEAM 930_16086-20506;36;1;1404;603;3000;20;107;77;White;Aluminium - Fagerhult - White;7320049980686;16086-20506;18;Notor 36 Spot module;Keyhole slots permit individual or system surface-mounted installation.;Luminaire for surface-mounted installation, individually or in a system. Opal or Beta Opti Nano louvre.;min. 90;1
