;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Lighting Control##OTHER##
NOTOR 65 TRACK DELTA 1200 HL 830 OR_13674-20016;65;3.4;4000;3402;Acrylic - Fagerhult - Delta Microprism;1346;3402;4000;4000;20;65;126;White;Aluminium - Fagerhult - White;7316911826473;13674-20016;28.5;28.5;Notor 65 Track Delta;In Control Track.;Note 65 Track linear armature for mounting in lighting track. The Delta louvre in acrylic (PMMA) ensures high efficiency and optimal light comfort. The OR sensor is available as lighting control.;min. 80;C;1;1
NOTOR 65 TRACK DELTA 1200 HL 830 DALI_13674-20000;65;3.1;4000;3402;Acrylic - Fagerhult - Delta Microprism;1256;3402;4000;4000;20;65;134;White;Aluminium - Fagerhult - White;7316911784346;13674-20000;26.5;26.5;Notor 65 Track Delta;In Control Track.;Note 65 Track linear armature for mounting in lighting track. The Delta louvre in acrylic (PMMA) ensures high efficiency and optimal light comfort. The OR sensor is available as lighting control.;min. 80;C;1;0
