;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;LightDistribution##OTHER##;Track##OTHER##
TOUCH MINI G2 HL TW WIDE BEAM_84450-20011;135;1;4000;2317;195;20;270;89;White;Aluminium - Fagerhult - White;7316911401076;84450-20011;26;85;Touch Mini G2 Tunable White;In ceiling lighting track or pendent mounted. Control Track or iTrack (DALI), Lighting Track Pro (wireless control).;Spotlight installation on lighting track. Directed light with Tunable White that renders lighting with an extra dimension.;min. 90;F;1;Light : 84450-20011;1
