;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;LightDistribution##OTHER##
ZKYE 55 G2 WALL 927 WHITE NARROW BEAM_65220;55;0.7;2700;1501;175;20;117;107;White;Aluminium - Fagerhult - White;7316911259523;65220;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 927 WHITE NARROW BEAM_65220-402;55;0.7;2700;1501;175;20;117;105;White;Aluminium - Fagerhult - White;7316911259547;65220-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 927 BLACK NARROW BEAM_65221;55;0.7;2700;1501;175;20;117;107;Black;Aluminium - Fagerhult - Black;7316911259561;65221;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 927 BLACK NARROW BEAM_65221-402;55;0.7;2700;1501;175;20;117;105;Black;Aluminium - Fagerhult - Black;7316911259585;65221-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 927 WHITE MEDIUM BEAM_65222;55;0.7;2700;1498;175;20;117;107;White;Aluminium - Fagerhult - White;7316911259608;65222;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 927 WHITE MEDIUM BEAM_65222-402;55;0.7;2700;1498;175;20;117;105;White;Aluminium - Fagerhult - White;7316911259622;65222-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 927 BLACK MEDIUM BEAM_65223;55;0.7;2700;1498;175;20;117;107;Black;Aluminium - Fagerhult - Black;7316911259646;65223;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 927 BLACK MEDIUM BEAM_65223-402;55;0.7;2700;1498;175;20;117;105;Black;Aluminium - Fagerhult - Black;7316911259660;65223-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 927 WHITE WIDE BEAM_65224;55;0.7;2700;1542;175;20;117;110;White;Aluminium - Fagerhult - White;7316911259684;65224;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
ZKYE 55 G2 WALL 927 WHITE WIDE BEAM_65224-402;55;0.7;2700;1542;175;20;117;108;White;Aluminium - Fagerhult - White;7316911259707;65224-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
ZKYE 55 G2 WALL 927 BLACK WIDE BEAM_65225;55;0.7;2700;1542;175;20;117;110;Black;Aluminium - Fagerhult - Black;7316911259721;65225;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
ZKYE 55 G2 WALL 927 BLACK WIDE BEAM_65225-402;55;0.7;2700;1542;175;20;117;108;Black;Aluminium - Fagerhult - Black;7316911259745;65225-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
ZKYE 55 G2 WALL 930 WHITE NARROW BEAM_65226;55;0.7;3000;1516;175;20;117;108;White;Aluminium - Fagerhult - White;7316911259769;65226;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 930 WHITE NARROW BEAM_65226-402;55;0.7;3000;1516;175;20;117;106;White;Aluminium - Fagerhult - White;7316911259783;65226-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 930 BLACK NARROW BEAM_65227;55;0.7;3000;1516;175;20;117;108;Black;Aluminium - Fagerhult - Black;7316911259806;65227;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 930 BLACK NARROW BEAM_65227-402;55;0.7;3000;1516;175;20;117;106;Black;Aluminium - Fagerhult - Black;7316911259820;65227-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Narrow
ZKYE 55 G2 WALL 930 WHITE MEDIUM BEAM_65228;55;0.7;3000;1513;175;20;117;108;White;Aluminium - Fagerhult - White;7316911259844;65228;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 930 WHITE MEDIUM BEAM_65228-402;55;0.7;3000;1513;175;20;117;106;White;Aluminium - Fagerhult - White;7316911259868;65228-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 930 BLACK MEDIUM BEAM_65229;55;0.7;3000;1513;175;20;117;108;Black;Aluminium - Fagerhult - Black;7316911259882;65229;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 930 BLACK MEDIUM BEAM_65229-402;55;0.7;3000;1513;175;20;117;106;Black;Aluminium - Fagerhult - Black;7316911259905;65229-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Medium
ZKYE 55 G2 WALL 930 WHITE WIDE BEAM_65230;55;0.7;3000;1558;175;20;117;111;White;Aluminium - Fagerhult - White;7316911259929;65230;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
ZKYE 55 G2 WALL 930 WHITE WIDE BEAM_65230-402;55;0.7;3000;1558;175;20;117;109;White;Aluminium - Fagerhult - White;7316911259943;65230-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
ZKYE 55 G2 WALL 930 BLACK WIDE BEAM_65231;55;0.7;3000;1558;175;20;117;111;Black;Aluminium - Fagerhult - Black;7316911259967;65231;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
ZKYE 55 G2 WALL 930 BLACK WIDE BEAM_65231-402;55;0.7;3000;1558;175;20;117;109;Black;Aluminium - Fagerhult - Black;7316911259981;65231-402;14;Zkye 55 G2 Wall;For permanent wall installation.;A wall-mounted Ø 55 mm spotlight. Deep reflector for optimal light comfort and and good light distribution. Wall-mounted for direct connection from the rear, or with externally mounted cable from above.;min. 90;E;1;Light Zkye : Zkye_Wide
