;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##;Adapter##OTHER##
AIZING TRACK LENS WIDE 930 BLACK_58629;45;1.4;3000;2648;921;2648;3000;3000;20;85;142;Black;Aluminium - Fagerhult - Black;7316912295148;58629;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;E;1;1;1
AIZING TRACK LENS WIDE 930 BLACK_58629-504;45;1.5;3000;2401;911;2401;3000;3000;20;95;133;Black;Aluminium - Fagerhult - Black;7316912295155;58629-504;18;18;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;E;1;1;3
AIZING TRACK LENS WIDE 930 BLACK_58629-533;45;1.6;3000;2401;987;2401;3000;3000;20;94;128;Black;Aluminium - Fagerhult - Black;7316912295179;58629-533;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;E;1;2;2
AIZING TRACK LENS WIDE 930 WHITE_58630;45;1.4;3000;2648;921;2648;3000;3000;20;85;142;White;Aluminium - Fagerhult - White;7316912295117;58630;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;E;1;1;1
AIZING TRACK LENS WIDE 930 WHITE_58630-504;45;1.5;3000;2401;911;2401;3000;3000;20;95;133;White;Aluminium - Fagerhult - White;7316912295124;58630-504;18;18;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;E;1;1;3
AIZING TRACK LENS WIDE 930 WHITE_58630-533;45;1.6;3000;2401;987;2401;3000;3000;20;94;128;White;Aluminium - Fagerhult - White;7316912295131;58630-533;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;E;1;2;2
AIZING TRACK LENS WIDE 940 WHITE_58960;45;1.4;4000;2648;921;2648;4000;4000;20;85;142;White;Aluminium - Fagerhult - White;7316912295247;58960;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;D;1;1;1
AIZING TRACK LENS WIDE 940 WHITE_58960-504;45;1.5;4000;2401;911;2401;4000;4000;20;95;133;White;Aluminium - Fagerhult - White;7316912295254;58960-504;18;18;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;D;1;1;3
AIZING TRACK LENS WIDE 940 WHITE_58960-533;45;1.6;4000;2401;987;2401;4000;4000;20;94;128;White;Aluminium - Fagerhult - White;7316912295261;58960-533;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;D;1;2;2
AIZING TRACK LENS WIDE 940 BLACK_58961;45;1.4;4000;2648;921;2648;4000;4000;20;85;142;Black;Aluminium - Fagerhult - Black;7316912295292;58961;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;D;1;1;1
AIZING TRACK LENS WIDE 940 BLACK_58961-504;45;1.5;4000;2401;911;2401;4000;4000;20;95;133;Black;Aluminium - Fagerhult - Black;7316912295308;58961-504;18;18;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;D;1;1;3
AIZING TRACK LENS WIDE 940 BLACK_58961-533;45;1.6;4000;2401;987;2401;4000;4000;20;94;128;Black;Aluminium - Fagerhult - Black;7316912295315;58961-533;19;19;Aizing;Mounted on Lighting Track Pro 3-phase track or Control Track (DALI/OR).;Aizing is a linear rail-mounted luminaire, with multi-lens optics. The luminaire’s optics are well shielded, providing good light comfort. Control with Dali/phase pulse or Organic response.;min. 90;D;1;2;2
