;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Sensor##OTHER##
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166;295;2.2;3000;2093;Polystyrene - Fagerhult - Delta Microprism;598;2093;3000;3000;44;24;111;White;Steel - Fagerhult - White;7320047555565;23166;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-3;295;2.2;3000;2093;Polystyrene - Fagerhult - Delta Microprism;598;2093;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613852;23166-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-111;295;2.2;3000;2093;Polystyrene - Fagerhult - Delta Microprism;598;2093;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613845;23166-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-340;295;2.2;3000;2093;Polystyrene - Fagerhult - Delta Microprism;598;2093;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613869;23166-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-402;295;2.2;3000;2004;Polystyrene - Fagerhult - Delta Microprism;598;2004;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613883;23166-402;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-519;295;2.2;3000;2093;Polystyrene - Fagerhult - Delta Microprism;598;2093;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613876;23166-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-520;295;2.2;3000;2004;Polystyrene - Fagerhult - Delta Microprism;598;2004;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613890;23166-520;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-529;295;2.2;3000;2004;Polystyrene - Fagerhult - Delta Microprism;598;2004;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613913;23166-529;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167;295;2.2;4000;2206;Polystyrene - Fagerhult - Delta Microprism;598;2206;4000;4000;44;24;117;White;Steel - Fagerhult - White;7320047496226;23167;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-3;295;2.2;4000;2206;Polystyrene - Fagerhult - Delta Microprism;598;2206;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047613937;23167-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-111;295;2.2;4000;2206;Polystyrene - Fagerhult - Delta Microprism;598;2206;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047613920;23167-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-340;295;2.2;4000;2206;Polystyrene - Fagerhult - Delta Microprism;598;2206;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047657535;23167-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-402;295;2.2;4000;2112;Polystyrene - Fagerhult - Delta Microprism;598;2112;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047657511;23167-402;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-519;295;2.2;4000;2206;Polystyrene - Fagerhult - Delta Microprism;598;2206;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047657627;23167-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-520;295;2.2;4000;2112;Polystyrene - Fagerhult - Delta Microprism;598;2112;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047657658;23167-520;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-528;295;2.2;4000;2112;Polystyrene - Fagerhult - Delta Microprism;598;2112;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047657528;23167-528;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 840 VTB WHITE_23167-529;295;2.2;4000;2112;Polystyrene - Fagerhult - Delta Microprism;598;2112;4000;4000;44;23;117;White;Steel - Fagerhult - White;7320047657559;23167-529;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201;599;4;3000;3821;Polystyrene - Fagerhult - Delta Microprism;599;3821;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320046711658;23201;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-3;599;4;3000;3821;Polystyrene - Fagerhult - Delta Microprism;599;3821;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320046711672;23201-3;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-111;599;4;3000;3821;Polystyrene - Fagerhult - Delta Microprism;599;3821;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047258497;23201-111;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-340;599;4;3000;3821;Polystyrene - Fagerhult - Delta Microprism;599;3821;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047258534;23201-340;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-402;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;44;23;139;White;Steel - Fagerhult - White;7320046711696;23201-402;27;27;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-519;599;4;3000;3821;Polystyrene - Fagerhult - Delta Microprism;599;3821;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047258572;23201-519;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-520;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;44;23;139;White;Steel - Fagerhult - White;7320047258596;23201-520;25;25;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-528;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;44;23;139;White;Steel - Fagerhult - White;7320047258510;23201-528;25;25;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 830 HB WHITE_23201-529;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;44;23;139;White;Steel - Fagerhult - White;7320047258558;23201-529;25;25;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202;599;4;4000;4026;Polystyrene - Fagerhult - Delta Microprism;599;4026;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320046711719;23202;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-3;599;4;4000;4026;Polystyrene - Fagerhult - Delta Microprism;599;4026;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320046711733;23202-3;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-111;599;4;4000;4026;Polystyrene - Fagerhult - Delta Microprism;599;4026;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320047258619;23202-111;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-340;599;4;4000;4026;Polystyrene - Fagerhult - Delta Microprism;599;4026;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320047258657;23202-340;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-402;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320046711757;23202-402;27;27;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-519;599;4;4000;4026;Polystyrene - Fagerhult - Delta Microprism;599;4026;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320047258695;23202-519;28;28;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-520;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320047258718;23202-520;25;25;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-528;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320047258633;23202-528;25;25;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 840 HB WHITE_23202-529;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;44;23;146;White;Steel - Fagerhult - White;7320047258671;23202-529;25;25;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209;599;4;3000;3625;Polystyrene - Fagerhult - Delta Microprism;599;3625;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320046712136;23209;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-3;599;4;3000;3625;Polystyrene - Fagerhult - Delta Microprism;599;3625;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320046712150;23209-3;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-111;599;4;3000;3625;Polystyrene - Fagerhult - Delta Microprism;599;3625;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047258978;23209-111;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-340;599;4;3000;3625;Polystyrene - Fagerhult - Delta Microprism;599;3625;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259012;23209-340;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-402;599;4;3000;3335;Polystyrene - Fagerhult - Delta Microprism;599;3335;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320046712174;23209-402;35;35;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-519;599;4;3000;3625;Polystyrene - Fagerhult - Delta Microprism;599;3625;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259050;23209-519;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-520;599;4;3000;3335;Polystyrene - Fagerhult - Delta Microprism;599;3335;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259074;23209-520;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-528;599;4;3000;3335;Polystyrene - Fagerhult - Delta Microprism;599;3335;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047258992;23209-528;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 930 HB WHITE_23209-529;599;4;3000;3335;Polystyrene - Fagerhult - Delta Microprism;599;3335;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259036;23209-529;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210;599;4;4000;3860;Polystyrene - Fagerhult - Delta Microprism;599;3860;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320046712198;23210;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-3;599;4;4000;3860;Polystyrene - Fagerhult - Delta Microprism;599;3860;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320046712211;23210-3;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-111;599;4;4000;3860;Polystyrene - Fagerhult - Delta Microprism;599;3860;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320047259098;23210-111;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-340;599;4;4000;3860;Polystyrene - Fagerhult - Delta Microprism;599;3860;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320047259135;23210-340;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-402;599;4;4000;3551;Polystyrene - Fagerhult - Delta Microprism;599;3551;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320046712235;23210-402;35;35;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-519;599;4;4000;3860;Polystyrene - Fagerhult - Delta Microprism;599;3860;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320047259173;23210-519;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-520;599;4;4000;3551;Polystyrene - Fagerhult - Delta Microprism;599;3551;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320047259197;23210-520;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-528;599;4;4000;3551;Polystyrene - Fagerhult - Delta Microprism;599;3551;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320047259111;23210-528;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 HL 940 HB WHITE_23210-529;599;4;4000;3551;Polystyrene - Fagerhult - Delta Microprism;599;3551;4000;4000;44;23;124;White;Steel - Fagerhult - White;7320047259159;23210-529;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215;595;4;3000;3495;Polystyrene - Fagerhult - Delta Microprism;595;3495;3000;3000;44;23;115;White;Steel - Fagerhult - White;7320047265174;23215;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-3;595;4;3000;3495;Polystyrene - Fagerhult - Delta Microprism;595;3495;3000;3000;44;23;115;White;Steel - Fagerhult - White;7320047265228;23215-3;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-111;595;4;3000;3495;Polystyrene - Fagerhult - Delta Microprism;595;3495;3000;3000;44;23;115;White;Steel - Fagerhult - White;7320047265242;23215-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-340;595;4;3000;3495;Polystyrene - Fagerhult - Delta Microprism;595;3495;3000;3000;44;23;115;White;Steel - Fagerhult - White;7320047265266;23215-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-402;595;4;3000;3416;Polystyrene - Fagerhult - Delta Microprism;595;3416;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047265235;23215-402;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-519;595;4;3000;3495;Polystyrene - Fagerhult - Delta Microprism;595;3495;3000;3000;44;23;115;White;Steel - Fagerhult - White;7320047265280;23215-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-520;595;4;3000;3416;Polystyrene - Fagerhult - Delta Microprism;595;3416;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047265297;23215-520;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-528;595;4;3000;3416;Polystyrene - Fagerhult - Delta Microprism;595;3416;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047265259;23215-528;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 930 WHITE_23215-529;595;4;3000;3416;Polystyrene - Fagerhult - Delta Microprism;595;3416;3000;3000;44;23;119;White;Steel - Fagerhult - White;7320047265273;23215-529;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047265303;23216;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-3;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047265310;23216-3;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-111;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047265334;23216-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-340;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047265358;23216-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-402;595;4;4000;3638;Polystyrene - Fagerhult - Delta Microprism;595;3638;4000;4000;44;23;129;White;Steel - Fagerhult - White;7320047265327;23216-402;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-519;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047265372;23216-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-520;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;129;White;Steel - Fagerhult - White;7320047265389;23216-520;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-528;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;129;White;Steel - Fagerhult - White;7320047265341;23216-528;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA 600X600 VTB 940 WHITE_23216-529;595;4;4000;3722;Polystyrene - Fagerhult - Delta Microprism;595;3722;4000;4000;44;23;129;White;Steel - Fagerhult - White;7320047265365;23216-529;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406;599;4;3000;2558;Polystyrene - Fagerhult - Delta Microprism;599;2558;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320046596989;23406;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-3;599;4;3000;2558;Polystyrene - Fagerhult - Delta Microprism;599;2558;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320046711214;23406-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-111;599;4;3000;2558;Polystyrene - Fagerhult - Delta Microprism;599;2558;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259456;23406-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-340;599;4;3000;2558;Polystyrene - Fagerhult - Delta Microprism;599;2558;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259494;23406-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-402;599;4;3000;2383;Polystyrene - Fagerhult - Delta Microprism;599;2383;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320046711238;23406-402;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-519;599;4;3000;2558;Polystyrene - Fagerhult - Delta Microprism;599;2558;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259531;23406-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-520;599;4;3000;2383;Polystyrene - Fagerhult - Delta Microprism;599;2383;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259555;23406-520;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-528;599;4;3000;2383;Polystyrene - Fagerhult - Delta Microprism;599;2383;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259470;23406-528;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 930 HB WHITE_23406-529;599;4;3000;2383;Polystyrene - Fagerhult - Delta Microprism;599;2383;3000;3000;44;23;116;White;Steel - Fagerhult - White;7320047259517;23406-529;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407;599;4;4000;2725;Polystyrene - Fagerhult - Delta Microprism;599;2725;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320046597009;23407;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-3;599;4;4000;2725;Polystyrene - Fagerhult - Delta Microprism;599;2725;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320046711252;23407-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-111;599;4;4000;2725;Polystyrene - Fagerhult - Delta Microprism;599;2725;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047259579;23407-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-340;599;4;4000;2725;Polystyrene - Fagerhult - Delta Microprism;599;2725;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047259616;23407-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-402;599;4;4000;2538;Polystyrene - Fagerhult - Delta Microprism;599;2538;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320046711276;23407-402;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-519;599;4;4000;2725;Polystyrene - Fagerhult - Delta Microprism;599;2725;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047259654;23407-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-520;599;4;4000;2538;Polystyrene - Fagerhult - Delta Microprism;599;2538;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047259678;23407-520;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-528;599;4;4000;2538;Polystyrene - Fagerhult - Delta Microprism;599;2538;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047259593;23407-528;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 940 HB WHITE_23407-529;599;4;4000;2538;Polystyrene - Fagerhult - Delta Microprism;599;2538;4000;4000;44;23;123;White;Steel - Fagerhult - White;7320047259630;23407-529;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493;599;4;3000;2802;Polystyrene - Fagerhult - Delta Microprism;599;2802;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320046596897;23493;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-3;599;4;3000;2802;Polystyrene - Fagerhult - Delta Microprism;599;2802;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320046710897;23493-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-111;599;4;3000;2802;Polystyrene - Fagerhult - Delta Microprism;599;2802;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047259890;23493-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-340;599;4;3000;2802;Polystyrene - Fagerhult - Delta Microprism;599;2802;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047259937;23493-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-402;599;4;3000;2521;Polystyrene - Fagerhult - Delta Microprism;599;2521;3000;3000;44;23;137;White;Steel - Fagerhult - White;7320046710910;23493-402;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-519;599;4;3000;2802;Polystyrene - Fagerhult - Delta Microprism;599;2802;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047259975;23493-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-520;599;4;3000;2521;Polystyrene - Fagerhult - Delta Microprism;599;2521;3000;3000;44;23;137;White;Steel - Fagerhult - White;7320047259999;23493-520;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-528;599;4;3000;2521;Polystyrene - Fagerhult - Delta Microprism;599;2521;3000;3000;44;23;137;White;Steel - Fagerhult - White;7320047259913;23493-528;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 830 HB WHITE_23493-529;599;4;3000;2521;Polystyrene - Fagerhult - Delta Microprism;599;2521;3000;3000;44;23;137;White;Steel - Fagerhult - White;7320047259951;23493-529;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494;599;4;4000;2952;Polystyrene - Fagerhult - Delta Microprism;599;2952;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320046596903;23494;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-3;599;4;4000;2952;Polystyrene - Fagerhult - Delta Microprism;599;2952;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320046710934;23494-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-111;599;4;4000;2952;Polystyrene - Fagerhult - Delta Microprism;599;2952;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320047260018;23494-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-340;599;4;4000;2952;Polystyrene - Fagerhult - Delta Microprism;599;2952;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320047260056;23494-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-402;599;4;4000;2657;Polystyrene - Fagerhult - Delta Microprism;599;2657;4000;4000;44;23;144;White;Steel - Fagerhult - White;7320046710958;23494-402;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-519;599;4;4000;2952;Polystyrene - Fagerhult - Delta Microprism;599;2952;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320047260094;23494-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-520;599;4;4000;2657;Polystyrene - Fagerhult - Delta Microprism;599;2657;4000;4000;44;23;144;White;Steel - Fagerhult - White;7320047260117;23494-520;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-528;599;4;4000;2657;Polystyrene - Fagerhult - Delta Microprism;599;2657;4000;4000;44;23;144;White;Steel - Fagerhult - White;7320047260032;23494-528;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 600X600 LL 840 HB WHITE_23494-529;599;4;4000;2657;Polystyrene - Fagerhult - Delta Microprism;599;2657;4000;4000;44;23;144;White;Steel - Fagerhult - White;7320047260070;23494-529;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508;595;4;3000;4175;Polystyrene - Fagerhult - Delta Microprism;595;4175;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320046189686;23508;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-3;595;4;3000;4175;Polystyrene - Fagerhult - Delta Microprism;595;4175;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320046213169;23508-3;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-111;595;4;3000;4175;Polystyrene - Fagerhult - Delta Microprism;595;4175;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047260131;23508-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-340;595;4;3000;4175;Polystyrene - Fagerhult - Delta Microprism;595;4175;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047260179;23508-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-402;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046213176;23508-402;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-519;595;4;3000;4175;Polystyrene - Fagerhult - Delta Microprism;595;4175;3000;3000;44;23;138;White;Steel - Fagerhult - White;7320047260216;23508-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-520;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260230;23508-520;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-528;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260155;23508-528;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-529;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260193;23508-529;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509;595;4;4000;4399;Polystyrene - Fagerhult - Delta Microprism;595;4399;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320046213183;23509;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-3;595;4;4000;4399;Polystyrene - Fagerhult - Delta Microprism;595;4399;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320046213190;23509-3;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-111;595;4;4000;4399;Polystyrene - Fagerhult - Delta Microprism;595;4399;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320047260254;23509-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-340;595;4;4000;4399;Polystyrene - Fagerhult - Delta Microprism;595;4399;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320047260292;23509-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-402;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320046213206;23509-402;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-519;595;4;4000;4399;Polystyrene - Fagerhult - Delta Microprism;595;4399;4000;4000;44;23;145;White;Steel - Fagerhult - White;7320047260339;23509-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-520;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047260353;23509-520;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-528;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047260278;23509-528;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-529;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;44;23;150;White;Steel - Fagerhult - White;7320047260315;23509-529;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513;595;4;3000;3153;Polystyrene - Fagerhult - Delta Microprism;595;3153;3000;3000;44;23;153;White;Steel - Fagerhult - White;7320046282929;23513;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-3;595;4;3000;3131;Polystyrene - Fagerhult - Delta Microprism;595;3131;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046282936;23513-3;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-111;595;4;3000;3131;Polystyrene - Fagerhult - Delta Microprism;595;3131;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260377;23513-111;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-340;595;4;3000;3131;Polystyrene - Fagerhult - Delta Microprism;595;3131;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260414;23513-340;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-402;595;4;3000;2917;Polystyrene - Fagerhult - Delta Microprism;595;2917;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320046282943;23513-402;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-519;595;4;3000;3131;Polystyrene - Fagerhult - Delta Microprism;595;3131;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260452;23513-519;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-520;595;4;3000;2917;Polystyrene - Fagerhult - Delta Microprism;595;2917;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260476;23513-520;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-528;595;4;3000;2917;Polystyrene - Fagerhult - Delta Microprism;595;2917;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260391;23513-528;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB LL_23513-529;595;4;3000;2917;Polystyrene - Fagerhult - Delta Microprism;595;2917;3000;3000;44;23;142;White;Steel - Fagerhult - White;7320047260438;23513-529;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514;595;4;4000;3299;Polystyrene - Fagerhult - Delta Microprism;595;3299;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320046282950;23514;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-3;595;4;4000;3299;Polystyrene - Fagerhult - Delta Microprism;595;3299;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320046282967;23514-3;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-111;595;4;4000;3299;Polystyrene - Fagerhult - Delta Microprism;595;3299;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047260490;23514-111;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-340;595;4;4000;3299;Polystyrene - Fagerhult - Delta Microprism;595;3299;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047260537;23514-340;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-402;595;4;4000;3074;Polystyrene - Fagerhult - Delta Microprism;595;3074;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320046282981;23514-402;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-519;595;4;4000;3299;Polystyrene - Fagerhult - Delta Microprism;595;3299;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047260575;23514-519;22;22;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-520;595;4;4000;3074;Polystyrene - Fagerhult - Delta Microprism;595;3074;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047260599;23514-520;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-528;595;4;4000;3074;Polystyrene - Fagerhult - Delta Microprism;595;3074;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047260513;23514-528;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB LL_23514-529;595;4;4000;3074;Polystyrene - Fagerhult - Delta Microprism;595;3074;4000;4000;44;23;149;White;Steel - Fagerhult - White;7320047260551;23514-529;21;21;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM DELTA REC 300X600 830 VTB WHITE_23166-528;295;2.2;3000;2004;Polystyrene - Fagerhult - Delta Microprism;598;2004;3000;3000;44;23;111;White;Steel - Fagerhult - White;7320047613906;23166-528;18;18;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL PLUS_23495-546;595;5;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;20;23;132;White;Steel - Fagerhult - White;7320048521996;23495-546;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL PLUS_23496-546;595;5;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;20;23;139;White;Steel - Fagerhult - White;7320048522009;23496-546;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 3K VTB HL_23508-546;595;5;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;20;23;132;White;Steel - Fagerhult - White;7320048521965;23508-546;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM 600X600 DELTA 4K VTB HL_23509-546;595;5;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;20;23;139;White;Steel - Fagerhult - White;7320048521989;23509-546;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;1
MULTILUME SLIM REC 600X600 DELTA TW VTB_23512;595;4;4000;3585;Polystyrene - Fagerhult - Delta Microprism;595;3585;4000;4000;44;23;115;White;Steel - Fagerhult - White;7320049656147;23512;31;31;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM 600X600 DELTA HL T/W ORG.RESP. VTB_23595;595;4;4000;3585;Polystyrene - Fagerhult - Delta Microprism;595;3585;4000;4000;44;23;113;White;Steel - Fagerhult - White;7316910087486;23595;32;32;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM 600X600 DELTA HL T/W ORG.RESP. VTB_23595-3;595;4;4000;3585;Polystyrene - Fagerhult - Delta Microprism;595;3585;4000;4000;44;23;113;White;Steel - Fagerhult - White;7316910087530;23595-3;32;32;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM 600X600 DELTA HL T/W ORG.RESP. VTB_23595-111;595;4;4000;3585;Polystyrene - Fagerhult - Delta Microprism;595;3585;4000;4000;44;23;113;White;Steel - Fagerhult - White;7316910087561;23595-111;32;32;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM 600X600 DELTA HL T/W ORG.RESP. VTB_23595-340;595;4;4000;3585;Polystyrene - Fagerhult - Delta Microprism;595;3585;4000;4000;44;23;113;White;Steel - Fagerhult - White;7316910087608;23595-340;32;32;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM 600X600 DELTA HL T/W ORG.RESP. VTB_23595-519;595;4;4000;3585;Polystyrene - Fagerhult - Delta Microprism;595;3585;4000;4000;44;23;113;White;Steel - Fagerhult - White;7316910087615;23595-519;32;32;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;1
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. VTB_23425-3;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;20;23;140;White;Steel - Fagerhult - White;7316911437280;23425-3;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. VTB_23425;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;20;23;140;White;Steel - Fagerhult - White;7316911437266;23425;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. VTB_23425-111;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;20;23;137;White;Steel - Fagerhult - White;7316911437303;23425-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. VTB_23425-340;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;20;23;137;White;Steel - Fagerhult - White;7316911437327;23425-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. VTB_23425-519;595;4;3000;4081;Polystyrene - Fagerhult - Delta Microprism;595;4081;3000;3000;20;23;137;White;Steel - Fagerhult - White;7316911437341;23425-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. VTB_23426;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;20;23;148;White;Steel - Fagerhult - White;7316911437365;23426;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. VTB_23426-3;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;20;23;148;White;Steel - Fagerhult - White;7316911437389;23426-3;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. VTB_23426-111;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;20;23;145;White;Steel - Fagerhult - White;7316911437402;23426-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. VTB_23426-340;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;20;23;145;White;Steel - Fagerhult - White;7316911437426;23426-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. VTB_23426-519;595;4;4000;4300;Polystyrene - Fagerhult - Delta Microprism;595;4300;4000;4000;20;23;145;White;Steel - Fagerhult - White;7316911437440;23426-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 930 ORGANIC RESP. VTB_23427;595;4;3000;3503;Polystyrene - Fagerhult - Delta Microprism;595;3503;3000;3000;20;23;120;White;Steel - Fagerhult - White;7316911437464;23427;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 DELTA 930 ORGANIC RESP. VTB_23427-3;595;4;3000;3503;Polystyrene - Fagerhult - Delta Microprism;595;3503;3000;3000;20;23;120;White;Steel - Fagerhult - White;7316911437488;23427-3;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 DELTA 930 ORGANIC RESP. VTB_23427-111;595;4;3000;3416;Polystyrene - Fagerhult - Delta Microprism;595;3416;3000;3000;20;23;115;White;Steel - Fagerhult - White;7316911437501;23427-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 DELTA 930 ORGANIC RESP. VTB_23427-340;595;4;3000;3416;Polystyrene - Fagerhult - Delta Microprism;595;3416;3000;3000;20;23;115;White;Steel - Fagerhult - White;7316911437525;23427-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 DELTA 930 ORGANIC RESP. VTB_23427-519;595;4;3000;3416;Polystyrene - Fagerhult - Delta Microprism;595;3416;3000;3000;20;23;115;White;Steel - Fagerhult - White;7316911437549;23427-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 600X600 DELTA 940 ORGANIC RESP. VTB_23428;595;4;4000;3731;Polystyrene - Fagerhult - Delta Microprism;595;3731;4000;4000;20;23;128;White;Steel - Fagerhult - White;7316911437563;23428;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 600X600 DELTA 940 ORGANIC RESP. VTB_23428-3;595;4;4000;3731;Polystyrene - Fagerhult - Delta Microprism;595;3731;4000;4000;20;23;128;White;Steel - Fagerhult - White;7316911437587;23428-3;29;29;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 600X600 DELTA 940 ORGANIC RESP. VTB_23428-340;595;4;4000;3638;Polystyrene - Fagerhult - Delta Microprism;595;3638;4000;4000;20;23;122;White;Steel - Fagerhult - White;7316911437624;23428-340;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 600X600 DELTA 940 ORGANIC RESP. VTB_23428-111;595;4;4000;3638;Polystyrene - Fagerhult - Delta Microprism;595;3638;4000;4000;20;23;122;White;Steel - Fagerhult - White;7316911437600;23428-111;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 600X600 DELTA 940 ORGANIC RESP. VTB_23428-519;595;4;4000;3638;Polystyrene - Fagerhult - Delta Microprism;595;3638;4000;4000;20;23;122;White;Steel - Fagerhult - White;7316911437648;23428-519;30;30;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 300X600 DELTA 830 ORGANIC RESP. VTB_23435;595;2.6;3000;2004;Polystyrene - Fagerhult - Delta Microprism;295;2004;3000;3000;20;23;108;White;Steel - Fagerhult - White;7316911437662;23435;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 830 ORGANIC RESP. VTB_23435-3;595;2.6;3000;2004;Polystyrene - Fagerhult - Delta Microprism;295;2004;3000;3000;20;23;108;White;Steel - Fagerhult - White;7316911437686;23435-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 830 ORGANIC RESP. VTB_23435-111;595;2.6;3000;2004;Polystyrene - Fagerhult - Delta Microprism;295;2004;3000;3000;20;23;105;White;Steel - Fagerhult - White;7316911437709;23435-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 830 ORGANIC RESP. VTB_23435-340;595;2.6;3000;2004;Polystyrene - Fagerhult - Delta Microprism;295;2004;3000;3000;20;23;105;White;Steel - Fagerhult - White;7316911437723;23435-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 830 ORGANIC RESP. VTB_23435-519;595;2.6;3000;2004;Polystyrene - Fagerhult - Delta Microprism;295;2004;3000;3000;20;23;105;White;Steel - Fagerhult - White;7316911437747;23435-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 840 ORGANIC RESP. VTB_23436;595;2.6;4000;2112;Polystyrene - Fagerhult - Delta Microprism;295;2112;4000;4000;20;23;114;White;Steel - Fagerhult - White;7316911437761;23436;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 840 ORGANIC RESP. VTB_23436-3;595;2.6;4000;2112;Polystyrene - Fagerhult - Delta Microprism;295;2112;4000;4000;20;23;114;White;Steel - Fagerhult - White;7316911437785;23436-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 840 ORGANIC RESP. VTB_23436-111;595;2.6;4000;2112;Polystyrene - Fagerhult - Delta Microprism;295;2112;4000;4000;20;23;111;White;Steel - Fagerhult - White;7316911437808;23436-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 840 ORGANIC RESP. VTB_23436-519;595;2.6;4000;2112;Polystyrene - Fagerhult - Delta Microprism;295;2112;4000;4000;20;23;111;White;Steel - Fagerhult - White;7316911437846;23436-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 840 ORGANIC RESP. VTB_23436-340;595;2.6;4000;2112;Polystyrene - Fagerhult - Delta Microprism;295;2112;4000;4000;20;23;111;White;Steel - Fagerhult - White;7316911437822;23436-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 300X600 DELTA 930 ORGANIC RESP. VTB_23437;595;2.6;3000;1678;Polystyrene - Fagerhult - Delta Microprism;295;1678;3000;3000;20;23;90;White;Steel - Fagerhult - White;7316911437860;23437;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 300X600 DELTA 930 ORGANIC RESP. VTB_23437-3;595;2.6;3000;1678;Polystyrene - Fagerhult - Delta Microprism;295;1678;3000;3000;20;23;90;White;Steel - Fagerhult - White;7316911437884;23437-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 300X600 DELTA 930 ORGANIC RESP. VTB_23437-111;595;2.6;3000;1678;Polystyrene - Fagerhult - Delta Microprism;295;1678;3000;3000;20;23;88;White;Steel - Fagerhult - White;7316911437907;23437-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 300X600 DELTA 930 ORGANIC RESP. VTB_23437-340;595;2.6;3000;1678;Polystyrene - Fagerhult - Delta Microprism;295;1678;3000;3000;20;23;88;White;Steel - Fagerhult - White;7316911437921;23437-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 300X600 DELTA 930 ORGANIC RESP. VTB_23437-519;595;2.6;3000;1678;Polystyrene - Fagerhult - Delta Microprism;295;1678;3000;3000;20;23;88;White;Steel - Fagerhult - White;7316911437945;23437-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;E;1;2
MULTILUME SLIM 300X600 DELTA 940 ORGANIC RESP. VTB_23438;595;2.6;4000;1787;Polystyrene - Fagerhult - Delta Microprism;295;1787;4000;4000;20;23;96;White;Steel - Fagerhult - White;7316911437969;23438;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 300X600 DELTA 940 ORGANIC RESP. VTB_23438-3;595;2.6;4000;1787;Polystyrene - Fagerhult - Delta Microprism;295;1787;4000;4000;20;23;96;White;Steel - Fagerhult - White;7316911437983;23438-3;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 300X600 DELTA 940 ORGANIC RESP. VTB_23438-111;595;2.6;4000;1787;Polystyrene - Fagerhult - Delta Microprism;295;1787;4000;4000;20;23;94;White;Steel - Fagerhult - White;7316911438003;23438-111;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 300X600 DELTA 940 ORGANIC RESP. VTB_23438-340;595;2.6;4000;1787;Polystyrene - Fagerhult - Delta Microprism;295;1787;4000;4000;20;23;94;White;Steel - Fagerhult - White;7316911438027;23438-340;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 300X600 DELTA 940 ORGANIC RESP. VTB_23438-519;595;2.6;4000;1787;Polystyrene - Fagerhult - Delta Microprism;295;1787;4000;4000;20;23;94;White;Steel - Fagerhult - White;7316911438041;23438-519;19;19;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 90;D;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. HB_27972;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;20;23;135;White;Steel - Fagerhult - White;7316911651297;27972;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. HB_27972-3;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;20;23;135;White;Steel - Fagerhult - White;7316911651310;27972-3;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. HB_27972-111;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;20;23;133;White;Steel - Fagerhult - White;7316911651334;27972-111;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. HB_27972-519;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;20;23;133;White;Steel - Fagerhult - White;7316911651372;27972-519;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 830 ORGANIC RESP. HB_27972-340;599;4;3000;3505;Polystyrene - Fagerhult - Delta Microprism;599;3505;3000;3000;20;23;133;White;Steel - Fagerhult - White;7316911651358;27972-340;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. HB_27973;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;20;23;143;White;Steel - Fagerhult - White;7316911651396;27973;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. HB_27973-3;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;20;23;143;White;Steel - Fagerhult - White;7316911651419;27973-3;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. HB_27973-111;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;20;23;140;White;Steel - Fagerhult - White;7316911651433;27973-111;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. HB_27973-340;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;20;23;140;White;Steel - Fagerhult - White;7316911651457;27973-340;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
MULTILUME SLIM 600X600 DELTA 840 ORGANIC RESP. HB_27973-519;599;4;4000;3693;Polystyrene - Fagerhult - Delta Microprism;599;3693;4000;4000;20;23;140;White;Steel - Fagerhult - White;7316911651471;27973-519;26;26;Multilume Slim Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.<br>

<p><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</p>

<p><i>HB</i> – for suspended ceiling with concealed T-bars, symmetrical attachment of ceiling boards (20–22 mm thick).</p>";A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort. Recessed depth 23 mm.;min. 80;C;1;2
