;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Right##OTHER##
NOTOR RECESSED L-COUPLER DELTA 3K BODY ELOX LL_21900;611;2.3;3000;1254;Plastic - Fagerhult - Delta Microprism;647;1254;3000;3000;20;102;95;Anodised;Aluminium - Fagerhult - Anodised;7320046511852;21900;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 3K BODY ELOX LL_21900-402;611;3.5;3000;1334;Plastic - Fagerhult - Delta Microprism;647;1334;3000;3000;20;102;95;Anodised;Aluminium - Fagerhult - Anodised;7320046511876;21900-402;14;14;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY ELOX LL_21901;611;2.3;4000;1320;Plastic - Fagerhult - Delta Microprism;647;1320;4000;4000;20;102;100;Anodised;Aluminium - Fagerhult - Anodised;7320046511890;21901;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY ELOX LL_21901-402;611;2.3;4000;1230;Plastic - Fagerhult - Delta Microprism;647;1230;4000;4000;20;102;104;Anodised;Aluminium - Fagerhult - Anodised;7320046511913;21901-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 3K BODY ELOX HL_21902;611;2.3;3000;2446;Plastic - Fagerhult - Delta Microprism;647;2446;3000;3000;20;102;101;Anodised;Aluminium - Fagerhult - Anodised;7320046511937;21902;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY ELOX HL_21903-402;611;3.5;4000;2430;Plastic - Fagerhult - Delta Microprism;647;2430;4000;4000;20;102;97;Anodised;Aluminium - Fagerhult - Anodised;7320046511999;21903-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 3K BODY WHITE LL_21904;611;2.3;3000;1254;Plastic - Fagerhult - Delta Microprism;647;1254;3000;3000;20;102;95;White;Aluminium - Fagerhult - White;7320046512019;21904;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 3K BODY WHITE LL_21904-402;611;2.3;3000;1168;Plastic - Fagerhult - Delta Microprism;647;1168;3000;3000;20;102;99;White;Aluminium - Fagerhult - White;7320046512033;21904-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY WHITE LL_21905;611;2.3;4000;1320;Plastic - Fagerhult - Delta Microprism;647;1320;4000;4000;20;102;100;White;Aluminium - Fagerhult - White;7320046512057;21905;13;13;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY WHITE LL_21905-402;611;2.3;4000;1230;Plastic - Fagerhult - Delta Microprism;647;1230;4000;4000;20;102;104;White;Aluminium - Fagerhult - White;7320046512071;21905-402;12.5;12.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 3K BODY WHITE HL_21906;611;2.3;3000;1446;Plastic - Fagerhult - Delta Microprism;647;1446;3000;3000;20;102;101;White;Aluminium - Fagerhult - White;7320046512095;21906;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 3K BODY WHITE HL_21906-402;611;2.3;3000;2430;Plastic - Fagerhult - Delta Microprism;647;2430;3000;3000;20;102;104;White;Aluminium - Fagerhult - White;7320046512118;21906-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY WHITE HL_21907;611;2.3;4000;2578;Plastic - Fagerhult - Delta Microprism;647;2578;4000;4000;20;102;107;White;Aluminium - Fagerhult - White;7320046512132;21907;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY WHITE HL_21907-402;611;2.3;4000;2430;Plastic - Fagerhult - Delta Microprism;647;2430;4000;4000;20;102;108;White;Aluminium - Fagerhult - White;7320046512156;21907-402;24.5;24.5;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 3K BODY ELOX HL_21902-402;611;2.3;3000;2430;Plastic - Fagerhult - Delta Microprism;647;2430;3000;3000;20;102;104;Anodised;Aluminium - Fagerhult - Anodised;7320046511951;21902-402;25;25;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
NOTOR RECESSED L-COUPLER DELTA 4K BODY ELOX HL_21903;611;2.3;4000;2578;Plastic - Fagerhult - Delta Microprism;647;2578;4000;4000;20;102;107;Anodised;Aluminium - Fagerhult - Anodised;7320046511975;21903;24;24;Notor recessed LED Delta;Luminaire for mounted in ventilated or unventilated suspended ceilings. Installed in suspended ceilings with visible T-bars, VTB (15 or 24 mm) or one-piece suspended ceilings. For continuous installation with combinations of asymmetric/Control Track Unit and Delta/Opal flush, see documents below.;A recessed luminaire for all types of suspended ceilings. Delta louvres provide high efficiency and optimal lighting comfort.  Single or continuous installation.;min. 80;C;2;0
