;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Version##OTHER##;Sensor##OTHER##
RECESSO DELTA 150X1200 LL 830 WHITE_25825-340;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911459060;25825-340;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825-528;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911459046;25825-528;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825-529;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911459084;25825-529;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825-519;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911459107;25825-519;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825-520;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911459121;25825-520;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911458964;25825;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825-402;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911459008;25825-402;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825-111;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911459022;25825-111;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 830 WHITE_25825-3;147;2.1;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911458988;25825-3;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911459329;25826;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-3;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911459343;25826-3;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-402;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911459367;25826-402;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-111;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911459381;25826-111;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-528;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911459404;25826-528;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-340;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911459428;25826-340;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-529;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911459442;25826-529;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-519;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911459466;25826-519;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 LL 840 WHITE_25826-520;147;2.1;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911459480;25826-520;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 830 WHITE OR_25827;147;2.2;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911459688;25827;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 830 WHITE OR_25827-3;147;2.2;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911459701;25827-3;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 830 WHITE OR_25827-111;147;2.2;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911459725;25827-111;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 830 WHITE OR_25827-340;147;2.2;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911459749;25827-340;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 830 WHITE OR_25827-519;147;2.2;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911459763;25827-519;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 840 WHITE OR_25828;147;2.2;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911459787;25828;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 840 WHITE OR_25828-3;147;2.2;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911459800;25828-3;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 840 WHITE OR_25828-111;147;2.2;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911459824;25828-111;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 840 WHITE OR_25828-340;147;2.2;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911459848;25828-340;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1200 840 WHITE OR_25828-519;147;2.2;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911459862;25828-519;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 300X1200 LL 830 WHITE_25829-3;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911459909;25829-3;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911459886;25829;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829-402;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911459923;25829-402;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829-111;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911459947;25829-111;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829-528;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911459961;25829-528;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829-340;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911459985;25829-340;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829-529;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911460004;25829-529;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829-519;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;139;White;Steel - Fagerhult - White;7316911460028;25829-519;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 830 WHITE_25829-520;297;3;3000;2624;PMMA - Fagerhult - Delta;1197;2624;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911460042;25829-520;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911460240;25830;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-3;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911460264;25830-3;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-402;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911460288;25830-402;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-111;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911460301;25830-111;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-528;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911460325;25830-528;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-340;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911460349;25830-340;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-529;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911460363;25830-529;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-519;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;143;White;Steel - Fagerhult - White;7316911460387;25830-519;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 LL 840 WHITE_25830-520;297;3;4000;2700;PMMA - Fagerhult - Delta;1197;2700;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911460400;25830-520;19;19;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 830 WHITE OR_25831;297;3.1;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911460608;25831;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 830 WHITE OR_25831-111;297;3.1;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911460646;25831-111;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 830 WHITE OR_25831-3;297;3.1;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911460622;25831-3;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 830 WHITE OR_25831-519;297;3.1;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911460684;25831-519;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 830 WHITE OR_25831-340;297;3.1;3000;3402;PMMA - Fagerhult - Delta;1197;3402;3000;3000;20;88;133;White;Steel - Fagerhult - White;7316911460660;25831-340;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 840 WHITE OR_25832;297;3.1;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911460707;25832;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 150X1500 830 WHITE LL_25833;147;2.6;3000;3332;PMMA - Fagerhult - Delta;1497;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911460806;25833;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-3;147;2.6;3000;3332;PMMA - Fagerhult - Delta;1497;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911460820;25833-3;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-402;147;2.6;3000;3395;PMMA - Fagerhult - Delta;1497;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911460844;25833-402;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-111;147;2.6;3000;3332;PMMA - Fagerhult - Delta;1497;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911460868;25833-111;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-528;147;2.6;3000;3395;PMMA - Fagerhult - Delta;1497;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911460882;25833-528;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-340;147;2.6;3000;3332;PMMA - Fagerhult - Delta;1497;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911460905;25833-340;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-529;147;2.6;3000;3395;PMMA - Fagerhult - Delta;1497;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911460929;25833-529;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-519;147;2.6;3000;3392;PMMA - Fagerhult - Delta;1497;3392;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911460943;25833-519;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE LL_25833-520;147;2.6;3000;3395;PMMA - Fagerhult - Delta;1497;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911460967;25833-520;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834;147;2.6;4000;3332;PMMA - Fagerhult - Delta;1497;3332;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911460981;25834;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-3;147;2.6;4000;3332;PMMA - Fagerhult - Delta;1497;3332;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461001;25834-3;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-111;147;2.6;4000;3332;PMMA - Fagerhult - Delta;1497;3332;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461049;25834-111;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-402;147;2.6;4000;3395;PMMA - Fagerhult - Delta;1497;3395;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911461025;25834-402;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-528;147;2.6;4000;3395;PMMA - Fagerhult - Delta;1497;3395;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911461063;25834-528;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-340;147;2.6;4000;3332;PMMA - Fagerhult - Delta;1497;3332;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461087;25834-340;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-529;147;2.6;4000;3395;PMMA - Fagerhult - Delta;1497;3395;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911461100;25834-529;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-519;147;2.6;4000;3392;PMMA - Fagerhult - Delta;1497;3392;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461124;25834-519;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE LL_25834-520;147;2.6;4000;3395;PMMA - Fagerhult - Delta;1497;3395;4000;4000;20;88;148;White;Steel - Fagerhult - White;7316911461148;25834-520;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE OR_25835;147;2.7;3000;4454;PMMA - Fagerhult - Delta;1497;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911461520;25835;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 830 WHITE OR_25835-3;147;2.7;3000;4454;PMMA - Fagerhult - Delta;1497;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911461544;25835-3;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 830 WHITE OR_25835-111;147;2.7;3000;4454;PMMA - Fagerhult - Delta;1497;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911461568;25835-111;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 830 WHITE OR_25835-340;147;2.7;3000;4454;PMMA - Fagerhult - Delta;1497;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911461582;25835-340;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 830 WHITE OR_25835-519;147;2.7;3000;4454;PMMA - Fagerhult - Delta;1497;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911461605;25835-519;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 840 WHITE OR_25836;147;2.7;4000;4454;PMMA - Fagerhult - Delta;1497;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911461629;25836;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 840 WHITE OR_25836-3;147;2.7;4000;4454;PMMA - Fagerhult - Delta;1497;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911461643;25836-3;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 840 WHITE OR_25836-111;147;2.7;4000;4454;PMMA - Fagerhult - Delta;1497;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911461667;25836-111;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 840 WHITE OR_25836-340;147;2.7;4000;4454;PMMA - Fagerhult - Delta;1497;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911461681;25836-340;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA 150X1500 840 WHITE OR_25836-519;147;2.7;4000;4454;PMMA - Fagerhult - Delta;1497;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911461704;25836-519;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;1
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461728;25852;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-3;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461742;25852-3;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-402;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911461766;25852-402;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-111;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461780;25852-111;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-528;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911461803;25852-528;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-340;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461827;25852-340;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-529;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911461841;25852-529;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-520;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911461889;25852-520;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE LL_25852-519;147;3.1;3000;3392;PMMA - Fagerhult - Delta;1720;3392;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461865;25852-519;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462084;25853;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-3;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462107;25853-3;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-111;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462145;25853-111;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-402;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462121;25853-402;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-528;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462169;25853-528;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-340;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462183;25853-340;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-529;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462206;25853-529;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-519;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462220;25853-519;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE LL_25853-520;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462244;25853-520;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE OR_25854;147;3.1;3000;4454;PMMA - Fagerhult - Delta;1720;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911462442;25854;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 830 WHITE OR_25854-3;147;3.2;3000;4454;PMMA - Fagerhult - Delta;1720;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911462466;25854-3;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 830 WHITE OR_25854-111;147;3.2;3000;4454;PMMA - Fagerhult - Delta;1720;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911462480;25854-111;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 830 WHITE OR_25854-340;147;3.2;3000;4454;PMMA - Fagerhult - Delta;1720;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911462503;25854-340;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 830 WHITE OR_25854-519;147;3.2;3000;4454;PMMA - Fagerhult - Delta;1720;4454;3000;3000;20;88;144;White;Steel - Fagerhult - White;7316911462527;25854-519;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 840 WHITE OR_25855;147;3.2;4000;4454;PMMA - Fagerhult - Delta;1720;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911462541;25855;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 840 WHITE OR_25855-3;147;3.2;4000;4454;PMMA - Fagerhult - Delta;1720;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911462565;25855-3;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 840 WHITE OR_25855-111;147;3.2;4000;4454;PMMA - Fagerhult - Delta;1720;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911462589;25855-111;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 840 WHITE OR_25855-340;147;3.2;4000;4454;PMMA - Fagerhult - Delta;1720;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911462602;25855-340;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA BANDRASTER 150X1720 840 WHITE OR_25855-519;147;3.2;4000;4454;PMMA - Fagerhult - Delta;1720;4454;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911462626;25855-519;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;1
RECESSO DELTA 150X1500 830 WHITE HL_25856;147;2.6;3000;4420;PMMA - Fagerhult - Delta;1497;4420;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461162;25856;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-3;147;2.6;3000;4420;PMMA - Fagerhult - Delta;1497;4420;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461186;25856-3;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-402;147;2.6;3000;4518;PMMA - Fagerhult - Delta;1497;4518;3000;3000;20;88;146;White;Steel - Fagerhult - White;7316911461209;25856-402;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-111;147;2.6;3000;4420;PMMA - Fagerhult - Delta;1497;4420;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461223;25856-111;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-528;147;2.6;3000;4518;PMMA - Fagerhult - Delta;1497;4518;3000;3000;20;88;146;White;Steel - Fagerhult - White;7316911461247;25856-528;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-340;147;2.6;3000;4420;PMMA - Fagerhult - Delta;1497;4420;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461261;25856-340;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-529;147;2.6;3000;4518;PMMA - Fagerhult - Delta;1497;4518;3000;3000;20;88;146;White;Steel - Fagerhult - White;7316911461285;25856-529;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-519;147;2.6;3000;4420;PMMA - Fagerhult - Delta;1497;4420;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461308;25856-519;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 830 WHITE HL_25856-520;147;2.6;3000;4518;PMMA - Fagerhult - Delta;1497;4518;3000;3000;20;88;146;White;Steel - Fagerhult - White;7316911461322;25856-520;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-3;147;2.6;4000;4420;PMMA - Fagerhult - Delta;1497;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461360;25857-3;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857;147;2.6;4000;4420;PMMA - Fagerhult - Delta;1497;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461346;25857;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-402;147;2.6;4000;4518;PMMA - Fagerhult - Delta;1497;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911461384;25857-402;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-111;147;2.6;4000;4420;PMMA - Fagerhult - Delta;1497;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461407;25857-111;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-528;147;2.6;4000;4518;PMMA - Fagerhult - Delta;1497;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911461421;25857-528;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-340;147;2.6;4000;4420;PMMA - Fagerhult - Delta;1497;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461445;25857-340;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-529;147;2.6;4000;4518;PMMA - Fagerhult - Delta;1497;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911461469;25857-529;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-519;147;2.6;4000;4420;PMMA - Fagerhult - Delta;1497;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911461483;25857-519;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1500 840 WHITE HL_25857-520;147;2.6;4000;4518;PMMA - Fagerhult - Delta;1497;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911461506;25857-520;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461902;25887;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-3;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461926;25887-3;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-402;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911461940;25887-402;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-111;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911461964;25887-111;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-528;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911461988;25887-528;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-340;147;3.1;3000;3332;PMMA - Fagerhult - Delta;1720;3332;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911462008;25887-340;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-529;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911462022;25887-529;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-519;147;3.1;3000;3392;PMMA - Fagerhult - Delta;1720;3392;3000;3000;20;88;147;White;Steel - Fagerhult - White;7316911462046;25887-519;23;23;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 830 WHITE HL_25887-520;147;3.1;3000;3395;PMMA - Fagerhult - Delta;1720;3395;3000;3000;20;88;148;White;Steel - Fagerhult - White;7316911462060;25887-520;24.5;24.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462268;25888;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-3;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462282;25888-3;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-402;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462305;25888-402;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-111;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462329;25888-111;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-528;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462343;25888-528;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-340;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462367;25888-340;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-529;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462381;25888-529;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-519;147;3.1;4000;4420;PMMA - Fagerhult - Delta;1720;4420;4000;4000;20;88;147;White;Steel - Fagerhult - White;7316911462404;25888-519;30;30;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA BANDRASTER 150X1720 840 WHITE HL_25888-520;147;3.1;4000;4518;PMMA - Fagerhult - Delta;1720;4518;4000;4000;20;88;146;White;Steel - Fagerhult - White;7316911462428;25888-520;33.5;33.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894;147;2.1;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911459145;25894;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-3;147;2.1;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911459169;25894-3;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-402;147;2.1;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911459183;25894-402;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-111;147;2.1;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911459206;25894-111;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-528;147;2.1;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911459220;25894-528;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-340;147;2.1;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911459244;25894-340;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-529;147;2.1;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911459268;25894-529;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-519;147;2.1;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911459282;25894-519;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 830 WHITE_25894-520;147;2.1;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911459305;25894-520;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-3;147;2.1;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911459527;25895-3;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895;147;2.1;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911459503;25895;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-402;147;2.1;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911459541;25895-402;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-111;147;2.1;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911459565;25895-111;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-528;147;2.1;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911459589;25895-528;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-340;147;2.1;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911459602;25895-340;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-529;147;2.1;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911459626;25895-529;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-520;147;2.1;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911459664;25895-520;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 150X1200 HL 840 WHITE_25895-519;147;2.1;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911459640;25895-519;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896;297;3;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911460066;25896;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-3;297;3;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911460080;25896-3;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-402;297;3;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911460103;25896-402;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-111;297;3;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911460127;25896-111;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-528;297;3;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911460141;25896-528;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-340;297;3;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911460165;25896-340;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-529;297;3;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911460189;25896-529;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-519;297;3;3000;3324;PMMA - Fagerhult - Delta;1197;3324;3000;3000;20;88;136;White;Steel - Fagerhult - White;7316911460202;25896-519;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 830 WHITE_25896-520;297;3;3000;3464;PMMA - Fagerhult - Delta;1197;3464;3000;3000;20;88;140;White;Steel - Fagerhult - White;7316911460226;25896-520;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-3;297;3;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911460448;25897-3;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-402;297;3;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911460462;25897-402;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897;297;3;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911460424;25897;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-111;297;3;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911460486;25897-111;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-528;297;3;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911460509;25897-528;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-340;297;3;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911460523;25897-340;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-529;297;3;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911460547;25897-529;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-519;297;3;4000;3420;PMMA - Fagerhult - Delta;1197;3420;4000;4000;20;88;140;White;Steel - Fagerhult - White;7316911460561;25897-519;25;25;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 HL 840 WHITE_25897-520;297;3;4000;3564;PMMA - Fagerhult - Delta;1197;3564;4000;4000;20;88;144;White;Steel - Fagerhult - White;7316911460585;25897-520;26;26;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
RECESSO DELTA 300X1200 840 WHITE OR_25832-3;297;3.1;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911460721;25832-3;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 840 WHITE OR_25832-111;297;3.1;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911460745;25832-111;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 840 WHITE OR_25832-340;297;3.1;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911460769;25832-340;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
RECESSO DELTA 300X1200 840 WHITE OR_25832-519;297;3.1;4000;3500;PMMA - Fagerhult - Delta;1197;3500;4000;4000;20;88;137;White;Steel - Fagerhult - White;7316911460783;25832-519;27.5;27.5;Recesso Delta;"Recessed mounting in ventilated or unventilated suspended ceilings. Two optional designs.
<br>
<i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.";A recessed luminaire for suspended ceilings with visible T-bars. Delta louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
