,Type Comments##OTHER##,MaterialBody##OTHER##,MaterialLouvre##OTHER##,Weight_Kg##OTHER##,URL##OTHER##,Total Light Loss Factor##OTHER##,SuffixCode##OTHER##,Photometric Web File##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,LightSource##OTHER##,Light Loss Factor##OTHER##,Lamp##OTHER##,Keynote##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,FagerhultPartNumber##OTHER##,Emit from Circle Diameter##LENGTH##MILLIMETERS,COBieBarCode##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Description##OTHER##,Assembly Code##OTHER##,LOR##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,TotalLength##LENGTH##MILLIMETERS,TotalWidth##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,NumberOfLamps##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT
Sweep 700 Opal Black 3000K DALIPhasePulseControl_54920-402,Sweep 700 Opal Black 3000K,Fagerhult_Black_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54920-402.IES,Sweep Opal,Fagerhult,7730,LED,1,64,V59,7730,3000,3000,54920-402,595,7320046495626,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,120.78125
Sweep 700 Opal White 3000K DALIPhasePulseControl_54921-402,Sweep 700 Opal White 3000K,Fagerhult_White_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54921-402.IES,Sweep Opal,Fagerhult,7730,LED,1,64,V59,7730,3000,3000,54921-402,595,7320046495640,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,120.78125
Sweep 700 Opal Green 3000K DALIPhasePulseControl_54922-402,Sweep 700 Opal Green 3000K,Fagerhult_Green_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54922-402.IES,Sweep Opal,Fagerhult,7730,LED,1,64,V59,7730,3000,3000,54922-402,595,7320046495664,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,120.78125
Sweep 700 Opal Blue 3000K DALIPhasePulseControl_54923-402,Sweep 700 Opal Blue 3000K,Fagerhult_Blue_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54923-402.IES,Sweep Opal,Fagerhult,7730,LED,1,64,V59,7730,3000,3000,54923-402,595,7320046495688,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,120.78125
Sweep 700 Opal Light coral 3000K DALIPhasePulseControl_54924-402,Sweep 700 Opal Light coral 3000K,Fagerhult_Light coral_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54924-402.IES,Sweep Opal,Fagerhult,7730,LED,1,64,V59,7730,3000,3000,54924-402,595,7320046495701,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,120.78125
Sweep 700 Opal Black 4000K DALIPhasePulseControl_54925-402,Sweep 700 Opal Black 4000K,Fagerhult_Black_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54925-402.IES,Sweep Opal,Fagerhult,7880,LED,1,64,V59,7880,4000,4000,54925-402,595,7320046495725,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,123.125
Sweep 700 Opal White 4000K DALIPhasePulseControl_54926-402,Sweep 700 Opal White 4000K,Fagerhult_White_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54926-402.IES,Sweep Opal,Fagerhult,7880,LED,1,64,V59,7880,4000,4000,54926-402,595,7320046495749,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,123.125
Sweep 700 Opal Green 4000K DALIPhasePulseControl_54927-402,Sweep 700 Opal Green 4000K,Fagerhult_Green_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54927-402.IES,Sweep Opal,Fagerhult,7880,LED,1,64,V59,7880,4000,4000,54927-402,595,7320046495763,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,123.125
Sweep 700 Opal Blue 4000K DALIPhasePulseControl_54928-402,Sweep 700 Opal Blue 4000K,Fagerhult_Blue_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54928-402.IES,Sweep Opal,Fagerhult,7880,LED,1,64,V59,7880,4000,4000,54928-402,595,7320046495787,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,123.125
Sweep 700 Opal Light coral 4000K DALIPhasePulseControl_54929-402,Sweep 700 Opal Light coral 4000K,Fagerhult_Light coral_plastic,Fagerhult_Opal_acryl,8,http:__www.fagerhult.se,1,DALIPhasePulseControl,54929-402.IES,Sweep Opal,Fagerhult,7880,LED,1,64,V59,7880,4000,4000,54929-402,595,7320046495800,64,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock. ,D5020230,100,64,700,0,358,1,123.125
