,Type Comments##OTHER##,MaterialBody##OTHER##,MaterialLouvre##OTHER##,Weight_Kg##OTHER##,URL##OTHER##,Total Light Loss Factor##OTHER##,SuffixCode##OTHER##,Photometric Web File##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,LightSource##OTHER##,Light Loss Factor##OTHER##,Lamp##OTHER##,Keynote##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,FagerhultPartNumber##OTHER##,Emit from Circle Diameter##LENGTH##MILLIMETERS,COBieBarCode##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Description##OTHER##,Assembly Code##OTHER##,LOR##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,TotalLength##LENGTH##MILLIMETERS,TotalWidth##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,NumberOfLamps##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT
Sweep 500 Delta Black 3000K DALIPhasePulseControl_54910-402,Sweep 500 Delta Black 3000K,Fagerhult_Black_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54910-402.IES,Sweep Delta,Fagerhult,4200,LED,1,34,V59,4200,3000,3000,54910-402,420,7320046495428,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,123.529411764706
Sweep 500 Delta White 3000K DALIPhasePulseControl_54911-402,Sweep 500 Delta White 3000K,Fagerhult_White_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54911-402.IES,Sweep Delta,Fagerhult,4200,LED,1,34,V59,4200,3000,3000,54911-402,420,7320046495442,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,123.529411764706
Sweep 500 Delta Green 3000K DALIPhasePulseControl_54912-402,Sweep 500 Delta Green 3000K,Fagerhult_Green_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54912-402.IES,Sweep Delta,Fagerhult,4200,LED,1,34,V59,4200,3000,3000,54912-402,420,7320046495466,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,123.529411764706
Sweep 500 Delta Blue 3000K DALIPhasePulseControl_54913-402,Sweep 500 Delta Blue 3000K,Fagerhult_Blue_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54913-402.IES,Sweep Delta,Fagerhult,4200,LED,1,34,V59,4200,3000,3000,54913-402,420,7320046495480,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,123.529411764706
Sweep 500 Delta Light coral 3000K DALIPhasePulseControl_54914-402,Sweep 500 Delta Light coral 3000K,Fagerhult_Light coral_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54914-402.IES,Sweep Delta,Fagerhult,4200,LED,1,34,V59,4200,3000,3000,54914-402,420,7320046495503,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,123.529411764706
Sweep 500 Delta Black 4000K DALIPhasePulseControl_54915-402,Sweep 500 Delta Black 4000K,Fagerhult_Black_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54915-402.IES,Sweep Delta,Fagerhult,3980,LED,1,34,V59,3980,4000,4000,54915-402,420,7320046495527,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,117.058823529412
Sweep 500 Delta White 4000K DALIPhasePulseControl_54916-402,Sweep 500 Delta White 4000K,Fagerhult_White_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54916-402.IES,Sweep Delta,Fagerhult,3980,LED,1,34,V59,3980,4000,4000,54916-402,420,7320046495541,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,117.058823529412
Sweep 500 Delta Green 4000K DALIPhasePulseControl_54917-402,Sweep 500 Delta Green 4000K,Fagerhult_Green_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54917-402.IES,Sweep Delta,Fagerhult,3980,LED,1,34,V59,3980,4000,4000,54917-402,420,7320046495565,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,117.058823529412
Sweep 500 Delta Blue 4000K DALIPhasePulseControl_54918-402,Sweep 500 Delta Blue 4000K,Fagerhult_Blue_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54918-402.IES,Sweep Delta,Fagerhult,3980,LED,1,34,V59,3980,4000,4000,54918-402,420,7320046495589,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,117.058823529412
Sweep 500 Delta Light coral 4000K DALIPhasePulseControl_54919-402,Sweep 500 Delta Light coral 4000K,Fagerhult_Light coral_plastic,Fagerhult_Delta _microprisma,5,http:__www.fagerhult.se,1,DALIPhasePulseControl,54919-402.IES,Sweep Delta,Fagerhult,3980,LED,1,34,V59,3980,4000,4000,54919-402,420,7320046495602,34,Luminaire body in plastic lacquered in various colours. Supplied with 3 ?m wire. 2.2 m transparent cable and white. plastic ceiling cup. Height adjustment is done on the luminaire using a friction lock.,D5020230,100,34,500,0,256,1,117.058823529412
